
GENERAL CONDITIONS

	Number
	Condition

	1. 
	Approved Plans and supporting documentation

	
	Approved plans and supporting documentation Development must be carried out in accordance with the following approved plans and documents, except where the conditions of this consent expressly require otherwise.
Approved plans 

Plan number 

Revision number 

Plan title    

Drawn by 

Date of plan 

DA-0002

E

SITE PLAN

CEDAR DESIGN & CONSTRUCT

07/09/2025
DA-0003

E

DEMOLITION PLAN

07/09/2025
DA-0004

E

STREETSCAPE VIEW

07/09/2025
DA-1000

G

GA_BASEMENT 02

07/09/2025
DA-1001

G

GA_BASEMENT 01

07/09/2025
DA-1002

G

GA_GROUND LEVEL

07/09/2025
DA-1003

G

GA_ LEVEL 01

07/09/2025
DA-1004

G

GA_ LEVEL 02

07/09/2025
DA-1005

G

GA_LEVEL 03

07/09/2025
DA-1006

G

ROOF TOP LEVEL

07/09/2025
DA-3000

D

SECTION 1

07/09/2025
DA-3001

D

SECTION 2

07/09/2025
DA-3002

D

SECTION 3

07/09/2025
DA-3003

C

SECTION RAMP

07/09/2025
DA-7000

C

MATERIAL SCHEDULE

07/09/2025
In the event of any inconsistency between the approved plans and documents, the approved plans prevail. In the event of any inconsistency with the approved plans and a condition of this consent, the condition prevails.
1.101.S   

	
	Condition reason:   To ensure the development is built and remains consistent with approved plans and documentation.

	2. 
	Affordable Housing Management

	3. 
	The six (6) dwellings designated as affordable housing must be managed by a registered Community Housing Provider (CHP) for a minimum period of fifteen (15) years from the date of issue of the first Occupation Certificate.

Prior to the release of any Occupation Certificate, the applicant must submit to Council written confirmation from the registered CHP demonstrating acceptance of management responsibility for the affordable housing dwellings, together with details of the proposed management arrangements.

	4. 
	Condition reason: To ensure the affordable housing component is delivered, managed, and retained in accordance with the NSW Affordable Housing Ministerial Guidelines and the mandatory provisions of the Housing SEPP 2021.

	5. 
	Design Amendments - Street Tree Replacement

	
	The applicant must provide two (2) replacement street trees along Dutton Road to offset the removal of the existing street trees and maintain public domain amenity. Replacement trees are to be Corymbia ficifolia ‘Fairy Floss’, or an alternative species as approved by Council’s Tree Management Officer.

Details of the proposed street tree planting must be submitted to and approved by Council prior to the issue of the Construction Certificate. 

All approved street trees must be planted, established, and maintained to Council’s satisfaction prior to the issue of the Occupation Certificate.


	
	Condition reason:  To ensure appropriate reinstatement of street trees, maintain local amenity, and achieve a high-quality public domain outcome.

	6. 
	Design Amendments - Wheelchair Bypass Compliance

	
	The development must be amended to provide a compliant wheelchair bypass area in accordance with AS 1428.1.

The proposed ramps and circulation paths currently range between 1.5–1.6 metres in width and do not accommodate wheelchair bypass. A bypass area with a minimum dimension of 1800mm x 2000mm must be provided, consistent with the requirements of Section 6.4 of AS 1428.1.

Amended plans demonstrating compliance must be submitted to and approved by Council prior to the issue of the Construction Certificate.


	
	Condition reason:   To ensure equitable and safe access within the development and to achieve compliance with the minimum standards of AS 1428.1.

	7. 
	Design Amendments - Planter Soil Depth

	
	The applicant must provide documentation demonstrating that sufficient soil depth can be achieved for all proposed planting within the development’s planters:

Typical sections must be provided cutting through the planters showing:

· Shrubs: minimum 600mm soil depth

· Trees: minimum 1000mm soil depth

Soil depth details must be included in the landscape documentation for typical planter planting. Amended plans and supporting details must be submitted to and approved by Council prior to the issue of the Construction Certificate.


	
	Condition reason: To ensure the proposed landscaping is viable, provides adequate soil volume for healthy plant growth, and contributes to long-term amenity and sustainability.

	8. 
	Design Amendments -  Unit Window and Light Well Modifications

	
	The development must be amended to reduce the depth of the light well between Unit 205, 206, 305 and 306. One secondary window from each unit must be removed to improve audio and visual privacy. The kitchen windows must be relocated to the northern aspect to improve airflow and daylight access.
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Amended plans demonstrating these changes must support the Construction Certificate.


	
	Condition reason: To ensure adequate privacy, ventilation, and natural light for future occupants and to maintain good amenity outcomes.

	9. 
	Design Amendments - Removal of Side Balcony to Unit 108

	10. 
	The southern side balcony to Unit 108 must be removed as it does not comply with the Apartment Design Guide (ADG) separation requirements. Amended plans reflecting the removal of this balcony and revision to accommodate a comparable private open space area to the western orientation of the unit is to be submitted to Council prior to the issue of a construction certificate.

	11. 
	Condition reason: To ensure compliance with the ADG separation standards and to maintain privacy and amenity for neighbouring properties.

	12. 
	Hazardous Material Survey

	
	Prior to demolition, the entire site (includes any structures) is to be assessed for hazardous materials, especially asbestos. A Hazardous Materials (HAZMAT) Report is to be prepared by an inspection body accredited by NATA. 

All recommendations in the above-mentioned report are to be implemented and a clearance certificate issued by an appropriately qualified occupational hygienist who has not previously been involved in the preparation of the Hazardous Materials (HAZMAT) Report, is to be submitted to Council prior to the issue of a construction certificate.

	
	Condition reason:   To ensure that the development complies with Council’s Environmental Health Policies.

	13. 
	Ausgrid  - Overhead Powerlines are in the vicinity of the development

	14. 
	The developer should refer to SafeWork NSW Document – Work Near Overhead Powerlines: Code of Practice. This document outlines the minimum separation requirements between electrical mains (overhead wires) and structures within the development site throughout the construction process. It is a statutory requirement that these distances be maintained throughout the construction phase. 

Consideration should be given to the positioning and operating of cranes, scaffolding, and sufficient clearances from all types of vehicles that are expected be entering and leaving the site. The “as constructed” minimum clearances to the mains must also be maintained. These distances are outlined in the Ausgrid Network Standard, NS220 Overhead Design Manual. This document can be sourced from Ausgrid’s website at www.ausgrid.com.au. 

It is the responsibility of the developer to verify and maintain minimum clearances onsite. In the event where minimum safe clearances are not able to be met due to the design of the development, the Ausgrid mains may need to be relocated in this instance. Any Ausgrid asset relocation works will be at the developer’s cost.

	15. 
	Condition reason: To ensure the proposed works maintain statutory safety clearances to existing overhead powerlines during construction.

	16. 
	Ausgrid - New Driveways / Proximity to Existing Poles

	17. 
	Proposed driveways shall be located to maintain a minimum clearance of 1.5m from the nearest face of the pole to any part of the driveway, including the layback, this is to allow room for future pole replacements. Ausgrid should be further consulted for any deviation to this distance.

	18. 
	Condition reason: To maintain adequate clearance to existing Ausgrid poles to allow for safe access, maintenance and future pole replacement, and to ensure driveway locations do not compromise the electricity network infrastructure.

	19. 
	Ausgrid - New or modified connection

	
	To apply to connect or modify a connection for a residential or commercial premises. Ausgrid recommends the proponent to engage an Accredited Service Provider and submit a connection application to Ausgrid as soon as practicable. Visit the Ausgrid website for further details; https://www.ausgrid.com.au/Connections/Get-connected 

Additional information can be found in the Ausgrid Quick Reference Guide for Safety Clearances “Working Near Ausgrid Assets - Clearances". This document can be found  by visiting the following Ausgrid website:  www.ausgrid.com.au/Your-safety/Working-Safe/Clearance-enquiries 

Should you require further information please contact Ausgrid via email to 

Development@ausgrid.com.au


	
	Condition reason: To ensure the development obtains a compliant electrical connection and that all connection works are carried out by accredited contractors in line with Ausgrid’s requirements.


DEMOLITION WORK
	20. 
	Demolition

	
	The demolition of all structures on the property must be undertaken in accordance with all the following: 

a. Written notice must be issued to adjoining residents a minimum of seven (7) days before the commencement of demolition advising of the commencement date,
b. Written notice must be issued to Council for inspection a minimum of (7) days before the commencement of demolition. Written notice must include the date when demolition work will commence and details of the name, address, contact telephone number and licence number of the demolition contractor,

c. Inspections being undertaken by Council including: 
i. A pre-commencement demolition inspection when all site works required as part of this Determination Notice are installed on the site and before demolition work commencing, and

ii. A final demolition inspection when the demolition work has been completed to ensure that the site is left in a satisfactory manner, in accordance with the conditions of this Determination Notice,
d. Payment of an inspection fee at Council’s current rate must be paid before inspection. Council requires 48 hours’ notice to carry out an inspection,

e. A sign must be erected at the front of the property showing the name of the licenced demolition contractor, the licence number and a telephone number on which that person can be contact outside of working hours,

f. All demolition work must be carried out in accordance with Australian Standard 2601 – ‘The Demolition of Structures’,

g. Where asbestos containing materials are to be removed, demolition must be carried out by contractors who have a current SafeWork NSW licence in asbestos removal,

h. An asbestos clearance certificate issued under the Work Health and Safety Act 2011 must be submitted to Council after the completion of demolition work,

i. Hazardous and intractable wastes arising from the demolition process must be removed and disposed of in accordance with the requirements of SafeWork NSW and the NSW Environment Protection Authority, 

j. Demolition procedures must maximise the reuse and recycling of demolished materials to reduce the environmental impacts of waste disposal,

k. Adhere to the requirements stipulated in the approved Waste Management Plan, and

l. Demolition may only be carried out between 7.00 am and 5.00 pm on Monday to Saturday and no building work/s is to be carried out at any time on a Sunday or a public holiday.

A copy of the final demolition inspection report must be submitted to the principal certifier before the commencement of any building work.

3.201 

	
	Condition reason:  To ensure compliance with the relevant Canterbury Bankstown policy.


BUILDING WORK

BEFORE ISSUE OF A CONSTRUCTION CERTIFICATE

	21. 
	Development Contributions, Section 7.11

	
	Development Contributions of $395,574.88 must be paid for this development before the issue of any construction certificate. The contributions are levied under Canterbury Bankstown Local Infrastructure Contributions Plan 2022 and Section 7.11 of the Environmental Planning and Assessment Act 1979.The contributions will be used to provide, extend or augment public amenities or public services required due to additional demand for these facilities created by the new development. The development contribution will be allocated to the following purposes under the contributions plan:
LGA Open space and recreation facilities
$212,550.92
LGA Access and public domain facilities
$59,875.93
LGA Community and cultural facilities
$58,186.07
Plan management and administration
$4,961.96
LGA Open space and recreation facilities
$38,004.00
LGA Access and public domain facilities
$10,707.00
LGA Community and cultural facilities
$10,404.00
Plan management and administration
$885.00
TOTAL

$395,574.88

Indexing of the contribution amount to be paid: The development contribution payable will be adjusted, at the time of payment, to reflect Consumer Price Index increases which have occurred since the “Consent to operate from date” which appears on the front page of this Determination Notice.
No construction certificate is to be issued and no construction is to commence until payment of development contributions. The contribution must be paid to Council before the issue of any construction certificate. Construction of the development may NOT commence until the development contributions are paid.
A copy of the development contributions plan is available for inspection on Council's website and at Council's Administration offices in Bankstown and Campsie.

NOTE:  Development contribution amounts are non-refundable if you do not proceed with your development.

2.101

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	22. 
	Housing and Productivity Contribution

	
	Before the issue of the first construction certificate issued as part of this consent, the housing and productivity contribution (HPC) set out in the table below is required to be made.

Housing and productivity contribution

Amount

Housing and productivity contribution (base component)

$276,791.80
The HPC must be paid using the NSW planning portal. 

At the time of payment, the amount of the HPC is to be adjusted in accordance with the Environmental Planning and Assessment (Housing and Productivity Contributions) Order 2024 (HPC Order). 

The HPC may be made wholly or partly as a non-monetary contribution (apart from any transport project component) if the Minister administering the Environmental Planning and Assessment Act 1979 agrees. 

The HPC is not required to be made to the extent that a planning agreement excludes the application of Subdivision 4 of Division 7.1 of the Environmental Planning and Assessment Act 1979 to the development, or the HPC Order exempts the development from the contribution.

The amount of the contribution may be reduced under the HPC Order, including if payment is made before 1 July 2025.



	
	Condition Reason:  To require contributions towards the provision of regional infrastructure.

	23. 
	Payment of Fees

	
	Before Issuing a construction certificate, all the following must be paid to the relevant authority/entity and written evidence of these payments must be provided to the certifier.  

a. Levies

b. Bonds

c. Contributions

d. Inspection fees 

2.103.S   

	
	Condition reason:   To ensure compliance with the relevant New South Wales legislation.

	24. 
	Long Service Levy

	
	Before the issue of the relevant construction certificate, payment of the long service levy is required, under the Building and Construction industry Long Service Payments Act 1986, section 34.  Evidence of the payment is to be provided to the Certifier. Payment can be calculated using the Levy Portal Calculator at https://longservice.force.com/bci/s/levy-calculator. Payment must be made via the Long Service Levy Portal at https://www.longservice.nsw.gov.au.

2.104.S

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	25. 
	Construction Cranes May Require Separate Approval

	
	Separate approval must be sought (where required) under the relevant Regulations for any equipment (i.e. cranes) required to construct the building. Construction cranes may be required to operate at a height above the proposed development and consequently, may require separate approval under the Regulations. It is advisable that approval to operate equipment (i.e. cranes) be obtained before the issue of any construction certificate.

2.105

	
	Condition reason:  To ensure adequate approval of crane use.

	26. 
	Car Parking Details

	
	Before the issue of the relevant construction certificate, a suitably qualified engineer must review the plans which relate to parking facilities and provide written evidence, to the certifier’s satisfaction, that it complies with the relevant parts of AS 2890 – ‘Parking Facilities - Off-Street Carparking’ and Council’s development control plan.

2.110.S   

	
	Condition reason:   To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	27. 
	Access Intercom

	
	Where a boom gate or barrier control is in place, the visitor spaces must be accessible to visitors by the location of an intercom (or card controller system) at the car park entry, installed at least 4 metres recessed into the site, when measured from the property boundary with the street. The intercom is to be wired to all units. 

The intercom must comply with Australian Standard AS 1428.2: Design for access and mobility - Enhance and additional requirements - Building and facilities Sections 22 and 23.

2.111

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	28. 
	Bicycle Parking Spaces

	
	The minimum number of bicycle parking spaces is to be provided for the development must comply with the below.

a. Eight (8) Residential.
Note: The layout, design and security of bicycle facilities must comply with the minimum requirements of Australian Standard AS 2890.3 – ‘Parking Facilities’ Part 3: Bicycle Parking Facilities and ‘Austroads Bicycle Parking Facilities: Guidelines for Design and Installation.’

2.11

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement and parking.

	29. 
	Submit Plans to Sydney Water

	
	The Council approved plans, including demolition plans, must be submitted to Sydney Water for assessment. This will determine if the proposed structure(s) will affect any Sydney Water infrastructure or if there are additional requirements. Building plan approvals can be submitted online via Sydney Water Tap inTM.


Refer to www.sydneywater.com.au/tapin for Sydney Water’s Guidelines for building over or next to assets, visit www.sydneywater.com.au ‘Plumbing, building & developing’ then ‘Building Plan Approvals’ or call 13000 TAPINTM.

Sydney Water must issue either a Building Plan Assessment letter which states that the application is approved, or the appropriate plans must be stamped by a Water Servicing Coordinator.

2.202.S   

	
	Condition Reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	30. 
	BASIX Certificate

	
	The development must be carried out in accordance with the commitments shown on the submitted BASIX Certificate. The BASIX commitments must be reflected in the construction certificate plans and specifications. Any proposed changes to the BASIX commitments after the construction certificate has been issued will require an updated BASIX Certificate.

2.206   

	
	Condition reason:   To ensure compliance with the relevant New South Wales legislation.

	31. 
	Utilities and Services

	
	Before the issue of the relevant construction certificate, the consent holder must submit the following written evidence of service provider requirements to the certifier:

a. a letter of consent from the relevant electricity provider demonstrating that satisfactory arrangements can be made for the installation and supply of electricity; and

b. a response from the relevant water authority as to whether the plans proposed to accompany the application for a construction certificate would affect any of the relevant water authority infrastructure, and whether further requirements need to be met; and a letter of consent from the relevant telephone and broadband authority demonstrating that satisfactory arrangements can be made for the installation and supply of telephone and internet; and

c. other relevant utilities or services - that the development as proposed to be carried out is satisfactory to those other service providers, or if it is not, what changes are required to make the development satisfactory to them.

2.207   

	
	Condition reason:    To ensure works undertaken are carried out in a safe manner in accordance with relevant policies.  

	32. 
	Mobility Access

	
	The building must be designed and constructed to provide access and facilities for people with a physical disability in accordance with the Building Code of Australia.

If, in complying with this condition, amendments to the development are required, the design changes must be submitted to and approved by Council through a modification application before a construction certificate being issued.

2.208

	
	Condition reason:  To ensure compliance with the relevant Australian Standard and National Construction Code.

	33. 
	Adaptable Units

	
	Before the issue of the relevant construction certificate, the consent holder must ensure a report from a suitably qualified consultant is prepared and demonstrates, to the certifier’s satisfaction, that any adaptable dwellings specified in the approved plans or supporting documentation comply with the provisions of AS 4299 –  ‘Adaptable Housing Standards’.
2.210.S

	
	Condition reason:   To ensure compliance with the relevant Australian Standard and National Construction Code.

	34. 
	Erosion and Sediment Control Plan

	
	Before the issue of a construction certificate, the consent holder is to ensure that an erosion and sediment control plan is prepared in accordance with the following documents before it is provided to and approved by the certifier:

a. Council’s development control plan,

b. the guidelines set out in the NSW Department of Housing manual ‘Managing Urban Stormwater: Soils and Construction Certificate’ (the Blue Book), and

c. the ‘Do it Right On-Site, Soil and Water Management for the Construction Industry' (Southern Sydney Regional Organisation of Councils and the Natural Heritage Trust).

The consent holder must ensure the erosion and sediment control plan is kept onsite at all times during site works and construction.

2.211.S   

	
	Condition reason:   To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	35. 
	Dilapidation report

	
	Before the issue of a construction certificate, a dilapidation report must be prepared by a suitably qualified engineer detailing the structural condition of adjoining buildings, structures or works and public land, to the satisfaction of the certifier for the following properties:
· 113 Dutton Street, Yagoona
· 119 Dutton Street, Yagoona

Where access has not been granted to any adjoining properties to prepare the dilapidation report, the report must be based on a survey of what can be observed externally and demonstrate, in writing, to the satisfaction of the certifier, that all reasonable steps were taken to obtain access to the adjoining properties. 
No less than 14 days before any site work commences, adjoining building owners must be provided with a copy of the dilapidation report for their properties and a copy of the reports must be made available to Council upon request.

2.212.P

	
	Condition reason:   To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	36. 
	Mechanical Ventilation

	
	The premises must be ventilated in accordance with the Building Code of Australia and AS1668.1 and 2 – ‘The Use of Ventilation and Air- Conditioning in Buildings – Mechanical Ventilation in Buildings’.

Details of any mechanical ventilation and/or air-conditioning system complying with AS1668.1 and 2 – ‘The Use of Ventilation and Air- Conditioning in Buildings – Mechanical Ventilation in Buildings’, the Building Code of Australia and relevant Australian Standards must be prepared by a suitably qualified person and certified in accordance with Clause A2.2 (a) (iii) of the Building Code of Australia, to the satisfaction of the certifier before the issue of a construction certificate.

2.214  

	
	Condition reason:   To ensure compliance with the relevant Australian Standard and National Construction Code.

	37. 
	Combustible Cladding

	
	The external walls of the building including attachments must comply with the relevant requirements of the National Construction Code (NCC). Before the issue of a construction certificate and occupation certificate the certifier must:

a. Be satisfied that suitable evidence is provided to demonstrate that the products and systems proposed for use or used in the construction of external walls including finishes and claddings such as synthetic or aluminium composite panels comply with the relevant requirements of the NCC; and

b. Ensure that the documentation relied upon in the approval processes include an appropriate level of detail to demonstrate compliance with the NCC as proposed and as built.

2.216 

	
	Condition reason:  To ensure compliance with the BCA.

	38. 
	Retaining Walls

	
	Where Council approved cut or fill exceeds 200mm and stable batter of 1 vertical to 3 horizontal maximum grade cannot be achieved, then a masonry or other proprietary material retaining wall, intended and suitable for that purpose, shall be constructed within the development site. Note, filling of the site needs specific approval from Council. 

a. The retaining wall shall be located so that it will not impede or obstruct the natural flow of stormwater. Retaining walls exceeding 600mm in height shall be designed by an appropriately qualified person as defined in the Building and Development Certifiers Regulation 2020. Plans and details prepared and signed by an appropriately qualified person as defined in the Building and Development Certifiers Regulation 2020 are to be submitted to the certifier before the issue of the construction certificate.

b. All works associated with the construction of the wall, including backfilling and drainage, is to be located wholly within the allotment boundaries.

2.301   

	
	Condition reason:  To ensure works undertaken are carried out in a safe manner in accordance with relevant policies.  

	39. 
	Apply for Work Permit for Engineering Works

	
	The person having benefit of this Determination Notice shall apply for a Work Permit and obtain approval from Council, for any of the following applicable engineering works in front of the site, at their own expense:
a) 1 x Heavy Duty VFC at the property boundary fronting Dutton Street in accordance with Council’s VFC policy and standard drawing S-004. 
b) 1 x new Kerb inlet pit fronting Dutton lane in accordance with Council’s standard drawing S-101 with minimum 1.24m wide opening and 2.44m overall lintel,
c) Construction of new DN375 RCP council main pipe connecting new Kerb inlet pit to existing pit within Dutton street,
d) 1 x new stormwater connection to new kerb inlet pit fronting Dutton Street.
e) A new concrete footway paving along the site’s entire frontage to Dutton Street,
f) Removal of all driveway surfaces, reinstatement of laybacks to kerb and gutter and reshaping of the footway, all associated with redundant VFCs,
g) Repair of any damage to the public road including the footway occurring during building works, and
h) Reinstatement of the footway reserve and adjustment or relocation of existing public utility services to match the footway design levels as proposed on the approved Work Permit. Adjustment or relocation to any public utility services shall be carried out to the requirements of the public utility authority.

Note: Council is required to prepare a site survey and design in order to determine the necessary information. The person having benefit of this Determination Notice should make application and payment for the Work Permit at least twenty-one (21) days prior to the information being required and prior to the issue of the construction certificate. The Work Permit must be approved prior to any works commencing within the Council Road Reserve or on Council’s assets.
 

	
	Condition reason:  To provide  and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	40. 
	Basement Anchoring

	
	The basement of the development is located adjacent to a Council public road reserve. Separate approval and Work Permit is to be obtained from Council for any temporary or permanent anchoring works under Council's public road.

2.303

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	41. 
	Works Requiring a Work Permit

	
	As any works within, or use of, the footway or public road for construction purposes requires separate Council approval under Section 138 of the Roads Act 1993 and/or Section 68 of the Local Government Act 1993, Council requires the consent holder to obtain a Works Permit and or a Roadway / Footpath Building Occupation Permit  before the issue of any construction certificate for this development being issued where one or more of the following will occur, within, on or over the public footway or public road:

A PRIVATE CERTIFIER CANNOT ISSUE THESE PERMITS

WORKS REQUIRING A 'WORKS PERMIT'

a. Dig up, disturb, or clear the surface of a public footway or public road, 

b. Remove or interfere with a structure or tree (or any other vegetation) on a public footway or public road,

c. Connect a road (whether public or private) to a classified road, 

d. Undertake footway, paving, vehicular crossing (driveway), landscaping or stormwater drainage works within a public footway or public road,

e. Install utilities in, under or over a public road,

f. Pump water into a public footway or public road from any land adjoining the public road, 

g. Erect a structure or carry out a work in, on or over a public road,

h. Require a work zone on the public road for the unloading and or loading of vehicles,

i. Pump concrete from within a public road,

j. Stand a mobile crane within a public road,

k. Store waste and recycling containers, skips, bins and/or building materials on any part of the public road,

l. The work is greater than $25,000, and

m. Demolition is proposed.

The consent holder shall construct all works approved within the public road and footway under the supervision and to the satisfaction of Council and shall arrange for necessary inspections by Council whilst the work is in progress. 

The consent holder shall ensure that the person or company carrying out the work will carry public liability insurance to a minimum value of twenty million dollars and shall provide proof of the policy to Council, before commencing any work approved by the Work Permit including the Road Opening Permit. The policy must remain valid for the duration of the works. 

2.304   

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	42. 
	Finished surface levels

	
	Finished surface levels of all internal works and at the street boundary, including driveways, landscaping and drainage structures, must be as shown on relevant construction certificate plans. The levels at the street boundary must be consistent with the Street Boundary Alignment Levels issued by Council.

2.305   

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	43. 
	Stormwater Drainage

	
	Stormwater drainage from the proposed development shall be designed to comply with Council's Canterbury-Bankstown Development Control Plan 2023, Development Engineering Standards Guide and the BASIX Certificate requirements. A final detailed stormwater drainage system design shall be prepared by an appropriately qualified person as defined in the Building and Development Certifiers Regulation 2020 in accordance with the above requirements and shall generally be in accordance with the approved concept stormwater plans as shown in the table below. The final plan shall be certified by an appropriately qualified person as defined in the Building and Development Certifiers Regulation 2020 that it complies with the above stated Council DCP and guide, the BASIX Certificate requirements and the relevant Australian Standards.

· The proposed Kerb inlet pit fronting Dutton Lane shall be designed to comply with Council’s standard drawing S-101 with minimum 1.24m wide opening and 2.44m overall lintel.
Plan Name

Number

Date

Prepared By

Stormwater management plans
0496-C10, C-11, C15
04.09.2025
Enscape Studio


	
	Condition reason:   To ensure compliance with the relevant Australian Standard and National Construction Code.

	44. 
	Pump Out System

	
	The pump out drainage system for the driveway/access ramp and car parking area/open space area shall be provided in accordance with Council's Development Engineering Standards. The Engineer must design the Pump out drainage system to be in accordance with the Australian Standards AS 3500. Engineering details and manufacturers specifications for the pumps, switching system and sump pit shall be submitted to the certifier for approval before the issue of any construction certificate. The engineer must certify that the hydraulic design complies with the above relevant standards.

2.308 

	
	Condition reason:   To ensure the development is built and remains consistent with approved plans and documentation.

	45. 
	Pump Plans and Details

	
	Engineering details and manufacturers specifications for the pumps, switching system and sump pit shall be submitted to the certifier for approval before the issue of any construction certificate.

2.309 

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	46. 
	Driveway Design

	
	The design, layout, signage, line marking, lighting and physical controls of all off-street parking facilities must comply with the minimum requirements of Australian Standard AS/NZS 2890.1 Parking facilities Part 1: Off-street car parking, AS/NZS 2890.2 Parking facilities Part 2: Off-street commercial vehicle facilities and AS/NZS 2890.6 Parking facilities Part 6: Off-street parking for people with disabilities. The details must be submitted to and approved by the certifier before a construction certificate being issued.

Furthermore, for internal driveways with a gradient exceeding 10% (1 in 10), longitudinal profiles of all vehicular driveways and ramps shall be submitted for approval by the certifier before the issue of the construction certificate. The maximum grade of the driveway/ramp shall not exceed 25% and shall comply with AS 2890 parking series. The profile shall be drawn at a reduction ratio of 1 to 25 vertical and horizontal and shall be related to the datum used for the issue of the footway design levels and shall also show the road centre line levels, Council issued footway design levels and gutter levels. Council's Car Clearance Profile in Council's Development Engineering Standards, (Plan No. S 006) shall be used to design the profile.

2.313  

	
	Condition reason:   To ensure compliance with the relevant Australian Standard and National Construction Code.

	47. 
	Pavement Design

	
	An all-weather pavement shall be designed to withstand the anticipated wheel loads for all areas subjected to vehicular movements. Internal pavements specification prepared and certified by a qualified professional Civil Engineer to comply with the relevant Australian Standards, shall be submitted to the certifier for approval before the issue of a construction certificate.

2.314

	
	Condition reason:  To ensure compliance with the relevant Australian Standard and National Construction Code.

	48. 
	Gated Vehicle Access

	
	Where a car park is accessed by a security gate, that gate must be located at least 6 metres within the site from the property boundary with the street.

2.316

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	49. 
	Traffic Management Plan

	
	Before the issue of any construction certificate for this development, the consent holder must obtain approval from Council’s Traffic Section for a Site, Pedestrian and Traffic Management Plan (SPTMP). This Plan must address the measures that will be implemented for pedestrian safety and traffic management as specified below. 

A PRIVATE CERTIFIER CANNOT APPROVE YOUR SITE, PEDESTRIAN & TRAFFIC MANAGEMENT PLAN 

This plan shall include details of the following:

a. Proposed ingress and egress points for vehicles to and from the construction site;

b. Proposed protection of pedestrians, adjacent to the constructions site;

c. Proposed pedestrian management whilst vehicles are entering/exiting the construction site;

d. Proposed method of loading and unloading excavation machines, building material, construction materials and waste containers during the construction period;

e. Proposed traffic control measures such as advanced warning signs, barricades, warning lights, after hours contact numbers etc. are required to be displayed and shall be in accordance with Council's and the NSW Roads and Maritime Services requirements and AS1742.3.

f. Proposed route for transportation of bulk and excavation materials to and from the development site. 

The route for transportation to and from the development site of bulk construction and excavation materials shall be by the shortest practical route to the nearest "State  Road", with every effort to avoid school zones on public roads. . Alternate longer routes will only be considered in order to bypass school zones during school zone hours. If school zones cannot be avoided no heavy construction vehicle movements are to arrive or depart the site during signposted school zone periods 8:00am - 9:30am and 2:30pm - 4:00pm on school days.  The consent holder shall nominate the routes for approval by Council before commencement of any work on the site. All vehicles are to enter the on-street Works Zone adjacent to the site in a forward direction. U-turn and right-turn movements into the site, are generally not permitted.

An Agreement to Council's satisfaction, signed by the consent holder/owner specifying the approved route and acknowledging responsibility to pay Council for damages to public property adjacent to the site and for local roads along the transportation routes shall be lodged with Council before release of any Construction Certificate. All damage must be rectified upon completion of work.

Damage will be rectified as required by Council to remove unsafe conditions. All damage must be rectified upon completion of work to the satisfaction of Council.

The approved Site, Pedestrian and Traffic Management Plan is to be implemented before the commencement of any works on the construction site.

In addition, a TfNSW (formerly RMS) Approval / Road Occupancy Licence will be required for works on Regional or State Roads or within 100m of a traffic facility including roundabouts and traffic signals. Refer to Council's Development Engineering Standards for a list of Regional and State Roads.

Note: Approval by Council of a SPTMP may take up to six (6) moths. Accordingly, it is recommended the application to Council be submitted well in advance of the need for a construction certificate.

2.318

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	50. 
	Construction Site Management Plan

	
	Before the issue of a construction certificate, a Construction Site Management Plan (CSMP) must be prepared and approved by the certifier. The plan must include the following matters:
a. The location and materials for protective fencing and hoardings on the perimeter of the site; 

b. Provisions for public safety; 

c. Pedestrian and vehicular site access points and construction activity zones; 

d. Details of construction traffic management including:

i. Proposed truck movements to and from the site; 

ii. Estimated frequency of truck movements; and
iii.  Measures to ensure pedestrian safety near the site; 
e. Details of bulk earthworks to be carried out; 

f. The location of site storage areas and sheds; 

g. The equipment used to carry out works; 

h. The location of a garbage container with a tight-fitting lid; 

i. Dust, noise and vibration control measures;

j. The location of temporary toilets; 

k. The protective measures for the preservation of trees on-site and in adjoining public areas including measures in accordance with: 

i. AS 4970 – Protection of trees on development sites;

ii. An applicable Development Control Plan;
iii. An arborist’s report approved as part of this consent A copy of the construction site management plan must be kept on-site at all times while work is being carried out.
A copy of the construction site management plan must be kept on-site at all times while work is being carried out.
2.401.

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	51. 
	Work Vehicle Route

	
	The route for transportation to and from the development site of bulk and excavation materials shall generally be by the shortest possible route to the nearest "regional road", with every effort to avoid school zones on public roads. The consent holder shall nominate the route for approval by Council before commencement of any work on the site. An "Agreement" to Council's satisfaction, signed by consent holder specifying the approved route and acknowledging responsibility to pay Council for damages to public property adjacent to the site shall be lodged with Council before release of any construction certificate. All damage must be rectified before the issue of any occupation certificate.

2.402

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	52. 
	Traffic Signals on Site

	
	The consent holder is required to submit to Council the manufacturer’s specifications, design and operation of the ‘traffic signal’ facility to be installed along the driveway access ramp to the basement level. If required these details shall be illustrated on the plans to be submitted with the construction certificate application. The consent holder shall be responsible for the installation, operation and maintenance of the ‘traffic signal’ facility at no cost to Council.

2.403

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	53. 
	Sight Triangles on Plans

	
	Sight triangles are to be marked on relevant plans, being provided at the intersection of the driveway and the property boundary in accordance with AS 2890.1: ‘Figure 3.3 – Minimum Sight Lines for Pedestrian Safety’.  A splay extending 2 metres from the driveway edge along the front boundary and 2.5 metres from the boundary along the driveway shall be provided to give clear sight lines of pedestrians from vehicles exiting the site and is to be kept clear of any obstacles. Any structures, plantings or fencing within these triangles is to be a maximum height of 600mm to ensure sight lines are kept clear of any obstacles.  This shall be illustrated on plans submitted with the construction certificate.

2.406

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	54. 
	Return Bins to Council

	
	Before the commencement of any works, all domestic waste bins servicing the site are to be returned to Council.  

2.501

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	55. 
	Waste Management Plan

	
	Before the issue of a construction certificate, a Waste Management Plan (WMP) must be prepared and provided to the certifier. The plan must include the following matters:
The plan must be prepared 
a. in accordance with: 

i. the Environment Protection Authority’s Waste Classification Guidelines as in force from time to time, and

ii. a development control plan that provides for waste management that applies to the land on which the work or the clearing of vegetation is carried out, and 

b. include the following information—

iii. the contact details of the person removing waste, 

iv. an estimate of the type and quantity of waste, 
v. whether waste is expected to be reused, recycled or sent to landfill, 
vi. the address of the disposal location for waste. 
A copy of the waste management plan must be kept on-site at all times while work approved under the development consent is being carried out.
2.502   

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	56. 
	Plans to Include Bin Storage Area

	
	The construction certificate plans shall include details of the waste bin storage area. The bin storage area shall not be visible from the street. The bin storage area shall be located within the building or screened from the street by dense landscaping.

2.503

	
	Condition reason:   To ensure compliance with the relevant Canterbury-Bankstown policy.

	57. 
	Bin Carting Route

	
	The certifier must not issue a construction certificate unless provided with detailed plans that form part of the construction certificate which identify that the bin carting route from the communal bin storage room to the waste collection point identified on stamped plans complies with the following requirements as well as the requirements of Council’s “Waste Management Guide for New Developments”:

a.
Is direct and less than 10.0 in length, 

b.
Has a minimum width of 2.0 metres of hard surface;

c.
Is of non-slip material and free from obstacles and steps; 

d.
Is not located within a driveway or carpark; 

e.
Has a maximum grade of 1:30 (3%); 

f.
Has a kerbside ramp installed at the collection point; and

g.
Has compliance with Work, Health and Safety legislation and standards



	
	Condition reason:  To ensure the orderly collection of waste from the site.

	58. 
	Communal Bin Storage Room

	
	The certifier must not issue a construction certificate unless provided with detailed plans that form part of the construction certificate for the communal bin storage room that comply with the following requirements as well as the requirements of Council’s “Waste Management Guide for New Developments”:

a. Floors must be constructed of concrete at least 75mm thick and graded and drained to a Sydney Water approved drainage fitting; 

b. Floors must be finished so as to be non-slip with a smooth and even surface;

c. A designated room or enclosure and is to have a roof, with a minimum 2.1m unobstructed room height. 

d. Must be compatible with the overall design of the development;
e. Walls must be constructed of solid impervious material;

f. Ceilings must be finished with a smooth faced non-absorbent material capable of being cleaned;

g. Walls, ceiling and floors must be finished in a light colour;

h. An adequate supply of hot and cold water mixed through a centralised mixing valve with hose cock is to service the room;

i. A self-closing door openable from within the room;

j. Must be constructed to prevent the entry of birds and vermin;

k. Be provided with adequate light and ventilation. Light source must be through controlled light switches located both outside and inside the room;

l. Any doorways must be 2 metres wide and open outwards; and

m. Designed to fit the following bin allocations:
Number

Bin Size

Bin Type

4
1,100L

Garbage (Red)

6
1,100L

Recycling (Yellow)

3
240L

Garden (Green)



	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	59. 
	Bulky Waste Storage Room

	
	The certifier must not issue a construction certificate unless provided with detailed plans that form part of the construction certificate for the bulky waste storage room that comply with the following requirements as well as the requirements of Council’s “Waste Management Guide for New Developments”:

a. Floors must be constructed of concrete at least 75mm thick and graded and drained to a Sydney Water approved drainage fitting;

b. Floors must be finished so as to be non-slip with a smooth and even surface;

c. A designated room or enclosure and is to have a roof, with a minimum 2.1m unobstructed room height;

d. Must be compatible with the overall design of the development;

e. Walls must be constructed of solid impervious material;

f. Ceilings must be finished with a smooth faced non-absorbent material capable of being cleaned;

g. Walls, ceiling and floors must be finished in a light colour;

h. A self-closing door openable from within the room;

i. Must be constructed to prevent the entry of birds and vermin;

j. Any doorways must be 2 metres wide and open outwards; and

k. Designed to a minimum size of 5m2.



	
	Condition reason:  To ensure the orderly collection of waste from the site.

	60. 
	Temporary Bin Collection Area

	
	The certifier must not issue a construction certificate unless provided with detailed plans that form part of the construction certificate for the temporary bin collection area that comply with the following requirements as well as the requirements of Council’s “Waste Management Guide for New Developments”:

(For Collect and Return)

a.
Located less than 30 metres from the communal bin storage room;

b.
Located on the ground floor;

c.
Within 10 metres from the nominated kerbside collection point;

d.
Any doorways a minimum width of 2.0 metres;

e.
Be located fully within the property;

f.
Be of sufficient size to accommodate all bins, bins can be stacked


	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	61. 
	Waste Cupboards

	
	The certifier must not issue a construction certificate unless provided with detailed plans that form part of the construction certificate for the recycling cupboards that comply with the following requirements as well as the requirements of Council’s “Waste Management Guide for New Developments”:

a. Maximum distance of 30 metres from all dwellings;
b. Access is to be in accordance with AS 1428 (Set): ‘Design for access and mobility’;

c. Located directly adjacent to the chute hopper and contain only recycling bins;

d. Must be of adequate size to accommodate enough recycling bins, which allows for three days of recycling generated by the number of dwellings on that floor;

e. Designed to fit 240L bins facing forward;

f. Designed so the doors are of sufficient width to allow the transfer/rotation of 240L bins; and

g. The floor is to be constructed of a durable and impervious material with a smooth finish.

2.509

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	62. 
	On-Site Waste Collection

	
	Before the issue of any construction certificate, the certifier must receive written confirmation from Council, that Council has been provided to its satisfaction with the following: 

a. Detailed plans showing that the waste storage rooms identified on stamped plans will be capable of being accessed from the designed access roadway by a Heavy Rigid Vehicle (HRV) in accordance with AS2890.2, and that a loading area is available for the vehicle when collecting waste that meets the following requirements:

i. Within 5 metres of the all waste storage rooms or temporary holding area; 

ii. A separate parking area for the collection vehicle; and

iii. Include an extra 2 metres at the rear of the vehicle loading area. 

b. Certification from a suitably qualified engineer that the route of travel, loading area and entry and exit points will be constructed so as to support the following loading requirements:

i. Heavy Rigid Vehicle can enter and exit the site in a forward position;

ii. 30 tonne waste collection vehicles;

iii. Turning circle of 25 metres;

iv. Length of 12 metres; 

v. Clearance height of 4.5 metres / 6 metres

vi. Waste collection vehicle can access the basement, adequately manoeuvre into position, load bins and exit the basement in a forward position;

vii. The collection vehicle must be able to manoeuvre in the basement with limited need for reversing;

viii. The floor of the basement has been designed to carry the 30-tonne waste collection vehicle; and

ix. The gradient is to be suitable for a Heavy Rigid Vehicle as per AS2890.2. 

c. Detailed plans, specifications and other relevant information showing that the turntable identified on stamped plans:

i. Complies with required dimensions for an HRV as per AS2890.2, including the diameter for the turntable and required clearance heights; 

ii. Will always be available to waste collection vehicles; and

iii. Will be installed, operated and serviced on an ongoing basis, at no cost to Council.
2.511

	
	Condition reason:  To ensure the orderly collection of waste from the site.

	63. 
	Carpark Exhaust

	
	Before the issue of a construction certificate, the certifier is to ensure that all carpark exhaust does not directly vent into private or communal open space.

2.611

	
	Condition reason:  To ensure compliance with the relevant Australian Standard and National Construction Code.

	64. 
	Landscaping Plan

	
	A detailed landscape plan prepared by a qualified landscape architect or qualified landscape designer must be approved by the certifier before the issue of a construction certificate. The landscape plan must be prepared in accordance with Council’s DCP 2023 and must include the following features, notations and specifications:

a. The location of existing and proposed structures on the subject property/properties, including existing and proposed trees, impermeable areas, landscaped areas, deep soil zones, fixed furniture, shade structures, lighting, and other features,
b. Details of earthworks and soil depths, including mounding and retaining walls and planted boxes,

c. The location, number, pot size and type of chosen plant species. Details of planting procedures and long-term maintenance (if any), and

d. One 75ltr (minimum) major canopy tree shall be planted within the front setback to the development, and 

e. Details of drainage and watering systems (if any).

	
	Condition reason:   To ensure compliance with the relevant Canterbury Bankstown policy.

	65. 
	Landscape Management

	
	A site wide landscape management plan is to be submitted to and approved by the certifier before the issue of a construction certificate.. The plan is to demonstrate who is responsible for and how the landscape features will be installed and detail the responsibility of ongoing maintenance of the landscaping.

2.705   

	
	Condition reason:   To ensure compliance with the relevant Canterbury Bankstown policy.

	66. 
	Council’s Tree Management Order

	
	Approval is granted for the removal of the following trees:

· Any tree/s where the base of the trunk of the tree is located within 3 metres of the external wall of an approved dwelling;

· Any declared noxious plant. The applicant, builder and all contractors are to ensure that all noxious plants are properly identified, controlled and/or removed on this site without injury or death of any protected plants;

· Any tree species listed under clause 2.4 of Bankstown Development Control Plan 2015 Part B11 – Tree Management Order;

· Any of the trees as per Arboricultural Impact Assessment Report (Table 5.1) .
All tree removal works must comply with the Amenity Tree Industry – Code of Practice, 1998 (Workcover, NSW) and Guide to Managing Risks of Tree Trimming and Removal Work (Safe Work Australia 2016).

All other vegetation not specifically identified above, and protected by Councils Tree Management Order, is to be retained and protected from construction damage and pruning. The Tree Management Order protects trees over 5m in height.

2.703   

	
	Condition reason:   To ensure compliance with the relevant Canterbury Bankstown policy.

	67. 
	Design Verification SEPP 65

	
	A construction certificate shall not be issued until design verification from a qualified designer has been received. The design verification is a statement in which the qualified designer verifies that the plans and specifications achieve or improve the design quality of the development of which development consent was granted, having regard to the design quality principles set out in Schedule 1 of SEPP No. 65.

2.901 

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	68. 
	No Air conditioning units visible

	
	No air-conditioning equipment is to be visible from the public domain. Equipment and associated wiring shall:

a. Not be located on awnings or attached to the face of the building, 

b. Not be located on roofs in such a way that it is visible from any street, footpath or park,

c. Be visually screened if located 1.8 metres above ground level in other locations, and

d. Wiring shall be fully concealed.

All construction certificate documentation is to demonstrate compliance with these requirements.

2.902 

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	69. 
	Air conditioning units – BASIX requirements

	
	The location of any air-conditioning and hot water units and associated infrastructure must be located to ensure that they are not visible from the street, and that they do not result in a non-compliance with the relevant built form controls and private open space controls contained within the Apartment Design Guide. Confirmation from a suitably qualified architect that the BASIX commitments do not compromise the design guidance as contained within the Apartment Design Guide must be provided to the certifier before the issue of a construction certificate.

2.903 

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	70. 
	Hydrant boosters on plans

	
	All hydrant boosters and associated services and shield walls are to be contained within cabinets and / or designed to match the appearance of the main structure of the development.

2.904 

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	71. 
	Rooftop equipment

	
	All roof-top plant and associated equipment must be located within the approved building envelope and must not be visible from the public domain.

2.905

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.


BEFORE BUILDING WORK COMMENCES

	72. 
	Certifier details

	
	A construction certificate is required for the erection of a building in accordance with this Determination Notice. 

This Determination Notice does not authorise building work until a principal certifier has been appointed as the principal certifier for the work by (or with the approval of) the consent holder.

The following requirements apply before the commencement of building work in accordance with this Determination Notice: 

a. the principal certifier has, no later than two (2) days before the building work commences, notified the Consent Authority and the Council (if the council is not the Consent Authority) of their appointment as the principal certifier,
b. the principal certifier has, no later than two (2) days before the building work commences, notified the consent holder of any inspections that are required to be carried out in respect of the building work,

c. the person carrying out the building work has notified the principal certifier that the person will carry out the building work as an owner-builder, if that is the case,

d. the consent holder, if not carrying out the work as an owner-builder, has: 

i. appointed a principal contractor for the building work who must be the holder of a contractor licence if any residential building work is involved, and

ii. notified the principal certifier of the appointment, and

iii. unless that person is the principal contractor, notified the principal contractor of any inspections that are required to be carried out in respect of the building work,

e. the consent holder has given at least a 2-day notice to the Council, and the principal certifier if not the Council, of the person’s intention to commence the erection of the building.

3.202 

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	73. 
	Section 73 Compliance Certificate

	
	A Section 73 Compliance Certificate under the Sydney Water Act 1994 must be obtained from Sydney Water. It is recommended that the consent holder apply early for the certificate, as there may be water and sewer pipes to be built and this can take some time. This can also impact on other services and building, driveway or landscape design. Application can be made through an authorised Water Servicing Coordinator. For help either visit www.sydneywater.com.au > Plumbing, building and developing > Developing > Section 73 Compliance Certificates, or telephone 13 20 92.

3.203

	
	Condition reason:   To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	74. 
	Temporary fence or hoarding

	
	A fence must be erected around the area of the development site, except where an existing 1.8 metres high boundary fence is in good condition and can secure the area. Any new fencing must be temporary and at least 1.8 metres high. All fencing must be maintained throughout the construction period to ensure that the work area is secured.

Where the work is located within 3.6m of a public place, then a Type A or Type B hoarding must be constructed appropriate to the work proposed. An application for a Work Permit for such hoarding must be submitted to Council for approval before the commencement of building work/s. 

3.204 

	
	Condition reason:  To ensure works undertaken are carried out in a safe manner in accordance with relevant policies.

	75. 
	Dilapidation report

	
	No less than 14 days before the commencement of any site or building work, the adjoining owners must be provided with a copy of the dilapidation report for their properties: 

· 113 Dutton Street, Yagoona

· 119 Dutton Street, Yagoona.

3.205.S 

	
	Condition reason:   To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	76. 
	WC temporary toilet facilities on site

	
	Before the commencement of work, the consent holder must provide a temporary on-site toilet if access to existing toilets on site is not adequate/available. Temporary on-site toilet facilities must be installed and be adequately maintained throughout the construction period.

3.206

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	77. 
	Install Erosion control

	
	Before the commencement of any site or building work, the principal certifier must be satisfied the erosion and sediment controls in the erosion and sediment control plan, (as approved by the principal certifier) are in place until the site is rectified (at least 70% ground cover achieved over any bare ground on site). 

3.207

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	78. 
	Soil and water management warning sign

	
	Council’s warning sign for Soil and Water Management must be displayed throughout the construction period at the most prominent point of the site, visible to both the street and site.

3.208

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	79. 
	Sign with principal certifier details

	
	A sign must be erected in a prominent position on any site on which building work or demolition work is being carried out:

a. showing the name, address and telephone number of the principal certifier for the work, and
b. showing the name of the principal contractor (if any) for any building work and a telephone number on which that person may be contacted outside working hours, and

c. stating that unauthorised entry to the work site is prohibited.

Any such sign is to be maintained while the building work or demolition work is being carried out and must be removed when the work has been completed.
Note: This does not apply in relation to building work or demolition work that is carried out inside an existing building that does not affect the external walls of the building.
3.209.P

	
	Condition reason:  Prescribed condition under section 70 of the Environmental Planning and Assessment Regulation 2021.

	80. 
	Contract of Insurance

	
	In the case of residential building work for which the Home Building Act 1989 requires there to be a contract of insurance in force in accordance with Part 6 of that Act, that such a contract of insurance is in force before any building work authorised to be carried out by the consent commences.

3.210.P

	
	Condition reason:  Prescribed condition under section 69 of the Environmental Planning and Assessment Regulation 2021.

	81. 
	Residential building work

	
	Residential building work within the meaning of the Home Building Act 1989 must not be carried out unless the principal certifier for the development to which the work relates (not being the council) has given the council written notice of the following information —

a. In the case of work for which a principal contractor is required to be appointed—

i. the name and licence number of the principal contractor, and

ii. the name of the insurer by which the work is insured under Part 6 of that Act,

b. In the case of work to be done by an owner-builder—

i. the name of the owner-builder, and

ii. if the owner-builder is required to hold an owner-builder permit under that Act, the number of the owner-builder permit.

If arrangements for doing the residential building work are changed while the work is in progress so that the information notified becomes out of date, further work must not be carried out unless the principal certifier for the development to which the work relates (not being the Council) has given the Council written notice of the updated information.
3.211.P

	
	Condition reason:   Prescribed condition under section 71 of the Environmental Planning and Assessment Regulation 2021.

	82. 
	Tree protection measures

	
	Before the commencement of any site or building work, the principal certifier must ensure the measures for tree protection detailed in the construction site management plan are in place.

3.801.S

	
	Condition reason:  To protect the natural environment of the development site and adjoining lands.


DURING BUILDING WORK
	83. 
	Procedure for Critical Stage Inspections

	
	While building work is being carried out, the work must not continue after each critical stage inspection unless the principal certifier is satisfied the work may proceed in accordance with this consent and the relevant construction certificate.

4.101.S

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	84. 
	Works in accordance with Building Code of Australia (BCA)

	
	Building work must be carried out in accordance with the requirements of the Building Code of Australia (BCA).

4.201.P

	
	Condition reason:   Prescribed condition - EP&A Regulation clause 98(1)(a).

	85. 
	BASIX commitments

	
	While building work is being carried out, the consent holder must undertake the development strictly in accordance with the commitments listed in the BASIX certificate(s) approved by this consent, for the development to which the consent applies.

4.203.P

	
	Condition reason:   Prescribed condition under section 75 of the Environmental Planning and Assessment Regulation 2021.

	86. 
	Hours of Work

	
	Site work must only be carried out between the following times –

a. 7.00 am and 5.00 pm on Monday to Saturday.
b. No construction is to be carried out at any time on a Sunday or a public holiday.

Site work is not to be carried out outside of these times except where there is an emergency, or for urgent work directed by a police officer or a public authority.

4.204.S

	
	Condition reason:   To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	87. 
	Noise and Vibration

	
	While site work is being carried out, noise generated from the site must be controlled in accordance with the requirements of the approved documentation. 

Where no noise and vibration management plan is approved under this consent, the certifier is to ensure that any noise caused by demolition, vegetation removal or construction does not exceed an LAeq (15 min) of 5dB(A) above background noise, when measured at any lot boundary of the property where the site work is being carried out.

4.205.S

	
	Condition reason:   To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites

	88. 
	Unexpected Finds

	89. 
	In the instance works cause the generation of odours or uncovering of unexpected contaminants works are to immediately cease, Council is to be notified and a suitably qualified environmental consultant appointed to further assess the site. The exposed material/excavation is to be evaluated by the supervising environmental consultant and an appropriate response determined in consultation with the applicant, which is agreed to by Council.

Council may also request that an NSW EPA Accredited Site Auditor is involved to assist with the assessment of any unexpected finds, review any contamination information, prepare a site audit report, and site audit statement. The applicant must adhere to any additional conditions which may be imposed by the NSW EPA Accredited Site Auditor.

	90. 
	Condition reason:   To ensure that the development complies with Council’s Environmental Health Policies.

	91. 
	Disposal of Excavated Soil

	92. 
	93. All soils to be excavated and disposed of from the site must be analysed and classified by a suitably qualified environmental consultant, in accordance with relevant NSW EPA guidelines including the ‘Waste Classification Guidelines’ (NSW EPA, 2014) prior to off-site disposal.

All waste material for disposal to be transported to an appropriately licensed waste facility by an EPA licensed waste contractor in accordance with relevant NSW EPA guidelines. Receipts for the disposal of the waste must be submitted to Council prior to issuing of an occupation certificate.

	94. 
	Condition reason: To ensure compliance with the relevant New South Wales legislation.

	95. 
	Demolition and Construction Waste

	96. 
	All waste material generated during demolition and construction must be disposed of at an appropriately licensed waste facility for the specific waste. 

All waste must be transported by a contractor licensed to transport the specific waste, and in vehicles capable of carting the waste without spillage and meeting relevant requirements and standards. All loads must be covered prior to vehicles leaving the site.

	97. 
	Condition reason: To ensure that the development complies with Council’s Environmental Health Policies.

	98. 
	Duty to Report Contamination

	99. 
	If the Duty to Report contamination to the NSW EPA under Section 60 of the Contaminated Land Management Act 1997 is triggered, Council must be notified within seven (7) days of the notification to the NSW EPA.

	100. 
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	101. 
	Importation of Fill

	102. 
	Any fill imported onto the site must be virgin excavated natural material or excavated natural material, classified as such in accordance the ‘Waste Classification Guidelines’ (NSW EPA, 2014) or excavated natural material meeting the requirements of the Excavated Natural Material Exemption (NSW EPA, 2014). 

Certificates verifying that imported fill is virgin excavated natural material or excavated natural material must be provided to Council prior to the issue of an occupation certificate. All imported fill must be compatible with the existing soil characteristics of the site.

	103. 
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	104. 
	Surveys by a registered surveyor

	
	While building work is being carried out, the positions of the following must be measured and marked by a registered surveyor and provided to the principal certifier: 
a. All footings / foundations in relation to the site boundaries and any registered and proposed easements 
b. At other stages of construction – any marks that are required by the principal certifier.
4.206.S

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	105. 
	Civil and Hydraulic engineering works

	
	All civil and hydraulic engineering works on site must be carried out in accordance with Council's Development Engineering Standards.  All Civil and Hydraulic engineering works associated with Council's assets and infrastructure must be carried out in accordance with Council's Work Permit requirements and to Council's satisfaction.

4.301

	
	Condition reason:  To ensure compliance with the relevant Canterbury Bankstown policy.

	106. 
	Stormwater drainage system

	
	The stormwater drainage system shall be constructed in accordance with Council's Development Engineering Standards and the engineering plans and details approved by the principal certifier. Should the consent holder encounter any existing, live, underground stormwater drainage pipes, which carry flow from upstream properties, then they must maintain the stormwater flow and re-route the stormwater pipes around the subject building or structures at their own expense.
4.302

	
	Condition reason:  To ensure compliance with the relevant Canterbury Bankstown policy.

	107. 
	Driveway adequacy

	
	A suitably qualified Professional Civil or Structural Engineer shall be engaged by the developer to carry out inspections relating to construction of internal driveways and parking areas. The work shall be carried out in accordance with the approved plans and specifications and certification from the Civil or Structural Engineer is to be provided upon completion.

4.306

	
	Condition reason:  To ensure compliance with the relevant Canterbury Bankstown policy.

	108. 
	Responsibility for Changes to Public Infrastructure

	
	While site work is being carried out, any costs incurred as a result of the approved removal, relocation or reconstruction of infrastructure (including ramps, footpaths, kerb and gutter, light poles, kerb inlet pits, service provider pits, street trees or any other infrastructure in the street footpath area) must be paid as directed by the consent authority.

4.307.S

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	109. 
	Excavated safety

	
	All excavations and backfilling must be executed safely and in accordance with the relevant Australian Standards. 

If the development involves an excavation that extends below the level of the base of the footings of a building, structure or work (including any structure or work within a road or rail corridor) on adjoining land, the consent holder must, at their own expense:

a. Protect and support the building, structure or work from possible damage from the excavation, and

b. Where necessary, underpin the building, structure or work to prevent any such damage.

This consent condition does not apply if the consent holder owns the adjoining land or the owner of the adjoining land has given consent in writing to that condition not applying.

The owner of any affected buildings is not liable for any part of the cost of work carried out for the purposes of this clause, whether carried out on the allotment of land being excavated or on an adjoining allotment of land.

4.308

	
	Condition reason:  To ensure compliance with the relevant Australian Standard and National Construction Code.

	110. 
	Shoring and adequacy of adjoining properties

	
	If the development involves an excavation that extends below the level of the base of the footings of a building, structure or work on adjoining land (including any structure or work within a road or rail corridor), the consent holder must, at their own expense —

a. Protect and support the building, structure or work from possible damage from the excavation, and
b. Where necessary, underpin the building, structure or work to prevent any such damage.

This condition does not apply if the consent holder owns the adjoining land or the owner of the adjoining land has given consent in writing to that condition not applying.
4.309.P

	
	Condition reason:   Prescribed condition under section 74 of the Environmental Planning and Assessment Regulation 2021.

	111. 
	Excavation – Water

	112. 
	All excavations must be kept free from the accumulation of water. Prior approval must be sought from Council to discharge any water into the Council’s stormwater drainage system. Other options for the disposal of water include disposal to sewer with prior approval from Sydney Water, or off-site disposal by a liquid waste transporter for treatment/disposal to an appropriate waste treatment/processing facility.

	113. 
	Condition reason:   To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites

	114. 
	Retaining walls

	
	If soil conditions require it, retaining walls or other approved methods of preventing movement of the soil must be provided, and adequate provisions must be made for drainage. Should it be required, separate approval must be obtained for retaining walls.  
4.310

	
	Condition reason:  To ensure works undertaken are carried out in a safe manner in accordance with relevant policies.  

	115. 
	Inspection by resource recovery

	
	No work may be carried out to construct the ground floor slab unless the principal certifier is satisfied and provides evidence to Council of that satisfaction that the waste facilities within the basement comply with the specifications of the stamped plans. Council can be contacted on 9707 9000.

4.501

	
	Condition reason:   To ensure the development is built and remains consistent with approved plans and documentation.

	116. 
	Waste management

	
	While site work is being carried out:

a. all waste management must be undertaken in accordance with the waste management plan, and 

b. upon disposal of waste, records of the disposal must be compiled and provided to , detailing the following:

i. The contact details of the person(s) who removed the waste

ii.  The waste carrier vehicle registration

iii.  The date and time of waste collection

iv.  A description of the waste (type of waste and estimated quantity) and whether the waste is to be reused, recycled or go to landfill

v. The address of the disposal location(s) where the waste was taken 

vi. The corresponding tip docket/receipt from the site(s) to which the waste is transferred, noting date and time of delivery, description (type and quantity) of waste.

If waste has been removed from the site under an EPA Resource Recovery Order or Exemption, records in relation to that Order or Exemption must be maintained and provided to the principal certifier and council. 

4.502.S

	
	Condition reason:   To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	117. 
	Comply with Waste management plan

	
	The requirements of the submitted Waste Management Plan shall be complied with at all times that work is being carried out. Without limiting the foregoing, compliance shall include the following:

a. The disposal of any demolition and construction waste must be undertaken in accordance with the requirements of the Protection of Environment Operations Act 1997; and

b. All waste on site is to be stored, handled and disposed of in such a manner as to not create air pollution, offensive noise or pollution of land and water as defined by the Protection of Environment Operations Act 1997; and

c. Generation, storage, treatment and disposal of hazardous waste is conducted in accordance with the relevant waste legislation administered by the EPA and relevant Occupational Health and Safety legislation administered by WorkCover NSW; and

d. All waste generated (including excavated materials) which cannot be reused or recycled must be transported to a facility which can lawfully accept it; and

e. Records are required regarding the details and location of the disposal of all demolition and construction waste (including excavated material), description of waste and are to be kept on site as evidences of lawful disposal. Records are to include receipts and weighbridge dockets which verify material types and volumes, time and date of disposal, waste vehicle rego, and confirmation of the waste disposal facility. Records/ details are also to be kept of person removing the waste; and 

f. All materials and resources that are to be stored on site during construction works are contained on the site; and

g. The provisions of the Protection of Environment Operations Act 1997 must be complied with when placing/stock piling loose material, disposal of concrete waste or activities which have potential to pollute drains and water courses; and

h. The storage of waste and recycling containers must be within the boundaries of the development site at all times. Public footways and roads must not be used for the storage of any waste and must be kept clear of obstructions during all construction works. 
4.503

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	118. 
	Hazardous finds

	
	Any new information revealed during building work/s that has the potential to alter previous conclusions about site contamination or hazardous materials shall be immediately notified to the Council and the principal certifier. Works are to cease until the new information is evaluated by an appropriately qualified and experienced environmental consultant and an appropriate response determined by the consent holder and/or owner which is agreed to by Council. Council may also request that a NSW EPA accredited site auditor is involved to assist with the assessment of the new contamination information.
4.601

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	119. 
	No Stockpiling

	
	There must not be any stockpiling of building spoil, materials, or storage of equipment on the public road during the construction period. The footway and the road reserve must always be maintained in a safe condition. No work can be carried out on the public road, including the footway, unless a Work Permit authorised by Council has been obtained. 

4.605

	
	Condition reason:  To ensure works undertaken are carried out in a safe manner in accordance with relevant policies.

	120. 
	Keep free of water

	
	All excavations must be kept free from the accumulation of water. Before approval must be sought from Council to discharge any water into the Council’s stormwater drainage system. Other options for the disposal of water include disposal to sewer with before approval from Sydney Water, or off-site disposal by a liquid waste transporter for treatment/disposal to an appropriate waste treatment/processing facility.
4.609

	
	Condition reason:  To ensure works undertaken are carried out in a safe manner in accordance with relevant policies.   

	121. 
	Car wash bunding

	
	A carwash bay is to be bunded and connected to the sewer system to dispose of wastewater in accordance with the requirements contained in Council's Development Engineering Standards.

4.612

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	122. 
	Implementation of the site management plans

	
	While site work is being carried out: 

a. the measures required by the construction site management plan (where approved) and the erosion and sediment control plan must be implemented at all times, and
b. a copy of these plans must be kept on site at all times and made available to council officers upon request.

4.701.S

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	123. 
	Boundary fencing

	
	Where replacement boundary fencing is required to be installed, it must be 1.8 metres high unless otherwise shown on the approved plans or as stipulated within this Determination Notice. The materials and colours of the fence must be selected in consultation with the adjoining property owners unless the design of the fence and the type of material is specified to allow for overland flow. Fencing forward of the building line must not be greater than 1.2 metres in height. All costs related to fencing must be borne by the consent holder.
4.702

	
	Condition reason:   To ensure compliance with the relevant Canterbury Bankstown policy.

	124. 
	Tree protection during work

	
	While site work is being carried out, all required tree protection measures must be maintained in good condition in accordance with: 

a. the construction site management plan (where approved) under this consent, 
b. the relevant requirements of AS 4970 Protection of trees on development sites, 

c. Council’s relevant development control plan (in force as at the date of determination of this consent) and d)any arborist’s report approved under this consent. 

This includes maintaining adequate soil grades and ensuring all machinery, builders refuse, spoil and materials remain outside tree protection zones
4.807.S

	
	Condition reason:  To protect the natural environment of the development site and adjoining lands.

	125. 
	Tree protection

	
	All work carried out on or around protected trees during demolition, clearing and construction shall comply with Australian Standard AS 4373 – ‘Pruning of amenity trees’ and Australian Standard AS 4970 – ‘Protection of trees on development sites’. Site specific conditions relating to tree protection shall take precedence over this requirement.
4.806

	
	Condition reason:  To protect the natural environment of the development site and adjoining lands.

	126. 
	Threatening of trees

	
	If any trees to be retained and protected are threatened by demolition, building or other site works through accidental omission or unforeseen circumstances, the approving authority is to be notified immediately in writing before such work is continued so that this issue can be resolved.
4.810

	
	Condition reason:  To protect the natural environment of the development site and adjoining lands.

	127. 
	Discovery of relics and Aboriginal objects

	
	While site work is being carried out, if a person reasonably suspects a relic of Aboriginal object is discovered:

a. the work in the area of the discovery must cease immediately; 

b. the following must be notified 

i. for a relic – the Heritage Council; or

ii. for an Aboriginal object – the person who is the authority for the protection of Aboriginal objects and Aboriginal places in New South Wales under the National Parks and Wildlife Act 1974, section 85.

Site work may recommence at a time confirmed in writing by:

a. for a relic – the Heritage Council; or 

b. for an Aboriginal object – the person who is the authority for the protection of Aboriginal objects and Aboriginal places in New South Wales under the National Parks and Wildlife Act 1974, section 85.

In this condition:

“relic” means any deposit, artefact, object or material evidence that:

 relates to the settlement of the area that comprises New South Wales, not being Aboriginal settlement, and

 is of State or local heritage significance; and 

“Aboriginal object” means any deposit, object or material evidence (not being a handicraft made for sale) relating to the Aboriginal habitation of the area that comprises New South Wales, being habitation before or concurrent with (or both) the occupation of that area by persons of non-Aboriginal extraction and includes Aboriginal remains.
4.901.S

	
	Condition reason:   To ensure the protection of objects of potential significance during works

	
	


BEFORE ISSUE OF AN OCCUPATION CERTIFICATE
	
	Condition

	128. 
	Occupation certificate

	
	The occupation or use of the building must not commence unless an occupation certificate has been issued.

5.201

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	129. 
	Number of car parking spaces

	
	Forty two (42) off-street car parking spaces shall be provided and maintained for the use of visitor and employees to the premises in accordance with the submitted plans. Such spaces are to be sealed and line marked and maintained for the lifetime of the development.

5.105

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	130. 
	Allocation of car parking spaces

	
	Forty two (42) off-street car spaces being provided in accordance with the submitted plans. 
Note: Four (4) of the required car parking spaces are to be provided for people with mobility impairment in accordance with AS 2890.1. All car parking spaces shall be allocated and marked according to these requirements.
5.106

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	131. 
	Accessible car allocations

	
	For residential development, accessible car parking spaces for people with mobility impairment are only to be allocated as visitor parking or to adaptable units. Where allocated to adaptable units, the units and car spaces must be assigned to the unit in any future strata subdivision of the building.

5.107

	
	Condition reason:  To ensure orderly development of land.

	132. 
	Encroachment on Council land

	
	Before the issue of an occupation certificate, the principal certifier must ensure that no portion of the approved structure, including gates and doors during opening and closing operations, provides for encroachment upon Council’s footpath area.

5.202

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	133. 
	Slab certification

	
	A report as prepared by a registered surveyor must be submitted to the principal certifier verifying that the reduced level (RL) of the finished floor level at each level, the height of external walls, the maximum reduced level (RL) of roof structures / roof eaves overhangs and the external wall setbacks to the property boundaries all conform with the approved plans.

5.203

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	134. 
	Preservation of survey marks

	
	Before the issue of an occupation certificate, a registered surveyor must submit documentation to the principal certifier which demonstrates that:

a. no existing survey mark(s) have been removed, damaged, destroyed, obliterated or defaced, or 

b. any survey mark(s) that were damaged, destroyed, obliterated or defaced have been re-established in accordance with the Surveyor General’s Direction No. 11 – Preservation of Survey Infrastructure.

5.204.S

	
	Condition reason:   To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.  

	135. 
	Post-construction dilapidation report

	
	Before the issue of an occupation certificate, a post-construction dilapidation report must prepared by a suitably qualified engineer, to the satisfaction of the principal certifier, detailing whether:

a. after comparing the pre-construction dilapidation report to the post-construction dilapidation report required under this condition, there has been any structural damage to any adjoining buildings; and

b. where there has been structural damage to any adjoining buildings, that it is a result of the work approved under this development consent, and 

c. a copy of the post-construction dilapidation report must be provided to council (where council is not the principal certifier or a principal certifier is not required) and to the relevant adjoining property owners.

5.205.S

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.  

	136. 
	Mechanical ventilation

	
	Before the issue of an occupation certificate, the principal certifier must ensure that the car park is ventilated in accordance with the Building Code of Australia and, where necessary, Australian Standard AS 1668, Parts 1 and 2. Ventilation must be controlled by carbon monoxide monitoring sensors to ensure compliance with occupant health requirements.

5.206

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	137. 
	Completion of Public Utility Services

	
	Before the issue of the relevant occupation certificate, confirmation must be obtained from the relevant authority that any adjustment or augmentation of any public utility services including gas, water, sewer, electricity, street lighting and telecommunications, required as a result of the development, have been completed and this confirmation must be provided to the principal certifier.

5.207.S

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	138. 
	Section 73 certificate

	
	The Section 73 compliance certificate under the Sydney Water Act 1994 must be submitted to the principal certifier before the issue of an occupation certificate.

5.208

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	139. 
	Mechanical ventilation

	
	Before issue of an occupation certificate and following the completion, installation, and testing of all the mechanical ventilation systems, a Mechanical Ventilation Certificate of Completion and Performance in accordance with Clause A2.2 (a) (iii) of the Building Code of Australia, must be submitted to the principal certifier.

5.209

	
	Condition reason:  To ensure compliance with the relevant Australian Standard and National Construction Code.

	140. 
	Work Permit Compliance required

	
	An occupation certificate must not be issued until all conditions relating to demolition, building and subdivision works have been satisfied and Council has issued a Work Permit Compliance Certificate (where applicable).

5.301

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	141. 
	Repair of infrastructure

	
	Before the issue of an occupation certificate:

a. any public infrastructure damaged as a result of the carrying out of work approved under this consent (including damage caused by, but not limited to, delivery vehicles, waste collection, contractors, sub-contractors, concreting vehicles) must be fully repaired to the written satisfaction of council, and at no cost to council, or

b. if the works in (a) are not carried out to council’s satisfaction, council may carry out the works required and the costs of any such works must be paid as directed by council and in the first instance will be paid using the security deposit required to be paid under this consent.

5.302.S

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	142. 
	Works-as-executed plans and any other documentary evidence

	
	Before the issue of the relevant occupation certificate,  works-as-executed plans, any compliance certificates and any other evidence confirming the following completed works must be submitted to the satisfaction of the principal certifier:
a. All stormwater drainage systems and storage systems, and 
b. The following matters that council requires to be documented in accordance with the Councils relevant Development Control Plan. 
c. A copy of the plans must be provided to council with the occupation certificate.

5.303.S

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	143. 
	Restriction of use / covenant

	
	The developer shall register, on the title of the subject property, a Restriction on the Use of Land and Positive Covenant, in accordance with the standard terms for "Registration of OSD on title", as outlined in Council's Development Engineering Standards and in accordance with the appropriate provisions of the Conveyancing Act 1919. 

Where subdivision is not proposed, the surveyor shall show the location of the "On-Site Stormwater Detention System" on an A4 size site plan attached to the Section 88E Instrument to be registered, on the title of the subject property, before the issue of the Final Occupation Certificate. Alternatively, where subdivision is proposed, the developer shall register, on the title of the subject property, a Restriction on the Use of Land and Positive Covenant, in accordance with the standard terms for "Registration of OSD on title", as outlined in Council’s Development Engineering Standards and in accordance with the appropriate provisions of the Conveyancing Act. The surveyor shall show the location of the "On-Site Stormwater Detention System" on the plan of subdivision. The developer shall submit evidence of the final registration of the Restriction and Positive Covenant on the title of the property, to Council.

5.304

	
	Condition reason:   To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	144. 
	Confirmation of waste facilities

	
	No occupation certificate may be issued until such time as written confirmation has been received from Council that all waste management facilities and associated access have been constructed in accordance with the requirements of this consent.  The waste management facilities include the path of travel for all waste, from unit to point of waste collection, waste storage room sizing, access to water and sewer connections, finished materials, access and doorway dimensions, truck turntables, bin tugs and bin lifting equipment.

5.501

	
	Condition reason:  To ensure compliance with the relevant Canterbury Bankstown policy.

	145. 
	Agreement with Council

	
	Before the issue of any occupation certificate, an agreement must be entered into with Council on terms satisfactory to Council for the collection of waste.

5.502

	
	Condition reason:  To ensure compliance with the relevant Canterbury Bankstown policy.

	146. 
	Removal of Waste Upon Completion

	
	Before the issue of an occupation certificate: 

a. all refuse, spoil and material unsuitable for use on-site must be removed from the site and disposed of in accordance with the waste management plan, and
b. written evidence of the waste removal must be provided to the satisfaction of the principal certifier.


	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	147. 
	Completion of Landscape and Tree Works

	
	Before the issue of an occupation certificate, the principal certifier must be satisfied all landscape and tree-works have been completed in accordance with approved plans and documents and any relevant conditions of this consent.

5.701.S

	
	Condition reason:  To protect the natural environment of the development site and adjoining lands and to ensure the development is built and remains consistent with approved plans and documentation.

	148. 
	Key card access

	
	Before the issue of an occupation certificate, the principal certifier must ensure that access to the residential lobby is secured through a key card, swipe card, intercom or other method to restrict access to the lobby to only residents or visitors.

5.901

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	149. 
	Master locks

	
	Before the issue of an occupation certificate, the principal certifier must ensure that the letterboxes installed have non-master key locks, to prevent theft and fraud.

5.902

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	150. 
	CCTV surveillance cameras

	
	Before the issue of an occupation certificate, the principal certifier is to ensure that on-site CCTV surveillance cameras have been strategically installed and that they will operate and be maintained throughout the development with particular coverage to:

a. principal entrance/s and exits;

b. all areas within the premise occupied by the public (excluding toilets);

c. staircases in multilevel premises; and

d. the area within a 10m radius external to the public entrance(s) to the premise.

Installation of the surveillance system is to ensure suitable and clearly visible signage is displayed at the principal entrance(s) to the premise and in a prominent position on each floor accessible to the public, in lettering not less than 50mm in height with the words “Closed Circuit Television in use on these premises”.

All CCTV recording equipment and cameras shall be of high-grade digital quality capable of establishing the population and identification of patrons, offenders and incidents within the depth of field view of the cameras. 

CCTV recording discs or hard drive recordings shall be retained for 28 days before being re-used, destroyed or deleted. Time and date shall be auto recorded on the disc or hard drive. The CCTV recording equipment shall be capable of reproducing a CD, DVD, USB or other appropriate digital copy of recorded footage on demand of Council or Police Officers either immediately or within 12 hours of the request being made. Copy discs must be handed to Council, Police Officer or Special Inspectors as required.

All CCTV recording devices and cameras shall be regularly checked to ensure the equipment is operating correctly. If it is discovered at any time that the equipment is not in full operating order all reasonable steps must be taken to repair the system as soon as practicable. Where the system will not be functioning in full operating order for a period of longer than 24 hours the manager/licensee is to notify the relevant Local Area Commander of the NSW Police.

All CCTV recording devices and cameras shall be operated at all times when the premises are open to the public and, where premises do not operate 24 hours a day, continuously for at least 1 hour before opening and closing times of the premises.

The CCTV recording device shall be secured within the premises and only be accessible to senior management personnel so as to maintain the integrity of the recorded footage. 

Camera views are not to be obstructed by temporary or permanent structures, signage or other impediments.

5.903

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	151. 
	Property numbering

	
	The dwellings must be readily identified from the street with the allocated house numbers. An official "property numbering" letter is issued to the consent holder indicating the proposed numbering of the new development. House numbering without Council's written approval is not permitted.

5.904

	
	Condition reason:  To ensure compliance with the relevant Canterbury Bankstown policy.

	152. 
	Lighting must be provided to entries

	
	Lighting must be provided to the entries of the dwellings, driveways and parking areas to promote a high level of safety and security at night and during periods of low light. All lighting must be hooded, shielded or directed away from neighbouring dwellings to minimise glare and associated nuisances to residents.

5.906

	
	Condition reason:   To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	153. 
	Design of lighting

	
	Any lighting on the site shall be designed so as not to cause nuisance to other residences in the area or to motorists on nearby public roads and to ensure no adverse impact on the amenity of the surrounding area by light overspill. All lighting shall comply with the Interim Australian Standard AS 4282 – ‘The Control of the Obtrusive Effects of Outdoor Lighting’.

5.907

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites and to ensure compliance with the relevant Australian Standard and National Construction Code.

	154. 
	Design principles SEPP 65

	
	Before the issue of any occupation certificate a design verification from a qualified designer shall be submitted to the principal certifier. The design verification is a statement in which the qualified designer verifies that the development as shown in the plans and specifications in respect of which the construction certificate was issued, having regard to the design quality principles set out in Part 2 of SEPP No. 65.

5.908

	
	Condition reason:  To ensure compliance with the relevant New South Wales legislation.

	
	


OCCUPATION AND ONGOING USE

	
	Condition

	155. 
	Communal facilities

	
	The communal facilities must be available for the use all residents of the building, and must be operated as common property on any strata subdivision of the site, with no exclusive use rights given.

7.104

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	156. 
	Parking spaces

	
	No part of the common property, apart from the visitor vehicle spaces which are to be used only by visitors to the building, and service vehicle spaces which are to be used only by service vehicles, is to be used for the parking or storage of vehicles or boats.

7.106

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	157. 
	Car Wash Bay – Multistorey Residential

	158. 
	The designated car wash bays must be designed and constructed to ensure that wastewater is discharged to the sewer in accordance with the requirements of Sydney Water.


	159. 
	Condition reason:  To ensure compliance with the relevant Australian Standard and National Construction Code.

	160. 
	Acoustic Assessment

	161. 
	Should a noise issue arise, the owner and/or occupier must, upon request by Council, employ the services of a suitably qualified acoustic consultant who has not previously been involved with the development to undertake a post-occupation assessment of the development and complete an acoustic report with recommendations to rectify the noise issue. A copy of this acoustic assessment report must be submitted to Council for approval and from there noise attenuation works must be implemented. Submission of the acoustic report must be within 30 days from the date requested by Council.

Note: Suitably qualified acoustic consultant means a consultant who possesses the qualifications to render them eligible for membership of the Australian Acoustical Society, Institution of Engineers Australia or the Association of Australian Acoustical Consultants at the grade of member.


	162. 
	Condition reason: To protect the amenity of the surrounding area.

	163. 
	Compliance with Noise Control Legislation

	164. 
	The applicant must ensure that all activities within the premises comply with the relevant sections of the Protection of the Environment Operations Act 1997 and Regulations and the Noise Policy for Industry (NSW EPA, 2017).



	165. 
	Condition reason:   To protect the amenity of the surrounding area.

	166. 
	Vibration

	167. 
	The use of the premises and the operation of plant and equipment must not give rise to the transmission of a vibration nuisance or damage to other premises as defined in the ‘Assessing Vibration: A Technical Guideline’ (NSW Department of Environment and Conservation, 2006).



	168. 
	Condition reason:   To protect the amenity of the surrounding area.

	169. 
	POEO – General

	170. 
	Any activity carried out in accordance with this approval must not give rise to offensive odour, offensive noise or pollution of air, land or water as defined in the Protection of the Environment Operations Act 1997 and Regulations.



	171. 
	Condition reason:   To ensure compliance with the relevant New South Wales legislation.

	172. 
	Odour Emission Control

	173. 
	There are to be no emissions or discharges from the premises which will give rise to an offence under the Protection of the Environment Operations Act 1997 and Regulations.

Emission control equipment must be provided in the mechanical exhaust system serving the appliances, to effectively minimise the emission of odours, vapours and oils. Details of the proposed emission control equipment must be provided in the relevant plans and specifications for the construction certificate for the subject works.

Details demonstrating compliance with the requirements of this condition are to be submitted to the satisfaction of the principal certifier prior to the issue of any construction certificate.



	174. 
	Condition reason:   To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites

	175. 
	Excavation – Water

	176. 
	All excavations must be kept free from the accumulation of water. Prior approval must be sought from Council to discharge any water into the Council’s stormwater drainage system. Other options for the disposal of water include disposal to sewer with prior approval from Sydney Water, or off-site disposal by a liquid waste transporter for treatment/disposal to an appropriate waste treatment/processing facility.



	177. 
	Condition reason:   To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites

	178. 
	General Amenity

	179. 
	The operation of the development must not adversely affect the amenity of the neighbourhood or interfere unreasonably with the comfort or repose of a person who is outside the premises by reason of the emission or discharge of noise, fumes, vapour, odour, steam, soot, ash, dust, wastewater, waste products, grit, oil or other harmful products.



	180. 
	Condition reason: To protect the amenity of the surrounding area.

	181. 
	Lighting

	182. 
	Any lighting of the premises must be installed in accordance with AS/NZS 4282-2019, ‘Control of the obtrusive effects of outdoor lighting’, to avoid annoyance to the occupants of adjoining premises or glare to motorists on nearby roads. Flashing, moving or intermittent lights or signs are prohibited. The intensity, colour or hours of illumination of the lights must be varied at Council’s discretion if Council considers there to be adverse effects on the amenity of the area.


	183. 
	Condition reason: To protect the amenity of the surrounding area.

	184. 
	Waste Storage and Disposal – Multistorey Premises

	185. 
	The waste storage room must be provided with smooth and impervious walls and floors and coved at the intersection of the floor and walls. Floor areas must be graded and drained to a floor waste gully connected to the sewer. Waste storage rooms must be well ventilated and proofed against pests. The area or room must be provided with water service hose connectors to enable easy cleaning. Open waste storage areas must be appropriately covered and bunded. The ground must be paved with impervious material and must be graded and drained to a wastewater disposal system according to Sydney Water’s requirements. A hose tap connected to a water supply must be provided. 

All waste generated on the site is to be stored, handled and disposed of in such a manner as to not create offensive odour, offensive noise or pollution of land and/or water as defined under the Protection of the Environment Operations Act 1997. All waste generated must be removed and disposed of by an authorised waste removal contractor. A copy of the waste removal agreement and receipts must be made available to Council on request.



	186. 
	Condition reason:  To ensure compliance with the relevant Australian Standard and National Construction Code.

	187. 
	Use of roof

	
	No approval is granted or implied for the use of any roof element for any purpose other than for gaining access to carry out maintenance or repairs.

7.114

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	188. 
	Car parking not for storage

	
	The approved car parking spaces, driveways and manoeuvring areas are to be used for employees and visitors’ vehicles only and not for the storage of new or used materials, finished goods or commercial vehicles.

7.301

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation and to provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.

	189. 
	Waste generated on site

	
	All waste generated on the site is to be stored, handled and disposed of in such a manner as to not create offensive odour, offensive noise or pollution of land and/or water as defined under the Protection of the Environment Operations Act 1997. All waste generated shall be removed and disposed of by an authorised waste removal contractor. A copy of the waste removal agreement and receipts shall be made available to Council on request.  

7.504

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	190. 
	Stormwater Detention

	
	The on-site stormwater detention storage system within the site as constructed shall not be altered and shall be maintained in good working order to the satisfaction of Council.
7.302

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	191. 
	Maintenance of wastewater and stormwater treatment device

	
	During occupation and ongoing use of the building, all wastewater and stormwater treatment devices (including drainage systems, sumps and traps, and on-site detention) must be regularly maintained to remain effective and in accordance with any positive covenant (if applicable).

7.303.S

	
	Condition reason:  To protect existing public and private infrastructure and building works during demolition, construction and ongoing use of the development.

	192. 
	Traffic signal maintenance

	
	Any system using traffic light signals must maintain a green signal to entering vehicles at the point of entry and must maintain a red signal when an exiting vehicle is detected upon the ramp or driveway.  This is to ensure that vehicles entering the site do not have to wait at the top of the ramp, and vehicles wishing to exit the site must wait for entering vehicle in the basement at the waiting bay.

7.401

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.  

	193. 
	Enter / Exit in forward direction

	
	All vehicles associated with the development are to enter and exit the site in a forward direction.

7.402

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.  

	194. 
	Waste Management Plan

	
	The requirements of the submitted Waste Management Plan shall be complied with at all times that the approved development is being carried out.

7.501

	
	Condition reason: To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites. 

	195. 
	Bin room signage

	
	Adequate signage is to be provided and maintained on how to use the waste management system and what materials are acceptable for recycling within all waste storage areas of the development. Signage is also to be provided and maintained which clearly identifies which bins (and containers) are to be used for general waste and recycling and what materials can be placed in each bin.

7.505

	
	Condition reason:  To provide and maintain orderly and safe areas for vehicular and pedestrian movement / parking.  

	196. 
	Waste and recycling policy

	
	The development must be carried out in compliance with Council’s “Domestic Waste and Recycling Service Policy and Guideline”.

7.506

	
	Condition reason:  To ensure compliance with the relevant Canterbury Bankstown policy.

	197. 
	Waste containers

	
	No waste storage containers are to be located or placed outside the approved waste storage area at any time except for collection purposes.

7.507

	
	Condition reason:  To protect and enhance the amenity of the occupants of the development site and the occupants of adjoining sites.

	198. 
	Maintenance of landscaping

	
	The approved landscaping and external work must be maintained post occupation and must not be altered or changed without Council approval or unless the altered work is carried out in accordance with the relevant provisions of the State Environmental Planning Policy (Exempt and Complying Development Codes) 2008.

7.701

	
	Condition reason:  To ensure the development is built and remains consistent with approved plans and documentation.

	
	


General advisory notes

This consent contains the conditions imposed by the consent authority which are to be complied with when carrying out the approved development. However, this consent is not an exhaustive list of all obligations which may relate to the carrying out of the development under the EP&A Act, EP&A Regulation and other legislation. Some of these additional obligations are set out in the Conditions of development consent: advisory notes. The consent should be read together with the Conditions of development consent: advisory notes to ensure the development is carried out lawfully.

The approved development must be carried out in accordance with the conditions of this consent. It is an offence under the EP&A Act to carry out development that is not in accordance with this consent.

Building work or subdivision work must not be carried out until a construction certificate or subdivision works certificate, respectively, has been issued and a principal certifier has been appointed. 

A document referred to in this consent is taken to be a reference to the version of that document which applies at the date the consent is issued, unless otherwise stated in the conditions of this consent. 

Dictionary
The following terms have the following meanings for the purpose of this determination (except where the context clearly indicates otherwise): 
Approved plans and documents means the plans and documents endorsed by the consent authority, a copy of which is included in this notice of determination. 

AS means Australian Standard published by Standards Australia International Limited and means the current standard which applies at the time the consent is issued. 

Building work means any physical activity involved in the erection of a building. 

Certifier means a council or a person that is registered to carry out certification work under the Building and Development Certifiers Act 2018.

Construction certificate means a certificate to the effect that building work completed in accordance with specified plans and specifications or standards will comply with the requirements of the EP&A Regulation and Environmental Planning and Assessment (Development Certification and Fire Safety) Regulation 2021. 

Council means Canterbury Bankstown Council. 

Court means the Land and Environment Court of NSW.

EPA means the NSW Environment Protection Authority.

EP&A Act means the Environmental Planning and Assessment Act 1979. 
EP&A Regulation means the Environmental Planning and Assessment Regulation 2021. 
Independent Planning Commission means Independent Planning Commission of New South Wales constituted by section 2.7 of the EP&A Act.

Local planning panel means Canterbury Bankstown Local Planning Panel.

Occupation certificate means a certificate that authorises the occupation and use of a new building or a change of building use for an existing building in accordance with this consent.

Principal certifier means the certifier appointed as the principal certifier for building work or subdivision work under section 6.6(1) or 6.12(1) of the EP&A Act respectively. 

Site work means any work that is physically carried out on the land to which the development the subject of this development consent is to be carried out, including but not limited to building work, subdivision work, demolition work, clearing of vegetation or remediation work.

Stormwater drainage system means all works and facilities relating to: 

the collection of stormwater, 

the reuse of stormwater, 

the detention of stormwater, 

the controlled release of stormwater, and 

connections to easements and public stormwater systems. 

Strata certificate means a certificate in the approved form issued under Part 4 of the Strata Schemes Development Act 2015 that authorises the registration of a strata plan, strata plan of subdivision or notice of conversion.

Subdivision certificate means a certificate that authorises the registration of a plan of subdivision under Part 23 of the Conveyancing Act 1919. 
Subdivision works certificate means a certificate to the effect that subdivision work completed in accordance with specified plans and specifications will comply with the requirements of the EP&A Regulation.

Sydney District or Regional Planning Panel means Sydney South Planning Panel.

If you need help interpreting this document, please contact Council on 9707 9000.
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Requesting operational consent for a deferred
commencement Development Application

When a development application with a deferred commencement condition is approved through the NSW
Planning Portal, the applicant is required to submit a request for operational consent to the consent authority
within the specified period before the development consent can become operational.

This guide provides instructions on how to request for operational consent via the NSW Planning Portal.

Requesting operational consent

1. Loginto the NSW Planning Portal. Locate and open the relevant application in your Completed Work. Note: the
application will have a status of “Deferred commencement”.

Active work Completed work

Application Type

All Y
Reference number Submitted Date LGA Name Site address Status
] 20 SANCTUARY PLACE CATALINA Deferred
PAN-18593 15/12/22 EUROBODALLA 2536 commencement

2. Select Request for operational consent from the

Actions dropdown menu. pted application ~ ‘

Refresh

Request for operational consent

Reference number: PAN-18593 Council Id: DA22/034 Actions ~ Close and hol

DA Online

+/ Assessment +/ Determination Operational Consent

~/ Pre-lodgement Review +/ Lodgement

Request for operational consent @ rarekely

3. Enter the due date for evidence about relevant
Due date for evidence about relevant matters: = @

)

matters, as provided by the consent authority.

Note: This must be a future date.

© State of New South Wales through Department of Planning and Environment 2023. Information contained in this publication is based on knowledge and
understanding at the time of writing, February 2023, and is subject to change. For more information, please visit dpie.nsw.gov.au/copyright SF23/15060
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4. Enter details of how the conditions have been

. Enter details of how the conditions have been satisfied and/or upload documentation to
satisfied.

support your request (max 2000 characters) *

Remaining: 2000 characters

5. Click Upload.

a. Click Select files (s) or drag and drop your
file(s) in the space provided. %

Drag and drop files here

b. Categorise the file type(s)

or

c. Click Attach. |- |

Category

I Architectural Plans hs

Select, v

|
I Select. ~ ]
l

Select. N ]

Note: The name of the document has a maximum of 150 characters. If the name of your file exceeds this limit, you can
change the document name to bring it within the 150-character limit.

6. Click Submit. m

You can view your request for operational consent on the Relevant matters tab within the application.

Application details Relevant matters Documents Payer details Action summary Analytics Related cases

J Request operational consent

What Happens Next?

The consent authority will be notified of the request. Once the consent authority has reviewed your request and provided an
outcome, you will receive a notification. You can view their comments on the Relevant matters tab of the application. Any
associated documents can be accessed on the Documents tab.

If the request was declined, you can submit another request for operational consent by following the above steps.

End of steps
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If you need more information
e Click the Help link at the top of the screen to access the NSW Planning Portal help pages and articles.

e Review the Frequently Asked Questions - https://www.planningportal.nsw.gov.au/support/frequently-asked-

questions and / or contact ServiceNSW on 1300 305 695.
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