Attachment 1 – Draft Conditions of Consent  DA2025/28  for the construction of Motel and Function Centre at Lot 1 DP 1306742, 50 Lachlan Street NSW CONDOBOLIN 2877

ADMINISTRATIVE CONDITIONS 
1. APPROVED PLANS AND SUPPORTING DOCUMENTS
The development shall be carried out in accordance with the approved stamped and signed plans except where modified by any following condition or as amended in red ink.
A current copy of the Development Consent and Construction Certificate (including all plans, specifications and certificates) shall be maintained on the development site at all times until issue of an occupation certificate.
Note 1: Modifications to the approved plans will require the lodgement and consideration by Council of a modification pursuant to Section 4.55 of the Environmental Planning and Assessment Act 1979.
Note 2: The approved plans and supporting documentation may be subject to conditions imposed under section 4.17 of the Environmental Planning and Assessment Act 1979 modifying or amending the development (refer to conditions of consent which must be satisfied prior to the issue of any Construction Certificate).
	Reference /Dwg No.
	Title/Description
	Prepared By
	Date

	DA-101 Rev C
	Site Plan – Ground Floor
	Twohill & James
	8/12/25

	DA-102 Rev B
	Site Plan – Upper Floor
	Twohill & James
	30/7/25

	DA-103 Rev B
	Site Plan – Roof Plan
	Twohill & James
	30/7/25

	DA-104 Rev A
	Building A & B Ground Floor Plan
	Twohill & James
	30/6/25

	DA-105 Rev A
	Building A & B Upper Floor Plan
	Twohill & James
	1/7/25

	DA-106 Rev A
	Building A & B Roof Plan
	Twohill & James
	1/7/25

	DA-107 Rev B
	Building C Ground Floor Plan
	Twohill & James
	30/7/25

	DA-108 Rev A
	Building C Upper Floor Plan
	Twohill & James
	30/7/25

	DA-109 Rev A
	Building C Roof Plan
	Twohill & James
	30/7/25

	DA-201 Rev B
	Site Elevations
	Twohill & James
	30/7/25

	DA-202 Rev A
	Building B & C Elevations
	Twohill & James
	30/7/25

	DA-203 Rev B
	Building B & C Elevations
	Twohill & James
	30/7/25

	DA-204 Rev B
	Building A Elevations
	Twohill & James
	30/7/25

	DA-301 Rev A
	Building B & C Sections
	Twohill & James
	30/7/25

	DA-302 Rev A
	Building B & C Sections
	Twohill & James
	30/7/25

	DA-303  Rev A
	Building B & C Sections
	Twohill & James
	30/7/25

	DA-304 Rev B
	Building A Sections
	Twohill & James
	30/7/25

	DA-401
	Signage Details
	Twohill & James
	8/12/25

	DA-601
	Materiality
	Twohill & James
	Undated

	DA-602
	Materiality
	Twohill & James
	Undated

	18/25
	Landscape Plan
	Sally Bourne Landscapes
	24/6/25

	
	Landscape Document (13 pages)
	Sally Bourne Landscapes
	24/6/25

	G01 Rev B
	Stormwater Management Plan - Cover Sheet
	Calare Civil
	27/6/25

	C01 Rev B
	Stormwater Management Plan – General Arrangement Plan
	Calare Civil
	27/6/25

	C02 Rev B
	Stormwater Management Plan – Preliminary Site Grading Plan
	Calare Civil
	27/6/25

	C03 Rev B
	Stormwater Management Plan - Preliminary Site Grading Plan
	Calare Civil
	27/6/25

	C04 Rev B
	Stormwater Management Plan – Overland Flow Path Plan
	Calare Civil
	27/6/25

	
	Statement of Environmental Effects
	Currajong
	25/3/26

	
	Noise Management Plan
	Currajong
	25/3/26

	
	Crime Prevention Through Environmental Design Report
	Currajong
	9/12/25

	
	Detailed Site Investigation
	Enviroseer
	15/5/26

	
	Section J Report – Buildings A, B and C 
	Speckel
	3/6/25



1. Signage 
The approval includes two (2) freestanding advertising signs only. A separate development application for the erection of a sign or advertising structure, other than an advertisement listed as exempt development, is to be submitted to Lachlan Shire Council. 
The structures over the barbecue areas are an architectural feature and are not to be utilised as advertising signs.
1. Electricity Infrastructure
Any existing encumbrances in favour of Essential Energy (or its predecessors) noted on the title of the above property are to be complied with.




PRIOR TO ISSUE OF CONSTRUCTION CERTIFICATE
1. [bookmark: _Hlk211955765]Section 7.12 Contributions
Pursuant to section 4.17 of the Environmental Planning and Assessment Act 1979, and the Lachlan Shire Council Lachlan Section 7.12 Contributions Plan 2015, the monetary contribution set out in the following table is to be paid to Council, prior to the issue of any Construction Certificate.
The contribution is current as at the date of this consent and the amount to be paid is to be adjusted at the time of the actual payment, in accordance with the Lachlan Shire Council Section 7.12 Development Contributions Plan. 
It is the professional responsibility of the Principal Certifying Authority to ensure that the monetary contribution has been paid to Council in accordance with the above timeframes.
	Contribution Type
	Proposed Cost of Development¹
	Levy Percentage
	Total Contribution

	Section 7.12 Contribution
	$6,993,772.50
	1%
	$69,937.73




The Contributions plan is available on council’s website:  https://www.lachlan.nsw.gov.au/Development/Landuse-Planning/Local-Infrastructure-Contributions-and-Planning-Agreements
1. [bookmark: _Toc22225353]Headworks Contributions - Sewer
Pursuant to the provisions of Section 64 of the Local Government Act 1993 a contribution as specified in the following table is to be paid to Council as the Sewer Management Authority. Documentary evidence shall be provided to the Certifying Authority that that the contribution set below has been paid in full prior to the issue of any Construction Certificate.
Section 64 Sewerage (1 Equivalent Tenement (ET) = $4,047 based on Lachlan Shire Council Fees and Charges 2025/26)
	Equivalent Tenement (ET) detail
	ETs sewer
	Cost

	Existing vacant lot and former use as Bowling Green
	-1.0
	-$4,047 (credit)

	Motel and function centre– 28 guest rooms 
	+0.45 per room
	+$50,992.20

	Motel development –1 manager’s residence
	+1.0
	+$4,047

	TOTAL ETs and cost payable
	12.6
	$50,992.20



Note:	Council’s fees and charges (including Sewer Headwork’s Contribution Plans charges) are reviewed each June in accordance with CPI fluctuations and the fees quoted may be varied in accordance with that review. As this consent is valid for five (5) years from the date of this approval the charges required to be paid will be those applicable in the financial year that the work commences.
1. Headworks Contributions - Water
Pursuant to the provisions of Section 64 of the Local Government Act 1993 a contribution as specified in the following table is to be paid to Council as the Water Management Authority. Documentary evidence shall be provided to the Certifying Authority that that the contribution set out below has been paid in full prior to the issue of any Construction Certificate.
Section 64 Water (1 Equivalent Tenement (ET) = $14,097 based on Lachlan Shire Council Fees and Charges 2025/26)
	Dwelling detail
	ETs water
	Cost

	Existing vacant lot and former use as Bowling Green
	-1.0
	-$14,097.00 (credit)

	Motel and function centre– 28 guest rooms 
	0.3
	+$118,414.80

	Motel development –1 manager’s residence
	1.0
	+$14,097.00

	TOTAL ETs and cost payable
	8.4
	$118,414.80


 
Note:	Council’s fees and charges (including Water Headwork’s Contribution Plans charges) are reviewed each June in accordance with CPI fluctuations and the fees quoted may be varied in accordance with that review. As this consent is valid for five (5) years from the date of this approval the charges required to be paid will be those applicable in the financial year that the work commences.
1. [bookmark: _Hlk211955627]Long Service Levy
Prior to the issue of any Construction Certificate evidence is to be provided demonstrating payment of the prescribed Long Service Levy fee.
1. Section 68 Approvals
[bookmark: _Hlk211955616]Prior to the issue of a Construction Certificate, the applicant shall obtain approval from Council pursuant to Section 68 of the Local Government Act 1993 for any water supply, sewerage, and/or stormwater drainage works.
1. Stormwater Management
Prior to the commencement of any plumbing and drainage work, the internal stormwater drainage system shall be designed in accordance with the following standards:
(a) Lachlan Shire Council Engineering Standards 
(b) Cater for a 20%AEP (1-in-5 year ARI) 'minor' storm event and a 1% AEP (1in100year ARI) 'major' storm event. 
A plan complying with the above shall be detailed in the Construction Certificate application. Any on-site detention of stormwater shall include full engineering details of the detention structure to be submitted to and approved by Council (as the stormwater authority) prior to the issue of any Construction Certificate.
1. Water and Sewer Connections
Prior to the issue of a Construction Certificate, the applicant is to lodge a “Water and Sewer Connection Form” to Lachlan Shire Council and receive approval in writing.  
The development shall have a separate and distinct water and sewer connection directly with the public infrastructure, in accordance with the Local Government (General) Regulation 2023.
1. Development Adjacent to Sewer Main
Prior to the commencement of any plumbing and drainage work, Council’s sewer main alignment and depth shall be accurately located and the greater of the following clearance criteria must be achieved:
(a)	A line taken at an angle of 45 degrees downwards from the lower edge of the proposed footing will not intersect Council’s sewer main and its trench.
(b)	A minimum 1100mm between the building’s footings and centre line of the sewer main.
(c)	The building and its footings are located outside any existing sewer easement.
If the above criteria cannot be achieved, a design plan shall be submitted to Council from a suitably qualified engineer in accordance with Council’s “Build in Vicinity of Sewer Mains Policy”.  The design plan shall be detailed in the Construction Certificate application.
1. Utility Arrangements
Arrangements are to be made with utility authorities in respect to the services supplied by those authorities to the development. The cost associated with the provision or adjustment of services within the road and footway areas is to be at the developer’s expense. Such work includes (but is not limited to) upgrade or connection to sewer or stormwater mains, and alteration of stormwater pits and sewer manhole levels.
1. Driveways & Vehicular Crossings
Prior to the issue of a Construction Certificate, full engineering details of the vehicular access driveway shall be submitted to and approved by Council (as the roads authority).
1. Road Works Approval
Prior to the issue of a Construction Certificate, the applicant shall obtain approval from Council pursuant to Section 138 of the Roads Act 1993 for any work within the public road reserve. The application is to be submitted along with:
(a) Full engineering details of the proposed works that complies with Lachlan Shire Council Engineering Specifications
(b) a Traffic Control Plan prepared in accordance with the Roads and Traffic Authority Manual – version 4.
(c) A sediment control plan; 
(d) environmental management plans; and
(e) work method statements.
Note:	Concurrence from Transport for NSW is required before the Approval can be issued for any classified road.
1. Waste Management Plan
A Waste Management Plan (WMP) is to be prepared by a consultant suitably qualified and experienced in the preparation of WMPs, to ensure waste from the construction and operation phases of the development is appropriately managed so as to not cause pollution and to ensure waste is managed in accordance with the hierarchy of avoid, recovery and disposal. 
The Plan shall include techniques to temporarily store waste on site in suitable containers, arrangements for the removal of waste material from the site, destination of waste materials being removed from the site.  The WMP is to be submitted to and approved by Council prior to the issue of any Construction Certificate.
1. Food Preparation Areas
To ensure that adequate provision is made for the cleanliness and maintenance of all food preparation areas, all building work in connection with the occupation or use of the premises for the preparation and storage of food shall be designed and carried out in accordance with the requirements of:-
(a)	AS4674 (Design, Construction and Fit-Out of Food Premises);
Detailed plans and specification of work showing that these design requirements have been met shall be submitted to, and approved by, the Certifying Authority prior to the issue of a Construction Certificate.
1. Flooding
Prior to the issue of a Construction Certificate for any building work below the 1% AEP (1in100 year ARI) flood height is to be certified by a Structural Engineer stating that it is able to withstand flood velocities for that area. All materials below the 1:100 year flood event are to comply with the NSW Flood Manual.
1. Swimming Pools on Flood Prone Land
The swimming pool is to be installed on land that is prone to flooding. Certification is to be supplied by the design engineer demonstrating that the pool has been designed to withstand the flooding impacts (i.e. velocity and depth). The certification shall be submitted to the Principal Certifying Authority and incorporated into the design of the pool prior to the issue of a Construction Certificate.
1. Swimming Pool - Fencing
Prior to the issue of  Construction Certificate, the details of the fencing for the swimming pool shall be submitted and show compliance with the Swimming Pool Act 1992 and the AS1926.2.
1. Swimming Pool – Waste water and recirculation
All wastewater from the pool filtration system is to be discharged to Council’s sewer and the recirculation system shall comply with AS1926.3.
1. Engineer Designed Pavement 
	All vehicle parking areas, manoeuvring areas and the access aisle must be paved, drained and line marked.  The pavement must be designed by a qualified civil engineer and certified to be satisfactory for the expected traffic loadings for a development of this size and type.  AUSTROADS Guide to Pavement Technology can be used as the design guideline for the pavement design. 
1. Structural Engineering Plans
The following structural details must be provided to the Certifying Authority prior to commencing work:
1. structural engineer's design for all reinforced concrete footings and slabs,
1. structural engineers design for all structural steel beams, framing and connections,
1. roof truss and bracing details, and
1. manufacturer's specifications for any patented construction systems.
1. Retaining walls 
Where the retaining wall associated with the landscaped area is higher than 600mm, full details must be submitted prior to the issue of any construction certificate.
1. Erosion and Sediment Control Plan
An Erosion and Sediment Control Plan (ESCP) must be prepared to ensure erosion and sediment is controlled during high rainfall or dust events to prevent impact to downstream waterways. This must meet the standards outlined in the publication Soils and Construction: Managing Urban Stormwater Fourth Edition Vol. 1 (or subsequent amendments) prepared by Landcom.
1. Utility Arrangements
Arrangements are to be made with utility authorities in respect to the services supplied by those authorities to the development.  The cost associated with the provision or adjustment of services within the road and footway areas is to be at the developer’s expense. Such work includes (but is not limited to) upgrade or connection to sewer or stormwater mains, and alteration of stormwater pits and sewer manhole levels.
1. Construction Environmental Management Plan
Prior to the issue of the Construction Certificate, a Construction Environmental Management Plan (CEMP) is to be prepared by a suitably experienced / qualified person and submitted to Council for approval. If Council is not the certifying authority, a copy of Council’s approval is to be provided to the Principal Certifier. The CEMP is to address the environmental aspects of the construction phase of the development and is to include details on the environmental management practices and controls to be implemented on the site.
All construction activities on the site are to be implemented and carried out in accordance with the approved CEMP.
1. Compliance with the Noise Impact Assessment
Prior to the issue of the Construction certificate, plans showing compliance with the recommendations of the Noise Impact Assessment, including showing the location of the compressor, shall be submitted to Council for approval.



PRIOR TO COMMENCEMENT OF WORKS
1. Construction Certificate
Prior to the commencement of any building work, a Construction Certificate is to be obtained from either Council or an Accredited Certifier, certifying that the proposed works are in accordance with this Consent and the applicable standards.
1. Construction Certificate Requirements
Prior to commencement of work, the person having the benefit of the Development Consent:
(a) Shall appoint a Principal Certifying Authority (PCA).
(b) Shall ensure a Construction Certificate is issued by the PCA.
(c) Shall notify Council of their intention to commence the site works, at least two days prior to commencement of work.
Where Lachlan Shire Council is nominated as the Principal Certifying Authority, the following requirements shall be satisfied before the commencement of work:
(a) The LSC Principal Certifying Authority Service Agreement shall be completed and signed by the applicant.
(b) The LSC Notice of Commencement of Building Works and Appointment of Principal Certifying Authority shall be completed and issued to Council at least two days before undertaking any work in accordance with the Construction Certificate.
(c) Terms and conditions of the LSC Principal Certifying Authority Service agreement shall be satisfied.
Where Lachlan Shire Council is not the Principal Certifying Authority, the following requirements shall be satisfied before the commencement of work:
(a) Principal Certifying Authority name address and registration details from the Building Professionals Board shall be registered with Council.
(b) Construction Certificate shall be registered with Council.
1. Fencing
Prior to the commencement of any work, security fencing shall be installed around the perimeter of the site to a minimum height of 1.8 metres and in compliance with AS4687 Temporary Fencing and Hoardings and any other applicable WorkCover Guidelines. The fencing must be maintained throughout the construction phase.
1. Signage
Prior to the commencement of any work on the site, a sign shall be erected in a visually prominent position containing the following information:
(a)	the development application number.
(b)	name, address and telephone number of the principal certifying authority.
(c)	name of the principal contractor (if any) and 24-hour contact telephone number.
(d)	a statement that "unauthorised entry to the work site is prohibited”.
1. Insurances and Security
[bookmark: _Hlk211956011]Prior to the commencement of any work on the site, a Public Risk Insurance Policy with a minimum cover of $20,000,000 in relation to the work must be obtained, with a copy being provided to Council.

1. Sediment & Erosion Controls
Erosion and sediment control devices must be maintained throughout the entire construction phase of the development until the site is stabilised such that sediment will not be washed into the stormwater system during heavy rainfall.
1. Site Requirements
Prior to the commencement of construction works: 
1. Toilet facilities at or in the vicinity of the work site shall be provided at the rate of one toilet for every 20 persons or part of 20 persons employed at the site. Each toilet provided must be: 
· a standard flushing toilet connected to a public sewer, or 
· if that is not practicable, an accredited sewage management facility approved by the council, or 
· alternatively, any other sewage management facility approved by council.
1. All excavations and backfilling associated with the erection or demolition of a building must be executed safely and in accordance with the appropriate professional standards. All excavations associated with the erection or demolition of a building must be properly guarded and protected to prevent them from being dangerous to life or property.
1. If an excavation associated with the erection or demolition of a building extends below the level of the base of the footings of a building on an adjoining allotment of land, the person causing the excavation to be made:
· must preserve and protect the building from damage, and 
· if necessary, must underpin and support the building in an approved manner, and 
· must at least 7 days before excavating below the level of the base of the footings of a building on an adjoining allotment of land, give notice of intention to do so to the owner of the adjoining allotment of land and furnish particulars of the excavation to the owner of the building being erected or demolished. The owner of the adjoining allotment of land is not liable for any part of the cost of work carried out for the purposes of this condition, whether carried out on the allotment of land being excavated or on the adjoining allotment of land, (includes a public road and any other public place).
1. If the work involved in the erection or demolition of a building is likely to cause pedestrian or vehicular traffic in a public place to be obstructed or rendered inconvenient, or involves the enclosure of a public place, a hoarding or fence must be erected between the work site and the public place:
· if necessary, an awning is to be erected, sufficient to prevent any substance from, or in connection with, the work falling into the public place, 
· the work site must be kept lit between sunset and sunrise if it is likely to be hazardous to persons in the public place, and 
· any such hoarding, fence or awning is to be removed when the work has been completed.
1. Dilapidation Report 
Prior to the commencement of any work, a dilapidation report must be prepared by a suitably qualified engineer detailing the structural condition of the surrounding buildings and Council owned infrastructure that is proposed for use during the construction stage, shall be prepared and submitted to Council for approval.
1. Construction Traffic Management Plan
Prior to the commencement of any works on-site (including demolition works), a Construction Traffic Management Plan (CTMP) shall be submitted to Lachlan Shire Council for endorsement. The CTMP shall be prepared by a suitably qualified consultant with appropriate training and certification from Transport for NSW. The CTMP shall include details of any required road closures, work zones, loading zones and the like. Approval of the CTMP may require approval of the Local Traffic Committee. Please contact Council if Temporary Road Reserve Occupancy is required.
1. Traffic Guidance Scheme
Prior to commencement of any works associated with the development, a Traffic Guidance Scheme, including details for pedestrian management, shall be prepared in accordance with AS1742.3 Traffic Control Devices for Works on Roads and the Transport for NSW (TfNSW) publication Traffic Control at Worksites Technical Manual, and certified by an appropriately accredited TfNSW traffic controller.    
Traffic control measures shall be implemented during the construction phase of the development in accordance with the certified plan. A copy of the plan shall be available on site at all times.   
Note:      
· A copy of the Traffic Guidance Scheme shall accompany the Notice of Commencement to Lachlan Shire Council.  
· Traffic control measures may require road occupancy / road closure approvals issued under Section 138 of the Roads Act by Lachlan Shire Council prior to the issue of any Construction Certificate or Subdivision Works Certificate. 
CONDITIONS TO BE SATIFIED DURING WORKS
1. Building Set Out
The building(s) associated with the development must be set-out by a Registered Surveyor in accordance with the approved plans. A plan that identifies the location of the building(s) in relation to the allotment boundaries must be prepared upon completion of the ground floor and submitted to the Principal Certifying Authority.
1. Hours of Works
Construction works at the development site shall only be carried on between:
(a) Monday to Saturday 		7am to 5pm
(b) Sundays			Nil
(c) Public Holidays			Nil
1. Unexpected Finds
Should any material suspected of being an Aboriginal relic or artefact become unearthed in the course of works:
(a) all works impacting the objects or artefacts shall cease immediately; and 
(b) immediate contact is to be made with the Office of the Environment and Heritage to arrange for representatives to inspect the site. 
All workers on the site are to be made aware of this condition.
A stop work protocol must be implemented for any potential heritage items found during excavation including ceasing work immediately if any Aboriginal objects are found/uncovered, secure the site and inform Office of Environment and Heritage and Lachlan Shire Council immediately.
If human remains are found work is to stop, the site is to be secured and the NSW Police and the NSW Office of Environment and Heritage are to be contacted.
1. Erosion & Sediment Control Plan Compliance
The development is to be carried out in accordance with the approved Erosion & Sediment Control Plan at all times. All measures required by the ESCP are to be installed and maintained in accordance with the plan and maintained in good working order for duration of works.
1. Erosion & Sediment Control Installation and Maintenance
Prior to the commencement of any works, sediment and erosion controls shall be installed to prevent soil erosion, water pollution or the discharge of loose sediment on surrounding land, as follows:
(a) Divert uncontaminated run-off around cleared or disturbed areas.
(b) Erect a silt fence to prevent debris escaping into drainage systems or waterways.
(c) Prevent tracking of sediment by vehicles on roads.
(d) Stockpile topsoil, excavated material, construction and landscaping supplies and debris within the site.
(e) Silt and gross pollutant traps shall be fitted in all stormwater pits
These measures are to be maintained in good working order for the duration for the works.
The erosion and sedimentation controls are to be maintained for as long as necessary after completion of works to prevent soil erosion, water pollution or the discharge of loose sediment on surrounding land. The controls are to remain in place until all disturbed ground surfaces are rehabilitated / revegetated and stabilised to prevent erosion or sediment loss.
Where straw bale sediment fences are proposed, they shall generally comply with the following:
(a) Only weed free straw or natural thatch / litter is to be used.
(b) They are only used for low flows of water.
(c) Every 20 metres, there is one straw bale that is placed at a 90 degree angle to the others for stability.
(d) Straw bales tightly abut each other.
(e) Straw bales are held firmly in place with star pickets or the like.
1. Earthworks/Fill
Any fill material is to be placed in accordance with the standards specified in AS 3798 Guidelines on earthworks for commercial and residential developments.
All fill brought to the site must be clean and may comprised Excavated Natural Material (ENM) or Virgin Excavated Natural Material (VENM). Evidence is to be provided that the fill material is not contaminated.
1. Site Toilet Facilities
Adequate toilet facilities for workers must be provided at or in the vicinity of the work site.

1. Site Management
(a) All storage of goods and building materials and the carrying out of building operations related to the development proposal shall be carried out within the confines of the property. All vehicles must be parked legally and no vehicles are permitted to be parked over the public footpath. The unloading of building materials over any part of a public road by means of a lift, hoist or tackle projecting over the footway will require separate approval under Section 68 of the Local Government Act 1993. 
(b) There is to be no storage of materials, stockpiling of excavated material or parking of plant/machinery within the drip line of the crown of any retained trees.
(c) Public footways and roadways adjacent to the site must be cleared of obstructions during construction unless separate approval from Council is obtained to occupy the public road reserve.
(d) All waste materials generated on-site during demolition/construction are to be stored in enclosed containers and deposited in an approved landfill at regular periods.
(e) Any waste materials stored on site must be stored out of view or in such a manner so as not to cause unsightliness when viewed from nearby lands or roadways. 
(f) The site shall be maintained in a clean and orderly condition during construction works.
1. Inspections
The applicant is to obtain a Compliance Certificate from Council or an accredited certifying authority, certifying compliance with the Building Code of Australia, and any other relevant conditions of consent for the stages of construction listed in column 1. For the purpose of obtaining the compliance certificate the work must be inspected by an accredited certifying authority at the time specified in column 2. 
	
	Column 1
	Column 2

	A
	Footings
	When the footings have been excavated and all steel reinforcement has been placed in position. 

	
	Excavation
	When the excavation of the hole for the swimming pool has been completed and bedding material has been levelled out.

	
	Bond beam
	When reinforcement steel has been placed in position for the swimming pool.

	B
	Slab

	When reinforcement steel has been placed in position in any concrete slab, irrespective of whether the slab is suspended, on the ground, or on fill.

	C
	Wall Frame
	When the wall frame has been constructed, prior to cladding and hot and cold plumbing completed. 

	D
	Roof Frame
	When the roof frame has been constructed, prior to sheeting. 

	E
	Wet Areas
	When flashing to all wet areas, including the bathroom, wash room, water closet, shower recess have been completed. 

	F
	Internal drainage
	When all internal plumbing work is completed and prior to concealment.

	
	Pool fencing
	When fencing is complete (NB:  fencing is to be in situ prior to filling of the swimming pool)

	G
	External drainage
	When all external plumbing work is installed and prior to concealment.

	H
	Final
	Prior to occupation of the buildings and use of swimming pool.



1. Plumbing and Drainage
All plumbing and drainage work shall be carried out by a licensed plumber and drainer and to the requirements of AS/NZS 3500 and the National Plumbing Code of Australia (Volume 3 of the NCC).
Note1: Notice of Work is to be issued to the Council no later than 2 business days before the work concerned is carried out.
Note 2: A Certificate of Compliance for the plumbing and drainage work identified in Colum 1 at the times specified in Colum 2 must be obtained from Council: 
	
	Column 1
	Column 2

	A
	Internal Sewer Drainage
	When all internal plumbing and drainage work is installed and prior to concealment.

	B
	External Sewer Drainage
	When all internal plumbing and drainage work is installed and prior to concealment.

	C
	Stormwater Drainage
	When all external stormwater drainage work is installed and prior to concealment. 

	
	Waste Water Drainage
	When all external waste water drainage work is installed and prior to concealment.

	D
	Final
	Prior to occupation of the building or structure or use of swimming pool. 



Note 3: Sewer Diagram is to be issued to the Council and the owner of the land or the owner’s agent, on completion of the final inspection.
1. Swimming Pools - Pool Not to be Filled with Water
The swimming pool must not to be completely filled with water until such time as a child-resistant barrier that separates the swimming pool from any residential building situated on the premises and from any place (whether public or private) adjoining the premises, and is designed, constructed, installed and maintained in accordance with the standards set out in the Building Code of Australia. Where the depth of water in the pool exceeds 300mm during construction a temporary child-resistant barrier shall be erected.
1. Swimming Pools - Prevention of Spillage
The area surrounding the pool is to be constructed in such a manner as to prevent spillage flowing onto adjacent properties.
1. Rectifying damage to public infrastructure
Any damage caused to footpaths, roadways, utility installations, street trees and the like by reason of construction operations shall be made good and repaired to a standard equivalent to that existing prior to commencement of construction. The full cost of restoration / repairs of property or services damaged during the works shall be met by the Applicant.
1. Contamination – Unexpected Finds Protocol
Should any contamination or suspect material be encountered during site preparation, earth works, construction or any other stage of the development, works must cease immediately, and a suitably qualified consultant engaged to conduct a thorough contamination assessment and provide recommended management actions to guide the management of any contamination onsite. Council must be notified if this protocol is required to be enacted.
1. Dust Mitigation
[bookmark: _Toc323042326]Construction activities occurring at the premises must be carried out in a manner that will minimise emissions of dust from the premises. 
1. Mud Mitigation
Mud and soil from vehicular movements to and from the site must not be deposited on the road.
1. Works in proximity to electrical infrastructure
(a) Any activities in proximity to electrical infrastructure must be undertaken in accordance with the latest industry guideline currently known as ISSC 20 Guideline for the Management of Activities within Electricity Easements and Close to Infrastructure; 
(b) Prior to carrying out any works, a “Dial Before You Dig” enquiry should be undertaken in accordance with the requirements of Part 5E (Protection of Underground Electricity Power Lines) of the Electricity Supply Act 1995 (NSW); and 
(c) It is the responsibility of the person/s completing any works around powerlines to understand their safety responsibilities. SafeWork NSW (www.safework.nsw.gov.au) has publications that provide guidance when working close to electricity infrastructure. These include the Code of Practice – Work near Overhead Power Lines and Code of Practice – Work near Underground Assets. 
Note: If your site’s energy demand exceeds Essential Energy’s standard limits, electricity supply upgrades may be required, including the possible installation of a padmount substation within your development. It is advised to use Essential Energy’s Connection portal early to identify network needs and plan accordingly. Should network augmentation be necessary, consult the current list of Accredited Service Providers (ASPs) at https://www.energy.nsw.gov.au/households/guides-and-helpful-advice/being-more-energy-efficient/understand-your-energy-bill/altering-supply to arrange the necessary works.
1. Site Fill – Clean Material
Any proposed site fill must be of clean material only, free from organic matter, and compacted in horizontal layers not more than 250mm thick to 95% of the standard maximum dry density of the soil. A validation certificate shall be provided to Council verifying that the material to be used is free of contaminants and fit for purpose and re-use in residential, commercial or industrial use, prepared by a qualified Geotechnical Engineer. 
Note: Soil density tests from a NATA registered laboratory, and conducted in accordance with Australian Standard 1289, will be required, prior to the issue of a Construction Certificate for the erection of a building or the issue of a Subdivision Certificate.
1. Signage Installation
The proposed signage will be installed according to manufacturer and engineering requirements.



PRIOR TO OCCUPATION/USE
1. Occupation Certificate
An Occupation Certificate is to be obtained pursuant to Section 6.9 of the Environmental Planning and Assessment Act 1979, from the Principal Certifying Authority on completion of all works and prior to the occupation/use.
The “Occupation Certificate” shall not be issued if any conditions of this consent, but not the conditions relating to the operation of the development, are outstanding.
A copy of the Occupation Certificate and all necessary documentation supporting the issue of the Certificate is to be submitted to Lachlan Shire Council, if Council is not the Principal Certifying Authority.
1. Fire Safety Certificate 
Prior to issue of any Occupation Certificate, a Fire Safety Certificate shall be furnished to the Principal Certifying Authority for all the Essential Fire or Other Safety Measures forming part of this approval.  A copy of the Fire Safety Certificate must be submitted to Council by the Principal Certifying Authority with the Occupation Certificate. An electronic copy of the Final Fire Safety Certificate (together with a copy of the current Fire Safety Schedule) shall also be forwarded to the Fire Commissioner via the following dedicated email address: afss@fire.nsw.gov.au.
1. Wet Areas
Prior to the issue of any Occupation Certificate, a Certificate of Installation certifying that all the wet areas within the building have been protected by the installation of a water-proofing system conforming to AS 3740 and F2 D2 of the National Construction Code must be provided prior to the Principal Certifying Authority.
1. Occupancy Signage
A sign must be displayed in a prominent position within the Function Centre building that specifies the maximum number of persons that are permitted to occupy the Function Room as specified in this development consent, being 130 persons.
1. Parking
Prior to the Issue of any Occupation Certificate, all parking areas are to be provided and completed in accordance with the approved plans and to Council’s satisfaction.
Prior to the Issue of any Occupation Certificate, Tactile surface indicators shall be provided through the car park and pedestrian areas / walkways in accordance with the approved plans and AS2890.6-2004 Off-street Parking for People with Disabilities.
Directional signage and line marking shall be installed indicating directional movements and the location of customer parking to the satisfaction of the Principal Certifier.
1. Road Works
Prior to the issue of any Occupation Certificate, all temporary entrance cross-over material must be removed from the public road reserve.
Prior to the issue of any Occupation Certificate, all disused or redundant vehicle crossings and laybacks shall be removed and reinstated with concrete kerb and gutter or to the existing edging profile as specified by Council, with the footpath area also to be restored to the satisfaction of Council.


1. Post-construction dilapidation report
Prior to the issue of any occupation certificate a post-construction dilapidation report for the Unnamed Lane layback and pavement must be prepared by a suitably qualified engineer, detailing whether:
(a) after comparing the pre-construction dilapidation report to the post-construction dilapidation report required under this condition, there has been any structural damage to any adjoining buildings; and 
(b) where there has been structural damage to any adjoining buildings, that it is a result of the work approved under this development consent, and 
(c) a copy of the post-construction dilapidation report must be provided to Council.
1. Repair of public infrastructure
Prior to the issue of any occupation certificate:
(a) any public infrastructure damaged as a result of the carrying out of work approved under this consent (including damage caused by, but not limited to, delivery vehicles, waste collection, contractors, sub-contractors, concreting vehicles) must be fully repaired to the written satisfaction of council, and at no cost to council, or 
(b) if the works in (a) are not carried out to council’s satisfaction, council may carry out the works required and the costs of any such works must be paid as directed by council and in the first instance will be paid using the security deposit required to be paid under this consent.
1. Pavement of Vehicle Access and Parking Areas
Prior to the issue of Occupation Certificate, the paving of all vehicular access areas including vehicle parking spaces must be either a minimum of 150mm thick flexible pavement and sealed or 150mm thick reinforced concrete or as per the approved design.
1. Road Works
Prior to the issue of any Occupation Certificate, the Principal Certifier shall ensure that all works associated with a S138 Roads Act approval or S68 Local Government Act approval have been inspected and signed off by Lachlan Shire Council. 

1. Vehicle Parking Areas
Prior to the issue of Occupation Certificate, all parking areas are to be provided and completed in accordance with the approved Construction Certificate Plans and to Council’s Satisfaction.
1. Works As Executed - Stormwater Drainage
Prior to the issue of an Occupation Certificate, Works As Executed Plans must be submitted the Certifying Authority by a registered surveyor certifying compliance of all drainage works with the approved design plans.  The Works As Executed dimensions and levels must be shown in red on a copy of the approved Construction Certificate plans.  This plan must verify surface and invert levels on all pits, invert levels and sizes of all pipelines, and finished surface levels on all paved areas.  All levels must relate to Australian Height Datum.
1. [bookmark: OCCCON][bookmark: ANGCON]Stormwater Drainage
Prior to the issue of any Occupation Certificate, the Principal Certifier shall ensure that the stormwater management systems :
(a) have been satisfactorily completed in accordance with the approved Construction Certificate or Subdivision Works Certificate and the requirements of this consent; 
(b) have met the design intent with regard to any construction variations to the approved design, and; 
(c) Any remedial works required to be undertaken have been satisfactorily completed.   
Details of the approved and constructed system/s shall be provided as part of the Works As Executed drawings. 
1. Hydrants
An on-site fire hydrant and a booster facility at the street entrance to the site shall be installed in accordance with the requirements of AS 2419.1-2005 Fire Hydrant Installations - System Design, Installation and Commissioning. All of the work must be properly completed, including inspections required by the principal certifying authority, prior to the issue of an Interim Occupation Certificate. Alternatively, documentary evidence may be provided from the NSW Fire Brigade detailing their approval of alternative arrangements.
1. Swimming Pools
Prior to the issue of an Occupation Certificate, evidence shall be provided to demonstrate that the swimming pool has been registered in accordance with the Swimming Pools Act 1992.
Note:	The NSW swimming pool register can be accessed at www.swimmingpoolregister.nsw.gov.au
1. Swimming Pools
Prior to the issue of any Occupation Certificate access to the pool shall be restricted by a child resistant barrier in accordance with the regulations prescribed in the Swimming Pools Act, 1992, and:
(a) the pool must not to be completely filled with water until such time as a safety fence has been erected in accordance with this certificate.
(b) Where the depth of water in the pool exceeds 300mm during construction a temporary barrier or fence must be erected or other precautions taken so as to prevent the entry of children into the pool.
(c) The swimming pool including overflow water must be drained to the sewer or, if the sewer is not available, overflow water must be disposed of to Council’s satisfaction.
(d) The consent of the Council must be obtained 48 hours prior to any emptying of pool water into the sewer.
Certification from an appropriately qualified person confirming compliance with these requirements shall be provided prior to the issuing of any Occupation Certificate.
1. Swimming Pools
Prior to the issue of any Occupation Certificate the owner of the pool shall display a notice showing:
(a) the words:
(i) “YOUNG CHILDREN SHOULD BE SUPERVISED WHEN USING THIS SWIMMING POOL”, and
(ii) “POOL GATES MUST BE KEPT CLOSED AT ALL TIMES”, and
(iii) “KEEP ARTICLES, OBJECTS AND STRUCTURES AT LEAST 900 MILLIMETRES CLEAR OF THE POOL FENCE AT ALL TIMES”,
(b) a simple flow sequence (which may be the flow sequence depicted in the Cardiopulmonary Resuscitation Guideline) containing details of resuscitation techniques (for infants, children and adults):
(i) That are set out in accordance with the relevant provisions of that Guideline, and
(ii) That comply with the other relevant guidelines of the Australian Resuscitation Council, and
(iii) That is illustrated by drawings with key words only in bold print,
(c) A statement to the effect that formal instruction in resuscitation is essential,
(d) The name of the teaching organisation or other body that published the sign and the date of its publication.
Details demonstrating compliance are to be provided with any Occupation Certificate issued for the pool.
1. Pool Filter
Prior to the issue of an Occupation Certificate, the pool filtering equipment shall be encased by a soundproof cover and shall be located as far as is practical from adjoining premises so that noise levels shall not exceed 5dBA above the ambient noise level when measured at the property boundary. Pool equipment shall not operate between 9.00 pm and 7.00 am.
1. Pool Recirculation System
The certifying authority shall not issue an Occupation Certificate to authorise a person to commence the use of a spa or swimming pool unless the certifying authority has received a certificate that verifies that the recirculation system of the spa or swimming pool was installed, has been tested and performs in accordance with the requirements set out in AS 1926.3—2010, Swimming pool safety, Part 3: Water recirculation systems as published by Standards Australia, as in force from time to time. That certificate must be provided by: 
(a) The principal contractor who installed the spa or swimming pool, or
(b) In the event that the spa or swimming pool has been installed or constructed under the authority of an owner-builder permit, from the installer or constructor of the spa or swimming pool, or
(c) Some other person who, in the opinion of the certifying authority, is suitably qualified to provide the certificate.
1. Signage quality and lighting
The approved signage shall have a high quality and finish, and any lighting of the sign must comply with Australian Standard AS 4282:2019 - Control of the Obtrusive Effects of Outdoor Lighting
1. Plan of Management
Prior to the issue of any Occupation Certificate, a Plan of Management (POM) for the motel and function centre is to be developed and submitted to Council for approval. The POM must include details of how noise nuisance will be mitigated to surrounding receivers. 
The Plan of Management is to satisfactorily addresses management of potential acoustic and amenity impacts in accordance with the operational details in Condition 82.
1. Flood Evacuation Plan
Prior to the issue of any Occupation Certificate, a Flood Evacuation Plan is to be developed and submitted to Council for approval.
1. Wastewater
Wastewater from the washing of garbage bins and vehicles is not to enter the stormwater system.
1. Landscaping
Prior to the issue of any occupation certificate, the landscaping (including installation of an adequate watering system) is to be carried out and maintained in accordance with the approved landscape plan.
1. Street Trees
Prior to the issue of any occupation certificate, street trees are to be planted along the road frontages to offset any removed during construction, having regard to location of services and driveways.


DURING USE
1. Operating and Delivery Hours
The hours of operation of the are restricted to the times listed below:
· The motel reception is to operate between the hours 7.00am to 10.00pm, 7 days a week. 
· The motel kitchen is to operate between the hours 6.00am to 10.00pm, 7 days a week. 
· Deliveries are to occur between 7.00am to 7.00pm, 7 days a week. 
· The function centre is to operate between the hours 7.00am to 12.00am, 7 days a week, subject to all music / amplified sound after 10.00pm being located inside the function centre building, with bass noise kept at low levels, and all music and amplified sound equipment to be turned off at 11.30pm.
· The outdoor areas of the motel are to be sign-posted as a ‘quiet area between 10.00pm and 7.00am’.
· The onsite manager is to be responsible for the control of noise at the motel and function centre and the keeping of a complaints register.
1. Plan of Management
The approved Plan of Management is to be adhered to at all times during operation.
1. [bookmark: _Toc22225507]Noise
At no time shall the use of the premise give rise to ‘offensive noise’ as defined under the Protection of the Environment Operations Act 1997.
During ongoing use of the premises, the premises must be operated in accordance with the Noise Impact Assessment report approved under this consent.
Should substantiated noise complaints be received by Council, Council reserves the right to seek an Acoustic Report, to be paid for by the operator of the premises, to determine the noise impacts of the development in accordance with the Noise Policy for Industry (NPI). Mitigation measures required to bring the development into compliance with the NPI are to be implemented and maintained for the duration of the development. Noting that the works may require modification of this development consent.
1. Land-use Limitations
The approved capacity for the Function Centre venue shall not exceed 130 persons and must comply with the relevant provisions of Section 72 and 73 of the Environmental Planning & Assessment Regulation 2021.
1. Liquid Waste/Trade Waste
No contaminated waste water or liquid waste is to be discharged into Lachlan Shire Council's stormwater or sewerage system without a prior Trade Waste Agreement being entered into with Council and the Applicant.


1. Disability Access
The premises shall comply with the Disability (Access to Premises - Buildings) Standards 2010.
1. Swimming Pools
(a) The swimming pool (spa) must comply with the Swimming Pools Act 1992 and Swimming Pools Regulation 2018 at all times. This includes any maintenance or modifications.
(b) The child-resistant barrier must remain installed and maintained around the pool (spa) (unless exemptions apply) to the standards set out in AS 1926.1 -2012 and AS 1926.2 - 2007 and be in good repair at all times.
(c) The Warning Notice shall be maintained in a legible manner in accordance with Part 3 of the Swimming Pools Regulation 2008 for the life of the swimming pool.
(d) The noise of any filtration equipment or pumps must not exceed 5dBA above the ambient background noise level measured at the property boundary.
1. Fire Safety
The owner of the building must maintain each essential fire safety measure in the building premises to a standard no less than that specified in the Schedule. 
The owner of the building is required to submit to Council at least once in each period of 12 months following the completion of the building an Annual Fire Safety Statement(s) with respect to each essential fire safety measure associated with the building.
Copies of the subject Annual Fire Safety Statements must also be forwarded by the owner to the Commissioner of Fire and Rescue NSW and displayed within the subject building in a prominent position. In this regard, Fire and Rescue NSW has requested that only electronic copies of the statement be forwarded to their dedicated email address, being afss@fire.nsw.gov.au
1. Manoeuvring of Vehicles
All vehicles to enter and exit the site in a forward direction and are not to be reversed onto the adjoining road reserve. 
Internal vehicular manoeuvring aisles, parking areas and loading bays shall be maintained clear of obstruction and used exclusively for the purposes of vehicle access, parking and loading and unloading respectively. Under no circumstances shall these areas be used for the storage of goods or waste receptacles or any other purpose. 
1. Vehicle Parking Spaces
A minimum of 42 on-site parking spaces including one (1) disabled space and two (2) EV bays must be made available on site at all times in accordance with the approved plans and relevant Australian Standards 
1. Amenity - General
The development is to be conducted in a manner that will not interfere with the amenity of the locality by reason of the emission of noise, vibration, smell, fumes, smoke, vapour, steam, soot, ash, dust, waste water, waste products, grit, oil, by causing interference to television or radio reception or otherwise.
1. Landscaping
The landscaped area of the development is to be maintained at all times in accordance with the approved Landscape plan.  Any vegetation that dies shall be replaced.
Any landscaping, fencing and signage to be provided within the site or along the boundary with any adjoining road reserve is to be designed and maintained to provide safe sight distance to pedestrians for motorists entering and exiting the site to minimise conflict in accordance with AS2890.1 “Off-street car parking”. 
1. Product display limitation
No product display is permitted within the setbacks. The landscaped areas are to be maintained and not used for product display.
1. Waste Management and Disposal 
Provision shall be made for the disposal, and containment, of garbage and waste generated by the development. Receptacles shall ensure garbage and waste cannot escape by wind or water and must be cleaned regularly.
1. Lighting
	All exterior lighting associated with the development must be designed and installed so that no obtrusive light will be cast onto any adjoining property. All lighting must comply with the AS 4282:1997 Control of the Obtrusive Effects of Outdoor Lighting.
1. Storage and Handling of Flammable and Combustible Liquids
At all times the storage and handling of any flammable and combustible liquids is to be in accordance with AS 1940-2004 The storage and handling of flammable and combustible liquids
All above ground storage facilities containing flammable and combustible liquids must be bunded, stored and managed in accordance with AS 1940-2004 The storage and handling of flammable and combustible liquids.
1. Contamination
No contaminated waste water or liquid waste is to be discharged into Lachlan Shire Council's stormwater or sewerage system without a prior Trade Waste Agreement being entered into with Council and the Applicant.



Prescribed conditions under the Environmental Planning and Assessment Regulation 2021
All development must comply with the following where relevant:
P.1	Compliance with Building Code of Australia and insurance requirements under the Home Building Act 1989
P.1.1	 It is a condition of a development consent for development that involves building work that the work must be carried out in accordance with the requirements of the Building Code of Australia.
 P.1.2	It is a condition of a development consent for development that involves residential building work for which a contract of insurance is required under the Home Building Act 1989, Part 6 that a contract of insurance is in force before building work authorised to be carried out by the consent commences.
 P.1.3 	It is a condition of a development consent for a temporary structure used as an entertainment venue that the temporary structure must comply with the Building Code of Australia, Volume 1, Part B1 and NSW Part I5.
In condition  P.1.1, a reference to the Building Code of Australia is a reference to the Building Code of Australia as in force on the relevant date.
Relevant date has the same meaning as in the Environmental Planning and Assessment (Development Certification and Fire Safety) Regulation 2021, section 19.
 In condition  P.1.3, a reference to the Building Code of Australia is a reference to the Building Code of Australia as in force on the day on which the application for development consent was made.
 This condition  P.1 does not apply—
(a) to the extent to which an exemption from a provision of the Building Code of Australia or a fire safety standard is in force under the Environmental Planning and Assessment (Development Certification and Fire Safety) Regulation 2021, or
(b) to the erection of a temporary building, other than a temporary structure to which condition  P.1.3 applies.
 P.2 	Erection of signs
This condition applies to a development consent for development involving building work, subdivision work or demolition work.
P.2.1	It is a condition of the development consent that a sign must be erected in a prominent position on a site on which building work, subdivision work or demolition work is being carried out—
(a) 	showing the name, address and telephone number of the principal certifier for the work, and
(b) 	showing the name of the principal contractor, if any, for the building work and a telephone number on which the principal contractor may be contacted outside working hours, and
 (c) 	stating that unauthorised entry to the work site is prohibited.
P.2.2	 The sign must be—
(a)	maintained while the building work, subdivision work or demolition work is being carried out, and
(b) 	removed when the work has been completed

This condition does not apply in relation to—
(a) 	building work, subdivision work or demolition work carried out inside an existing building, if the work does not affect the external walls of the building, or
(b) 	Crown building work certified to comply with the Building Code of Australia under the Home Building Act 1989, Part 6
  P.3 	Notification of Home Building Act 1989 requirements
This condition applies to a development consent for development involving residential building work if the principal certifier is not the council.
P.3.1 	It is a condition of the development consent that residential building work must not be carried out unless the principal certifier for the development to which the work relates has given the council written notice of the following—
(a) 	for work that requires a principal contractor to be appointed—
(i)	the name and licence number of the principal contractor, and
(ii)	the name of the insurer of the work under the Home Building Act 1989, Part 6,
(b) 	for work to be carried out by an owner-builder—
(i) 	the name of the owner-builder, and
(ii) 	if the owner-builder is required to hold an owner-builder permit under the Home Building Act 1989—the number of the owner-builder permit.
P.3.2 	If the information notified under the above condition is no longer correct, it is a condition of the development consent that further work must not be carried out unless the principal certifier has given the council written notice of the updated information.
 P.4 	Condition relating to shoring and adequacy of adjoining property
This condition applies to development that involves excavation that extends below the level of the base of the footings of a building, structure or work on adjoining land, including a structure or work in a road or rail corridor.
P.4.1 It is a condition of the development consent that the person having the benefit of the development consent must, at the person’s own expense—
(a) 	protect and support the building, structure or work on adjoining land from possible damage from the excavation, and
(b) 	if necessary, underpin the building, structure or work on adjoining land to prevent damage from the excavation.
This condition does not apply if—
(a) 	the person having the benefit of the development consent owns the adjoining land, or
(b) 	the owner of the adjoining land gives written consent to the condition not applying

Reasons for Conditions:
Development Application № 2025/28 was assessed using current procedures developed by the Lachlan Shire Council and other resource information.  This includes:
· the requirements of Section 4.15 of the Environmental Planning and Assessment Act 1979 which states:
Section 4.15(1) Matters for consideration – general
In determining a development application, a consent authority is to take into consideration such of the following matters as are of relevance to the development the subject of the development application:
(a) the provisions of:
(i)      any environmental planning instrument, and
(ii)     any draft environmental planning instrument that is or has been placed on public exhibition and details of which have been notified to the consent authority, and
(iii)    any development control plan, and
(iv)    any matters prescribed by the regulations that apply to the land to which the development application relates
(b) the likely impacts of that development, including environmental impacts on both the natural and built environments and social and economic impacts in the locality
(c) the suitability of the site for the development
(d) any submissions made in accordance with this Act or the regulations
(e) the public interest
· the requirements of the Lachlan Local Environmental Plan 2013
· the requirements of the following Development Control Plans and Council Policies:
(i)      Lachlan Shire Development Control Plan 2018
· field inspection and liaison between officers of the Lachlan Shire Council
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