


Attachment A: Draft Conditions of Consent
	DA Number
	DA-19/2025

	Applicant

	Applicant Name
	ATJs Earthworks Pty Ltd

	Applicant Address
	472 Eddy Park Lane, Gum Flat NSW 2360

	Owner

	Owner Name
	Glen and Sonya Hough

	Owner Address
	472 Eddy Park Lane, Gum Flat NSW 2360

	Land to be Developed

	Property Address
	472 Eddy Park Lane, Gum Flat NSW 2360

	Property Title
	Lot 106 DP 656030

	Proposed Development

	Development Description
	Continued operation of existing gravel quarry with a maximum extraction rate of 90,000 tonnes per year





Conditions
	General Conditions

	1. 
	Approved Plans and Supporting Documentation 
Development must be carried out in accordance with the following approved plans and documents, except where the conditions of this consent expressly require otherwise.

	Document Title
	Rev No. 
	Prepared by
	Dated

	Environmental Impact Statement including:
Appendix A Quarry Plans
Appendix B Secretary’s Environmental Assessment Requirements
Appendix I AHIMS Search Results
Appendix K Historic Imagery
	5
	SMK Consultants
	19/03/2026

	EIS Appendix C Noise Impact Assessment
	01-B
	Soundscape Acoustic Consultants
	10/09/2025

	EIS Appendix D Land Use Conflict Risk Assessment
	1
	SMK Consultants
	Mar 2026

	EIS Appendix E Matters of National Environmental Significance Assessment
	
	SMK Consultants
	Undated

	EIS Appendix F NSW Biodiversity Act 2016 Test of Significance
	
	SMK Consultants
	Undated

	EIS Appendix G Traffic Impact Assessment
	1
	SMK Consultants
	Nov 2025

	EIS Appendix H Rehabilitation Plan
	2
	SMK Consultants
	Feb 2026

	EIS Appendix J Soil and Water Management Plan
	2
	SMK Consultants
	10/03/2026

	EIS Appendix L Operational and Environmental Management Plan
	1
	SMK Consultants
	10/03/2026

	EIS Appendix M Air Quality Impact Assessment
	1
	Advitech
	19/03/2026

	EIS Appendix N Bushfire Assessment Report
	0
	SMK Consultants
	Nov 2025

	EIS Appendix O Pollution Incident Response Management Plan
	0
	SMK Consultants
	Nov 2025

	EIS Appendix P Biosecurity Risk Management Plan
	0
	SMK Consultants
	Mar 2026


In the event of any inconsistency between the approved plans and the supporting documentation, the approved plans prevail. In the event of any inconsistency between the approved plans and a condition of this consent, the condition prevails.

Reason: To ensure all parties are aware of the approved plans and supporting 
documentation that applies to the development.

	2. 
	General Terms of Approval – External Agencies
Development must be carried out in accordance with the General Terms of Approval issued by external agencies (which are attached to this Consent), except where the conditions of this consent expressly require otherwise.

	External Agency
	Attachment
	Date GTAs Issued

	NSW Environment Protection Authority
	1
	24/12/2025



In the event of any inconsistency between the General Terms of Approval and the approved plans and the supporting documentation, the General Terms of Approval prevail. In the event of any inconsistency between the approved plans and a condition of this consent, the condition prevails.

Reason: To ensure all parties are aware of the approved plans and supporting 
documentation that applies to the development.


	3. 
	Limitations to Approval
To confirm and clarify the terms of this approval, consent is given for the following:
(a) Quarry extraction and/or transport of no more than 90,000 tonnes of material, including hard rock, gravel, fines and sand from the development site in any calendar year.
(b) The applicant shall not extract material from outside the designated area as shown in drawing “Site Plan” prepared by SMK Consultants and dated included in Appendix A of the EIS Version 5 dated 19/03/2026.
(c) The applicant shall not import material, other than products that are essential for quarrying operations, onto the site without prior consent. 
(d) The applicant shall not dispatch more than 20 10 laden trucks from the site per day. 
(e) The operator shall notify the Council in writing, within three (3) months of the end of each calendar year, the total quantity of material quarried and provide details of final output in terms of product.
(f) This consent is time limited to 30 years from the date of consent or when the material to be extracted has been exhausted, whichever occurs first.

Reason: To confirm and clarify the terms of this approval.


	4. 
	Quarry Boundary Delineation
Within three months of the date of this consent, the extent of the quarry area as approved under this consent shall be surveyed and pegged out by a Registered Land Surveyor. A Survey Plan of the delineated area, prepared by the Registered Surveyor, shall be submitted to Council prior to the commencement of any quarrying operations in accordance with this consent. The pegs delineating the approved quarry area are to be maintained for the life of quarry Operations.

Reason: To clarify the extent of the approval on the subject land.


	5. 
	Section 7.11 Contributions 
A Section 7.11 (formerly Section 94) contribution is to be paid to Council for road maintenance at a rate of $0.50 per tonne of product or extracted material and is subject to CPI adjustment each financial quarter.

The operator is to provide Council with details of extracted material each financial year at the date that payment is made. If Council does not receive these details, the contribution will be levied on the maximum extraction of 90,000 tonnes of material for that financial year. 

Note: The CPI rate will be the All Groups rate as released by the ABS on a quarterly basis. The applicable CPI rate will be as per the previous quarter to ensure there is an available CPI rate at time of calculation.

Reason: Statutory requirement.


	6. 
	Chemical Storage and Use
During site works and for the life of the project: 
(a) Store all chemicals in accordance with relevant Australian standards and the Environment Protection Authority’s Storing and Handling of Liquids: Environmental Protection – Participants Manual (Department of Environment and Climate Change, 2007).
(b) Place all chemicals inside a secured shed or covered bunded area with 110% capacity of the total volume of the chemical stored.
(c) Store chemicals in closed, labelled containers, and store copies of Safety Data Sheets (SDS) for all chemicals along with spill clean-up kits on site. 
(d) Ensure that any spills are cleaned up immediately in accordance with the SDS.
(e) Train all staff how to safely use and store these chemicals prior to the commencement of work.

In the event of any inconsistency between this condition and the Environmental Protection Licence (EPL) for the premisesquarry, the EPL prevails.

Reason: To require the effective management and correct storage of chemicals to mitigate pollution risk on construction sites.


	7. 
	Discovery of Relics and Aboriginal Objects
While works are being carried out, if a person reasonably suspects a relic or Aboriginal 
object is discovered:
(a) the work in the area of the discovery must cease immediately;
(b) the following must be notified:
(i) for a relic – the Heritage Council; or
(ii) for an Aboriginal object – the person who is the authority for the protection of Aboriginal objects and Aboriginal places in New South Wales under the National Parks and Wildlife Act 1974, section 85.

Works may recommence at a time confirmed in writing by:
(a) for a relic – the Heritage Council; or
(b) for an Aboriginal object – the person who is the authority for the protection of Aboriginal objects and Aboriginal places in New South Wales under the National Parks and Wildlife Act 1974, section 85.

Reason: To ensure the protection of objects of potential significance during works.


	8. 
	Contaminated Land Unexpected Finds
During site works and for the life of the project, in the instance works cause the generation of odours or uncovering of unexpected contaminants, works are to immediately cease, Council is to be notified and a suitably qualified environmental scientist appointed to further assess the site. 

The exposed material/excavation is to be evaluated by the supervising environmental consultant and an appropriate response determined in consultation with the applicant, which is agreed to by Inverell Shire Council.

Note: Council may also request that a NSW EPA accredited site auditor is involved to assist with the assessment of the contaminated land situation and review any new contamination information. The applicant must also adhere to any additional conditions which may be imposed by the accredited site auditor.

Reason: To ensure compliance with statutory requirements.


	Before Site Work Commences

	9. 
	Environmental Protection Licence (EPL)
Prior to any works associated with this consent, an Environmental Protection Licence from the NSW Environmental Protection Authority (EPA) shall be obtained. 

The premises quarry must be operated and managed in accordance with the EPL at all times. See the EPA's General Terms of Approval attached.

Reason: Statutory requirement.


	10. 
	Environmental Management Plan
Prior to any works associated with this consent, an Environmental Management Plan (EMP) must be prepared and shall be submitted to Council for approval. This plan must provide the following (at a minimum):
(a) Provide the strategic framework for environmental management of the project; 
(b) Identify the statutory approvals that apply to the project; 
(c) Set out the role, responsibility, authority and accountability of all key personnel involved in the environmental management of the project; 
(d) Set out the procedures to be implemented to: 
(i) keep the local community and relevant agencies informed about the operation and environmental performance of the project; 
(ii) receive, record and respond to complaints; 
(iii) resolve any disputes that may arise during the course of the project; 
(iv) respond to any non-compliance and any incident; and 
(v) respond to emergencies. 
(e) A protocol for periodic review of the plan if required;
(f) Include plans for the management and monitoring to ensure the operations comply with the relevant criteria and conditions of this approval for the following: 
(i) Noise including the recommendations in the Noise Impact Assessment prepared by Soundscape and dated 10/09/2025
(ii) Air quality and dust control
(iii) Surface water and Groundwater 
(iv) Traffic including Driver Code of Conduct
(v) Aboriginal cultural heritage 
(vi) Biodiversity 
(vii) Bushfire 
(viii) Waste
(g) A summary of any environmental monitoring to be carried out under the conditions of this approval and EPL. 
(h) Describe the procedures that would be implemented for health and safety at the site, including a detailed emergency plan, developed in consultation with local emergency services.

The approved Environmental Management Plan shall be implemented at all times during site works and during operations.

Reason: To ensure that environmental impacts are adequately managed.


	11. 
	Primary haulage route – Eddy Park Lane south bound to the Gwydir Highway via Copeton Dam Road east bound
Prior to any works associated with this consent, the approved primary haulage route from the site access via Eddy Park Lane south bound to Copeton Dam Road must be upgraded and bitumen sealed. This includes the access crossing from Eddy Park Lane to the site boundary.

Before the road upgrade and access sealing works commence, a separate application must be made to Council for approval under Section 138 of the Roads Act 1993 for these works.

The application for approval under Section 138 of the Roads Act 1993 must be accompanied by detailed engineering survey and design.

Reason: To ensure the road is upgraded to a sufficient standard relative to the use and ensure all necessary approvals under the Roads Act 1993 are obtained for the development.


	12. 
	Secondary haulage route – Eddy Park Lane north bound to the Gwydir Highway
Eddy Park Lane is not an approved route for Restricted Access Vehicles.

Significant upgrade works are required to Eddy Park Lane before any haulage is undertaken north bound via Eddy Park Lane connecting to the Gwydir Highway.

The road upgrades, must include but not necessarily be limited to, road realignment to achieve suitable geometry, road widening, and bitumen sealing.

Before any road upgrade works commence to the secondary haulage route, a separate application must be made to Council for approval under Section 138 of the Roads Act 1993 for these works.

The application for approval under Section 138 of the Roads Act 1993 must be accompanied by detailed engineering survey and design to achieve Restricted Vehicle Access standard of road geometry and construction.

In the event that the proponent elects to not proceed with upgrades for the secondary route, only the primary route as specified under Condition 11 is permitted to be used.

Reason: To ensure the road is upgraded to a sufficient standard to accommodate the heavy vehicle movements and ensure all necessary approvals under the Roads Act 1993 are obtained for the development.


	13. 
	Traffic Management Plan
Prior to any works associated with this consent, a Traffic Management Plan is to be submitted to and approved by Council. The TMP is to address the construction (as relevant to the existing 
operation), ongoing operation, and decommissioning phases of the proposed 
development. 

The TMP should be prepared and implemented in accordance with Australian Standard 
1742.3 and the Work Health and Safety Regulation 2017. 

The TMP should address, but not necessarily be limited to, the following matters:

· A map of the primary transport route/s highlighting critical locations, 
· An induction process for vehicle operators and regular toolbox meetings, 
· Procedures for travel through residential areas, school zones and/or bus route/s, 
· Any proposed temporary measures, such a Traffic Guidance Scheme (TGS), 
· A Driver Code of Conduct for heavy vehicle operators, 
· A complaint resolution and disciplinary procedure, 
· Community consultation measures proposed for peak periods.

Reason: To comply with the requirements of Transport for NSW.


	14. 
	Soil and Water Management Plan
Prior to any works associated with this consent, a Soil and Water Management Plan must be prepared by a suitably qualified person in accordance with the following documents and provided to Council for approval:

1. The guidelines set out in 'Managing Urban Stormwater: Soils and Construction’ prepared by Landcom (the Blue Book) (as amended from time to time), and
2. The ‘Guidelines for Erosion and Sediment Control on Building Sites’ (Department of Planning, Housing and Infrastructure) (dated 2024, as amended from time to time).

The approved controls must remain in place until any bare earth has been restabilised in accordance with the erosion and sediment control plan.

A plan must always be kept on site during works and made available to Council officers and any other relevant authorities on request. 

The approved Soil and Water Management Plan shall be implemented at all times during site works and during operations.

In the event of any inconsistency between this condition and the Environmental Protection Licence (EPL) for the premises, the EPL prevails.

Reason: To ensure sediment laden runoff and site debris do not impact local 
stormwater systems, waterways, downstream properties or the road.


	15. 
	Waste Management Plan
Prior to any works associated with this consent, a waste management plan for the development must be 
prepared and provided to Council for approval. The plan must be prepared:
(a) in accordance with— 
(i) the Environment Protection Authority’s Waste Classification Guidelines as in force from time to time; and
(ii) any development control plan that provides for waste management that applies to the land on which the work or the clearing of vegetation is carried out; and
(b) include the following information—
(i) the name and contact details of who is responsible for the plan and management of the waste onsite,
(ii) the name and contact details of the person(s) removing waste,
(iii) a description of each different waste type and an estimate of the and quantity of each waste type expected to be produced,
(iv) how each waste type will be managed onsite and offsite, including whether the waste is expected to be reused, recycled or sent to landfill,
(v) where any onsite management of waste will occur, such as for consolidation and collection,
(vi) how each waste type will be characterised and classified for waste management and transport,
(vii) where each waste type is intended to be transported for disposal or other fate,
(viii) how the quantity of each waste type will be measured and recorded,
(ix) how each waste movement will be tracked,
(x) contingencies including managing unexpected finds, such as asbestos.

A copy of the waste management plan must be kept on-site at all times while work approved under the development consent is being carried out.

The approved Waste Management Plan shall be implemented at all times during site works and during operations.

In the event of any inconsistency between this condition and the Environmental Protection Licence (EPL) for the premisesquarry, the EPL prevails.

Reason: To ensure waste management practices are undertaken, resource 
recovery is promoted and local amenity protected during construction site works.


	16. 
	Bush Fire Emergency Management and Evacuation Plan
Prior to any works associated with this consent, a Bush Fire Emergency and Evacuation Plan prepared by a qualified consultant, in accordance with Planning for Bushfire Protection 2019 and any other relevant guidelines is to be submitted to and approved by Council.

The approved Bush Fire Emergency Management and Evacuation Plan is to be kept updated, and a copy of the updated plan provided to Council and kept on site.

Reason: To ensure the safety of employees, visitors and residents on bush fire prone land.


	17. 
	Rehabilitation Plan
Prior to any works associated with this consent, a Rehabilitation and Closure Plan must be prepared and submitted to Council for approval. At a minimum, a rehabilitation plan must:
(a) outline the final land use and landform options considered, and justification of the preferred option; 
(b) detail any rehabilitation methods to be implemented for both planned and unplanned closure of the site, including the testing of imported material to confirm it is suitable for rehabilitation; 
(c) list suitable completion criteria; 
(d) include a risk assessment to demonstrate any post-closure hazards associated with the proposed final landform and land use are acceptable; and 
(e) provide an estimate of the closure costs prepared in accordance with the current industry recognised guidelines.

The approved Rehabilitation Plan shall be implemented at all times during site works and during operations.

Reason: To make the site safe and suitable for future use, minimise erosion, reintroduce biodiversity, prevent introduction of noxious weeds and pests, and limit visual impacts. 


	18. 
	Site Safety Fencing
Prior to any works associated with this consent, site fencing shall be erected to a minimum height of 1.8m 
complying with SafeWork NSW Guidelines, to exclude access to the site throughout 
works. The site shall be maintained in a clean and orderly condition during works.

The site fencing required by this consent is to be maintained for the life of the quarry. Appropriate signage, fencing, bunding or the like must be installed to prevent visitor and unauthorised vehicle access to working areas of the quarry.

Business identification signage and the rural address of the site is to be provided in a visible place near the entrance for the convenience of contractors and emergency services. 

Reason: Statutory requirement and to ensure adequate public safety and health and safety measures.


	Occupation and Ongoing UseDuring Site Works

	19. 
	Site Management During Works
During site preparation worksongoing use the following procedures apply: 
(a) All possible and practical steps shall be taken to prevent nuisance to the inhabitants of the surrounding neighbourhood from windblown dust, debris, noise and the like;
(b) Prevent sediment and materials being carried or washed onto the road, or into nearby waterways; 
(c) Ensure soil/excavated material is not transported on wheels or tracks of vehicles or plant and deposited on surrounding roadways; 
(d) Ensure safe access to and from the site including the road reserve, crossings by heavy equipment, plant and materials delivery, or static loads from cranes, concrete pumps and the like; 
(e) Ensure safe loading and unloading of excavation machines, materials, etc. within the site; 
(f) Ensure storage on site of all excavated material, construction materials and waste containers during the works period (except where otherwise approved); and 
(g) Ensure support of any excavation beside any adjoining property or the road reserve is designed by a Chartered Civil Engineer.
(h) A single entrance is permitted to service the site.
(i) No blasting, crushing or screening is to be carried out at any time.
(j) Adjoining owner property rights and the need for owner's permission must be observed at all times, including the entering onto land for the purpose of undertaking works.
(k) The disposal of construction and demolition waste must be in accordance with the requirements of the Protection of the Environment Operations Act 1997.
(l) All waste on the site is to be stored, handled and disposed of in such a manner as to not create air pollution (including odour), offensive noise or pollution of land and/or water as defined by the Protection of the Environment Operations Act 1997. All excavated material should be removed from the site in the approved manner and be disposed of lawfully to a tip or other authorised disposal area. 
(m) Section 143 of the Protection of the Environment Operations Act 1997 requires waste to be transported to a place which can lawfully accept it. All non-recyclable demolition materials are to be disposed of at an approved waste disposal depot in accordance with legislation. 
(n) All materials on site or being delivered to the site are to be contained wholly within the site. The requirements of the Protection of the Environment Operations Act 1997 must be complied with when placing/stockpiling loose material, disposing of concrete waste, or other activities likely to pollute drains or water courses. 
(o) Details as to the method and location of disposal of demolition materials weight dockets, receipts etc. should be kept on site as evidence of approved methods of disposal and recycling. 
(p) Any materials stored on site must be stored out of view or in such a manner so as not to cause unsightliness when viewed from nearby lands or roadways. 
(q) Public roadways and road reserves adjacent to the site must be fully maintained and cleared of obstructions during works.

In the event of any inconsistency between this condition and the Environmental Protection Licence (EPL) for the premisesquarry, the EPL prevails.

Reason: To ensure adequate environmental protection.


	20. 
	Soil Management
While site work is being carried out, all soil removed from or imported to the site shall be managed in accordance with the following requirements: 
(a) All excavated material removed from the site must be classified in accordance with the Environment Protection Authority’s Waste Classification Guidelines before it is disposed of at an approved waste management facility or otherwise lawfully managed, and the classification, and the volume of material removed, and the receival facility’s details must be reported to the Council.
(b) All fill material imported to the site must be: 
(i) Virgin Excavated Natural Material as defined in Schedule 1 of the Protection of the Environment Operations Act 1997; or
(ii) a material identified as being subject to a resource recovery exemption by the NSW EPA; or
(iii) a combination of Virgin Excavated Natural Material as defined in Schedule 1 of the Protection of the Environment Operations Act 1997 and a material identified as being subject to a resource recovery exemption by the NSW EPA.

In the event of any inconsistency between this condition and the Environmental Protection Licence (EPL) for the premises, the EPL prevails.

Reason: To ensure soil removed from the site is appropriately disposed of and
soil imported to the site is not contaminated and is safe for future occupants.


	21. 
	Waste Management
While site work is being carried out:
(a) All waste management must be undertaken in accordance with the approved Waste Management Plan; and 
(b) Upon disposal or removal of the waste, records of the disposal or other fate (such as re-use on site) must be compiled and provided to the Principal Certifier detailing the following: 
(i) The name and contact details of the person(s) who removed the waste,
(ii) The waste carrier vehicle registration,
(iii) The date and time of waste collection,
(iv) A description of the waste (type of waste, classification and estimated quantity) and whether the waste is to be reused, recycled, go to landfill or other fate.
(v) The contact details and address of the disposal location or other offsite location(s) where the waste was taken,
(vi) The corresponding tip docket/receipt from the site(s) to which the waste is transferred, noting date and time of delivery, description (type and quantity) of waste.
(c) The waste generated on site during construction must be classified in accordance with the Environment Protection Authority’s Waste Classification Guidelines, 2014 (as amended from time to time) and disposed of to an approved waste management facility or otherwise lawfully managed.

If waste has been removed from the site where the waste is under an Environment Protection Authority Resource Recovery Order or Exemption, records in relation to and required by that Order or Exemption must be maintained and provided to the Principal Certifier and Council.

In the event of any inconsistency between this condition and the Environmental Protection Licence (EPL) for the premises, the EPL prevails.

Reason: To require records to be provided, during site work, documenting the lawful disposal of waste.


	Occupation and Ongoing Use

	22. 
	Quarterly Reporting
A quarterly report is to be submitted to Council including:
· Extraction volumes
· Truck movements
· Environmental monitoring and results against relevant requirements
· Complaints and responses/resolutions by quarry management

Reason: To allow environmental impacts to be monitored regularly.


	23. 
	Compliance with Approved Management Plans
During operations, the development is to comply with all management plans required by this consent, as follows:
· Environmental Management Plan
· Traffic Management Plan
· Soil and Water Management Plan
· Waste Management Plan
· Bushfire Emergency Management and Evacuation Plan
· Rehabilitation Plan

A copy of these plans must be kept on site at all times while work approved under the development consent is being carried out.

The operator of the quarry must ensure that all employees and contractors (and their sub-contractors) are made aware of, and instructed to comply with, the conditions of this approval relevant to activities they carry out in respect of the project. 

This includes all obligations under the relevant Management Plans and Driver Code of Conduct.

Reason: To ensure the operation is appropriately managed, ensure public safety and protect the amenity of the local area.


	24. 
	Compliance with Land Use Conflict Risk Assessment
During operations, the development is to implement the mitigation measures set out in Section 3.5 of the approved Land Use Conflict Risk Assessment.

Reason: To ensure land use conflicts are appropriately mitigated.


	25. 
	Hours of Operation
The hours of operation of the quarry pit operations, product loading and transportation shall be as follows (as required and licensed by the NSW Environmental Protection Authority):
· Monday to Friday – 7.00am to 5.00pm
· Saturday, Sunday and Public Holiday – No Operations

Maintenance and servicing of plant and equipment may only be undertaken during the following hours (as required and licensed by the NSW Environmental Protection Authority):
· Monday to Friday – 7.00am to 5.00pm
· Saturday, Sunday and Public Holiday – 7.00am to 5.00pm

Reason: To protect the amenity of the local area.


	26. 
	Parking
A designated parking area for employee and visitor vehicles is to be provided on site. The parking area does not need to be linemarked, but should be signposted. 

Reason: To improve safety for workers and visitors.

	27. 
	Aquifer Test Pits
As the quarry floor deepens, test pits of 1-2 metres in depth are to be dug to ensure operations will not breach the aquifer. Operations are to cease when there is a minimum of 1m of resource remaining over the aquifer.

Reason: To ensure the aquifer is not breached.

	28. 
	Noise Management
During ongoing use of the land, the quarryquarry, it must be operated in accordance with the acoustic reportNoise Impact Assessment Version 01-B prepared by Soundscape Acoustic Consultants dated 10/09/2025 approved under this consent and all noise requirements of the Environmental Protection License.

The recommendations in Section 5.3 of the Noise Impact Assessment are to be adhered to, with the exception of pre-loaded trucks leaving prior to 7.00am. This consent does not allow for any heavy vehicle movements prior to 7.00am.

In the event of any inconsistency between report recommendations and the Environmental Protection Licence (EPL) for the premisesquarry, the EPL prevails.

Reason: To protect the amenity of the local area.


	29. 
	Telephone Complaints Line
A telephone complaints line must operate during its operating hours for the purpose of receiving any complaints from members of the public in relation to activities conducted at the premises quarry or by the vehicle or mobile plant, unless otherwise specified in the Environmental Protection Licence.

The operator must notify the public of the complaints line telephone number and the fact that it is a complaints line so that the impacted community knows how to make a complaint. The complaints telephone number must also be displayed on site, in a location visible to the public (such as the front entrance).

Reason: To protect the amenity of the local area.


	30. 
	Incident and Complaint Reporting
An Incident and Complaint Register is to be established for the life of the quarry. Council and any relevant agencies are to be provided with a detailed report on any complaints, incidents or non-compliance, as a component of the annual return and such further reports as may be requested.

The applicant must provide an annual return in accordance with EPL conditions in relation to the development. In the return the applicant must report on the annual monitoring undertaken (during a pollution incident), provide a summary of complaints relating to the development and report on any compliance matters.

Reason: To protect the amenity of the local area.


	31. 
	Compliance
The operator of the quarry must ensure that all employees and contractors (and their sub-contractors) are made aware of, and instructed to comply with, the conditions of this approval relevant to activities they carry out in respect of the project. 

This includes all obligations under the relevant Environmental Management Plan and Driver Code of Conduct.

Reason: To ensure public safety, protect the amenity of the local area, and manage environmental impacts.


	32. 
	Storage and Disposal of Waste Materials
During ongoing use of the premisesquarry:
(a) All garbage and recyclable materials generated from the premises must be stored wholly within a suitable storage area, which shall be screened from the road and neighbouring dwellings at all times.
(b) Arrangements must be implemented for the separation of recyclable materials from garbage
(c) The waste storage area must be appropriately maintained to prevent litter and the entry of pests.
(d) The operator must make arrangements for regular disposal of waste. All waste shall be assessed, classified and disposed of in accordance with the NSW Environment Protection Authority’s Waste Classification Guidelines. Whilst recycling and reuse are preferable to landfill disposal, all disposal options (including recycling and reuse) must be undertaken with lawful authority as required under the Protection of the Environment Operations Act 1997 to a suitable licenced facility. Evidence of waste disposal shall be kept on premises and provided to relevant authorities including council officers on request. OR A contract must be entered into with a licensed contractor to provide waste collection services for the premises, and a copy of the contract must be kept on premises and provided to relevant authorities including council officers on request.
(e) The collection / transfer of garbage and recyclable materials from the premises must only occur between 7am and 5pm Mondays to Fridays.

In the event of any inconsistency between this condition and the Environmental Protection Licence (EPL) for the premises, the EPL prevails.

Reason: To ensure proper handling of waste, garbage and recyclable materials 
generated during operation of the quarry.


	33. 
	Soil Management
During ongoing use of the premisesquarry, all soil removed from or imported to the site shall be managed in accordance with the following requirements: 
(a) All excavated material removed from the site must be classified in accordance with the Environment Protection Authority’s Waste Classification Guidelines before it is disposed of at an approved waste management facility or otherwise lawfully managed, and the classification, and the volume of material removed, and the receival facility’s details must be reported to the Council.
(b) All fill material imported to the site must be: 
(i) Virgin Excavated Natural Material as defined in Schedule 1 of the Protection of the Environment Operations Act 1997; or
(ii) a material identified as being subject to a resource recovery exemption by the NSW EPA; or
(iii) a combination of Virgin Excavated Natural Material as defined in Schedule 1 of the Protection of the Environment Operations Act 1997 and a material identified as being subject to a resource recovery exemption by the NSW EPA.

In the event of any inconsistency between this condition and the Environmental Protection Licence (EPL) for the premisesquarry, the EPL prevails.

Reason: To ensure soil removed from the site is appropriately disposed of and soil imported to the site is not contaminated and is safe for future occupants.


	34. 
	Decommissioning Plan
A Decommissioning Plan must be provided to Council (or relevant approval authority) generally consistent with the approved Environmental Impact Statement, Rehabilitation Plan and additional information, prepared by SMK Consultants, for review and approval no later than 12 months prior to the proposed cessation of operations. It must include, but not be limited to, the following:
(a) Expected timeline for rehabilitation completion;
(b) Decommissioning of all quarry equipment, plant, any above and below ground 
(c) infrastructure, fencing, detention basins, and any other structures or infrastructure relating the approved development;
(d) Programme of site restoration to return the land to agricultural use, with the retention of landscaping; and
(e) Details on waste management and recycling of all materials arising from the 
development. 
(f) The quarry project owner or operator shall be responsible for all decommissioning and rehabilitation works and associated costs.

Within 12 months of the development ceasing operation all rehabilitation works must be completed. The rehabilitation works must be actively maintained in accordance with the Decommissioning Plan and Rehabilitation Plan until such a time as the works are fully established.

Note: this condition does not prevent the site from being progressively rehabilitated, as set out in the approved Environmental Impact Statement and additional information, prepared by SMK Consultants.

Reason: To ensure the decommissioning of the quarry occurs in an orderly and sustainable manner, that the amenity of the area is maintained while the quarry is being decommissioned and to ensure the site can be returned to a suitable condition.








