Attachment A: Draft Conditions of Consent

Administrative conditions

Approved Plans and Documentation
1. The development of a solar farm and battery energy storage system, comprising 12,000 solar panels on tracking arrays, 1 central inverter, 1 medium voltage power station, 4 battery energy storage systems and associated fencing, pole and road/intersection works a must be carried out in accordance with the following approved plans and supporting documentation (stamped by Council), except where the conditions of this consent expressly require otherwise.
In the event of any inconsistency between the approved plans and the supporting documentation, the approved plans prevail. In the event of any inconsistency between the approved plans and a condition of this consent, the condition prevails. 
NOTE: an inconsistency occurs between an approved plan and supporting documentation or between an approved plan and a condition when it is not possible to comply with both at the relevant time.
	Plan Title
	Drawn by
	Issue/Rev
	Drawing No
	Date

	4.95MVA PV Export System 
Site Plan (x2 sheets)
	Green Gold Energy 
	H
	
	25/09/2025

	76 Module Tracker Details, Sheet M-101
	NexTracker
	A
	GEN MECH. SET
	07/09/2021

	38 Module Tracker Details
	NexTracker
	A
	GEN MECH. SET
	07/09/2021

	Pier Tolerances
	NexTracker
	A
	GEN MECH. SET
	07/09/2021

	General Solar Farm Electrical Equipment Elevations
	Green Gold Energy
	A
	
	08/11/2023

	General Solar Farm Electrical Equipment Elevations
	Green Gold Energy
	B
	
	20/11/2020

	Chain wire Mesh Security Fence & Gate
	Ace Microgrid
	B
	GG21-10-003-1
	16/09/2022

	Two-Dimensional Strategic Design
	Trafficworks
	P1
	230729a-CTP-01
	22/09/2025

	Typical Sections
	Trafficworks
	P1
	230729a-CTP-02
	22/09/2025

	SISD Check
	Trafficworks
	P1
	230729a-CTP-03
	22/09/2025

	SISD Check
	Trafficworks
	P1
	230729a-CTP-04
	22/09/2025

	Swept Path Assessment
	Trafficworks
	P1
	230729a-SKT-01
	22/09/2025

	Swepth Path Assessment
	Trafficworks
	P1
	230729a-SKT-02
	22/09/2025

	Swepth Path Assessment
	Trafficworks
	P1
	230729a-SKT-03
	22/09/2025



	Approved documents

	Title
	Author
	Rev
	Job No
	Date

	Statement of Environmental Effects
	Chris Smith & Associates/Green Gold Energy
	3
	24033
	Oct 2025

	Bushfire Management & Emergency Response Plan
	Harris Environmental Consulting
	1
	6784BF
	10/10/2024

	Traffic Impact Assessment Report
	Trafficworks
	Final 2
	230729
	23/09/2025

	Construction Phase Waste Management Plan
	Low Impact Development Consulting 
	1
	
	06/03/2025

	Construction Environmental Management Plan
	Green Gold Energy
	-
	GG-CEMP
	undated

	Biodiversity Assessment Report
	OzArk
	3
	4371
	06/08/2024



2. Compliance with Building Code of Australia and insurance requirements under Home Building Act 1989
(1)  It is a condition of a development consent for development that involves building work that the work must be carried out in accordance with the requirements of the Building Code of Australia.
(2)  It is a condition of a development consent for development that involves residential building work for which a contract of insurance is required under the Home Building Act 1989, Part 6 that a contract of insurance is in force before building work authorised to be carried out by the consent commences.
(3)  It is a condition of a development consent for a temporary structure used as an entertainment venue that the temporary structure must comply with the Building Code of Australia, Volume 1, Part B1 and NSW Part I5.
(4)  In subsection (1), a reference to the Building Code of Australia is a reference to the Building Code of Australia as in force on the relevant date.
(5)  In subsection (3), a reference to the Building Code of Australia is a reference to the Building Code of Australia as in force on the day on which the application for development consent was made.
(6)  This section does not apply—
(a)  to the extent to which an exemption from a provision of the Building Code of Australia or a fire safety standard is in force under the Environmental Planning and Assessment (Development Certification and Fire Safety) Regulation 2021, or
(b)  to the erection of a temporary building, other than a temporary structure to which subsection (3) applies.
Note: In this section relevant date has the same meaning as in the Environmental Planning and Assessment (Development Certification and Fire Safety) Regulation 2021, section 19.
Condition reason: 
To comply with the provisions of clause 69 of the Environmental Planning and Assessment Regulation 2021.

3. National Construction Code
All building work shall be carried out in accordance with the provisions of the Building Code of Australia. A reference to the National Construction Code / Building Code of Australia is a reference to that Code as in force on the date the application is made for the relevant construction certificate. 
Note: Under Part 4A of the EP&A Act, the Applicant is required to obtain construction and occupation certificates for the propped building works.
Condition reason:
To ensure the building work complies with the National Construction Code. 

4. Time limited consent
The use of the site for a solar farm and battery energy storage system is limited to a period of thirty (30) years from the release of an occupation certificate.
Condition reason:
To limit the period during which the approval may operate, in accordance with the provisions of section 4.17(d) of the Environmental Planning and Assessment Act 1979.
5. Decommissioning 
Prior to the cessation of operations, the applicant must prepare and submit a Decommissioning and Rehabilitation Plan to Council for approval. The Plan must detail the method, timing and responsibilities for decommissioning the solar farm and rehabilitating the site.
Upon decommissioning of the development:
· All solar farm infrastructure, plant, equipment, footings, underground cabling (unless otherwise agreed by the landowner and Council), hardstand areas and associated works must be fully removed from the site.
· The land must be reinstated to its pre‑existing condition, including the pre‑existing land and soil capability class, where the land was previously used for agricultural purposes.
· Disturbed areas must be stabilised, re‑vegetated and rehabilitated to a condition that supports the former land use and prevents erosion, sedimentation or land degradation.
Responsibility for decommissioning and rehabilitation rests with the solar energy project owner or operator, unless a legally binding agreement with the host landowner is provided to Council that clearly assigns alternate responsibilities.
Condition reason: 
To ensure that plant is removed to avoid potentially hazardous chemical spills from the Bess systems, and the land is rehabilitated.

Requirements of Government Agencies (General Terms of Approval)
Essential Energy
6. Essential Energy requirements
If the proposed development changes, there may be potential safety risks and it is recommended that Essential Energy is consulted for further comment; 
· Any existing encumbrances in favour of Essential Energy (or its predecessors) noted on the title of the above property should be complied with; 
· Any activities in proximity to electrical infrastructure must be undertaken in accordance with the latest industry guideline currently known as ISSC 20 Guideline for the Management of Activities within Electricity Easements and Close to Infrastructure; 
· Prior to carrying out any works, a “Dial Before You Dig” enquiry should be undertaken in accordance with the requirements of Part 5E (Protection of Underground Electricity Power Lines) of the Electricity Supply Act 1995 (NSW); and 
· It is the responsibility of the person/s completing any works around powerlines to understand their safety responsibilities. SafeWork NSW (www.safework.nsw.gov.au) has publications that provide guidance when working close to electricity infrastructure. These include the Code of Practice – Work near Overhead Power Lines and Code of Practice – Work near Underground Assets.

Condition reason:
To ensure compliance with the terms of approval and notations from Essential Energy and to maintain the safety of workers and others in and around the site, and, to protect electricity infrastructure.
Transport for NSW
7. Signage
A signage schedule identifying the location, type and placement of all proposed signs is to be prepared. The schedule is to be consistent with Drawing no 230729a-CTP-01 and designed in accordance with AS 1742 and TfNSW requirements. This schedule is to be submitted to Council for final approval by TfNSW as concurrence authority.
Condition reason:
To comply with the requirements of Transport for NSW.
8. Mitchel Highway intersection
The intersection of the Mitchell Highway with the proposed site access is to be upgraded to a BAR/BAL minimum design standard in accordance with Traffic Impact Assessment Strategic Concept design plans and the requirements of Transport for NSW.
A SISD of 341m is to be provided and maintained at all times.
Truck warning signs are to be displayed near the subject site access during the construction phase when heavy vehicles are entering the site. The following signs are to be displayed at a minimum:
· “Advance Truck” warnings igns (W5-22 Size B)
· Distance plate (W8-5 Size B) below the warning sign
The above signs are to be installed 250m in advance of the access on each of the Mitchell Highway advances.
Condition reason:
To provide appropriate and safe access to the site in accordance with the requirements of Transport for NSW.
9. Drain & Culvert
It is noted that the proposed intersection traverses an existing table drain and connects to land at a different reduced level. Detailed design to be submitted to the determining authority, is to include survey, drainage assessment and vertical design to confirm the final intersection arrangement. The requirement for a culvert or other drainage structure through the intersection will be assessed and, if required, designed in accordance with Austroads and TfNSW drainage standards. It is noted the works will require re-profiling of the existing table drains and the installation of a culvert beneath the proposed access road.
Condition reason:
To comply with the requirements of Transport for NSW.

10. Telecommunications Utilities
A utilities investigation and service location is to be undertaken. Any required protection, adjustment or relocation of utilities is to be addressed in consultation with the relevant utility authorities and TfNSW.
Condition reason:
To comply with the requirements of Transport for NSW.

11. Shoulder width
The shoulder width shown is indicative only. A detailed site survey is required to be undertaken to confirm the existing road formation. TfNSW preference is to widen the shoulders to 3 metres.
Condition reason:
To comply with the requirements of Transport for NSW.

12. Design plans
The final design plans are to include an updated Traffic Impact Assessment to address the requirements of TfNSW. The updated TIA is to be submitted to Council with the final designs.
Condition reason:
To comply with the requirements of Transport for NSW.

Prior to the release of the Construction Certificate

13. Construction Certificate
Prior to the commencement of any physical works on the site, including but not limited to road construction, access tracks, drainage works, earthworks, culvert installation, stormwater management structures, hardstands or site entry upgrades, a Construction Certificate (CC) must be obtained from the Certifier.
The CC must include and certify the following:
· Final engineering drawings for all civil and building works, prepared by suitably qualified civil engineers, demonstrating compliance with this consent, Council’s engineering standards, Austroads Guides, Australian Rainfall and Runoff (ARR 2019), and relevant Australian Standards.
· Roads Act 1993 approval for any works within the public road reserve, including access upgrades, drainage tie‑ins, sight distance improvements and utility relocations.
· Stormwater and drainage design, including culverts, table drains, overland flow paths, scour protection, energy dissipation, and erosion and sediment controls, sized for the 1% AEP event and consistent with the approved flood assessment.
· Building‑related components, including but not limited to:
· structural design and certification for inverter stations, switchrooms, control buildings, battery enclosures, shade structures, footings, platforms, retaining walls and any other building or structure defined under the NCC
· fire safety measures applicable to buildings or enclosed structures
· access, egress and compliance with relevant NCC performance requirements.
· Bushfire access requirements, including trafficable width, passing bays, turning heads and all-weather construction, consistent with the approved Bushfire Management & Emergency Response Plan.
· Erosion and Sediment Control Plan (ESCP) consistent with the Blue Book and staged to match construction sequencing.
· Certification of earthworks, including finished levels, batters, compaction, and any retaining or structural elements.
· Utility protection or relocation plans where civil works interact with existing services.
No works may commence until the CC is issued and all associated approvals are in place.
A Construction Certificate issued by a Private Certifier is to be submitted to Council at least 48 hours prior to the commencement of any works.  
Condition reason:
To ensure compliance with the Environmental Planning and Assessment Act 1979.

14. Utilities
The Applicant is to negotiate with the utility authorities in connection with the relocation and/or adjustment of the services affected by the development. Any necessary alterations to, or relocations of, utility services must be carried out at no cost to the council.
Condition reason:
To ensure utility modifications are carried out in accordance with the requirements of the relevant authority and that responsibility for cost is clear.

15. Payment of Security Deposits, Levies and Contributions
The fees listed in the table below must be paid in accordance with the conditions of this consent and Council’s adopted Fees and Charges applicable at the time of payment. Payments must be made prior to the issue of the Construction Certificate or prior to the commencement of work (if there is no associated Construction Certificate). 

1. Payment of building and construction industry long service levy - The applicant must pay the long service levy of $13,786.41 as calculated at the date of this consent to the Long Service Corporation or Council under Section 34 of the Building and Construction Industry Long Service Payments Act 1986 and provides proof of this payment to the certifier.
1. Public liability insurance - Prior to the commencement of any works on Council land including a public road, the applicant is to obtain Public Liability Insurance in the minimum amount of $20 million. This insurance is to note Council’s interest and is to remain current for at least the period from the issue of the Construction Certificate until the issue of a Compliance Certificate/Occupation Certificate for the works. Documentary evidence of the Certificate of Currency is to be provided to Council prior to the issuing of any Construction Certificate for access. 

16. Construction Environmental Management Plan updates
The Construction Environmental Management Plan (CEMP) is to be updated to include the requirements below and submitted to the Principal Certifier. The Plan must be implemented during the construction of the solar electricity system and must include the range of measures as outlined in the approved SEE which include but are not limited to:
a) Aboriginal Heritage Management (chance find procedures);
b) Construction Traffic Management;
c) Erosion and Sediment Control – actions to support objectives;
f) Noise Management – actions to support objectives;
g) Dust Management – actions to support objectives;
h) Site Restoration;
k) Weed Management and Biosecurity.
Condition reason:
To ensure the CEMP accurately reflects actions to be taken where management controls have been identified.

17. Construction Traffic Management Plan
Prior to the issue of any Construction Certificate, a Construction Traffic Management Plan (CTMP) must be prepared by a suitably qualified and experienced professional. The CTMP must be submitted to the relevant roads authority for review to ensure that all traffic and access impacts associated with the construction of the development have been adequately addressed.
The CTMP must identify all light and heavy vehicle movements to and from the site, assess the potential traffic, safety and road‑condition impacts arising from construction activities, and specify the mitigation, management and monitoring measures to be implemented to ensure compliance throughout the construction phase.
The CTMP must address, at a minimum, the following matters:
a) A safe construction access point, as detailed on drawing no. 230729a-CTP-01 (Trafficworks) with a minimum sealed entrance 20 metres in to the property access;
b) A passing lane of a minimum of 3.0m along the Mitchell Highway past the intersection – BAR Treatment as per Austroads Guidelines.
d) A bitumen seal holding lane for the exit from the Mitchell Highway into the property access and entry onto the Mitchell Highway from the property access.
e) Road widths must show turning circles for the largest design vehicle expected to use the roadway.
f) A minimum of 20 m to be sealed into the access road.
g) All accesses to be designed as per Austroads Design Guide.
h) Require that all vehicular access to the site be via the approved route using the approved construction access point.
i) Detailed design information of road construction works must be provided and approved by the roads authority in accordance with Austroads Guidelines and RMS QA Road works specifications for road construction and design.
j) Submit inspection and test plans (ITPs) to the roads authority for approval.

Condition reason:
To ensure access related matters are assessed prior to construction.

18. Section 138 Roads Act approval
Under Section 138 of the Roads Act 1993, any works on the verge, footpath, or public road reserve require a Section 138 Roads Act Approval. This will need to be obtained from the relevant roads authority – Council and/or Transport for NSW. In this regard, the applicant is to make a formal application to Council. The Section 138 Roads Act Application is to be submitted to, and approved by the roads authority prior to works commencing and is to include the provision of Works as Executed Drawings after the completion of road works.
Condition reason:
To require an approval under the Roads Act where necessary.

19. Bushfire management & access
The Bushfire Management & Emergency Response Plan is to be updated to reflect the new access arrangements from the Mitchell Highway to the solar farm. Any changes required to access arrangements from these changes are to be ratified by the consultant to be in compliance with the requirement of Planning for Bushfire Protection 2019.
Condition reason:
To ensure approved documents match the intended construction for the site.

20. Access provisions & carparking
[bookmark: _Hlk192062760]All driveways, access ramps, vehicular crossings and car parking spaces shall be designed and constructed in accordance with the current version of Australian Standards, AS 2890.1-2004: Parking Facilities – Off-street Car Parking and AS 2890.2:2018 - Parking facilities Off-street commercial vehicle facilities. All car parking for the operation of the solar farm is to be provided on an all-weather surface and signposted with a minimum of twenty (20) car parking spaces are to be provided. Details are to be provided with the Construction Certificate application. 
Condition reason:
To ensure access and parking is provided in accordance with the relevant AS and the approved TIA.

Reason: To ensure driveways, access ramps, vehicular crossings and car parking complies with the relevant Australian Standards.
21. Easements for access
Proof of required additional easements (Section 88B instruments) for access, as registered on the title of the land under the Conveyancing Act 1919, and as identified in the TIA, are to be submitted to Council prior to works commencing on the access roads. 
Condition reason:
To ensure legal access to the land is available prior to construction.
22. Dilapidation report
Before the issue of a Construction Certificate, a suitably qualified engineer must prepare a pre-construction dilapidation report detailing the structural condition of roads and public land, to the satisfaction of the certifier. 
Any damage caused to other properties during construction shall be rectified by the applicant. A copy of the dilapidation survey and an insurance policy that covers the cost of any rectification works shall be submitted to Council prior to the commencement of the demolition works. The insurance cover shall be a minimum of $20 million. 
Condition reason:
 To ensure any damage caused by the development is documented prior to works commencing on the site.

Prior to the commencement of works
23. Roads inspection 
Prior to the commencement of works, an inspection of the site access from the Mitchell Highway is to be carried out and any roadside vegetation is to be trimmed/removed where which restricts compliance with the applicable sight distance requirement of 324 metres. Where whole trees are to be removed, the Principal Certifier is to liaise with Council to first determine whether an REF is required.
Condition reason: To comply with the recommendations of the TIA as approved by Council.
24. Waste
Prior to the commencement of works, a proposed Waste Agreement is to be provided to and approved by Council, outlining the arrangements for the disposal of construction waste if it is to be disposed of at a Council owned facility.
Condition reason:
To ensure the receiving authority is able to accept the waste as outlined in the Construction Phase Waste Management Plan.
25. Erosion controls
Erosion and sediment controls must be in place before the disturbance of any soils on the site.
Condition reason:
To ensure soil and water management is controlled.

26. Signs on site
A sign must be erected in a prominent position on any site on which building work or demolition work is being carried out:
1. showing the name, address and telephone number of the principal certifier for the work, and
1. showing the name of the principal contractor (if any) for any building work and a telephone number on which that person may be contacted outside working hours, and
1. stating that unauthorised entry to the work site is prohibited.
Any such sign is to be maintained while the building work or demolition work is being carried out but must be removed when the work has been completed.
Condition reason: 
Prescribed Condition under Clause 98A(2) and (3) of the Regulation.

27. Toilet Facilities during Construction
Toilet facilities must be provided on the work site during construction at the rate of one toilet for every 20 persons or part of 20 persons employed at the work site. Each toilet provided must be:
1. Connected to an on-site effluent disposal system approved by the council, or
1. A portable toilet.

Condition reason:
To provide appropriate on-site amenities during demolition and construction work. 

28. Implementation of relevant construction plans
The following plans associated with construction phases are to be fully implemented in accordance with this consent:
a) Construction Phase Waste Management Plan
b) Bushfire Management & Emergency Response Plan
c) Construction Environmental Management Plan

Condition reason:
To ensure measures that will protect the public, and the surrounding environment, during site works and construction are implemented prior to works commencing on the site.
29. Traffic Control Plan
Prior to the commencement of any works that impact the public road reserve, road shoulder, verge, or trafficable areas, a Traffic Control Plan (TCP) must be prepared by a person holding current TfNSW Prepare a Work Zone Traffic Management Plan (PWZTMP) accreditation.
The TCP must:
· Be prepared in accordance with AS 1742.3 – Traffic Control for Works on Roads and all relevant TfNSW Traffic Control at Work Sites manuals.
· Identify all proposed traffic management measures, signage, delineation, vehicle movements, and safe access arrangements for adjoining properties.
· Demonstrate how the safety of road users and workers will be maintained for the duration of works.
· Include details of any required partial or full lane closures, speed reductions, or temporary traffic arrangements.
The approved TCP must be submitted to Council at least 10 working days prior to works commencing and must be implemented in full for the duration of works.
Condition reason:
To ensure safe access to and from the site during construction works.

30. Bushfire Water Supply
A minimum 20,000 litres of static water must be provided within the development site for bushfire protection purposes. The water supply must be installed and maintained in accordance with the following requirements:
· Water must be stored in above‑ground metal or concrete tanks, or in underground tanks with a minimum 200 mm access hole and a hardened, all‑weather surface extending 4 metres around the access point.
· Any raised tanks must be installed on protected, non‑combustible stands.
· All external pipework, including taps, must be constructed of metal.
· Pumps must be shielded to ensure operability during a bushfire.
· A 65 mm Storz outlet fitted with a gate or ball valve must be provided to enable firefighting access to the water supply.
The bushfire water supply must be installed prior to the commencement of construction works and maintained for the life of the development.
Condition reason:
To ensure the infrastructure is protected with adequate fire fighting capabilities and water supply.

31. Rural Address
Prior to works commencing on site, the applicant must obtain a Rural Address for the site from Council in accordance with the NSW Address Policy & User Manual 2024 and AS/NZS 4819:2011 Rural and Urban Addressing.
The approved rural address number must be:
· Permanently displayed at the property entrance in a clearly visible location,
· Installed on a post, gate, or other suitable structure at the driveway entry,
· Displayed using reflective materials with numerals of a size and colour that always ensures visibility from the road.
The rural address number must be maintained in good condition for the life of the development.
Condition reason:  Because it is in the public interest that the property be easily identifiable.  

During Construction

32. Asset Protection and Internal Access
A defendable space managed as an Asset Protection Zone (APZ) must be established and maintained around the solar array within the fenced compound for the life of the development. Internal property access must comply with the requirements of Table 7.4a of Planning for Bush Fire Protection 2019, including:
· a minimum 4‑metre carriageway width
· turning areas capable of accommodating a fire tanker with a minimum inner turning radius of 6 metres and outer turning radius of 12 metres
· a minimum 4‑metre vertical clearance to any overhead obstructions
· curves with a minimum inner radius of 6 metres
· a minimum 6‑metre separation between inner and outer curves
· a crossfall not exceeding 10 degrees
· maximum grades not exceeding 15 degrees (sealed) or 10 degrees (unsealed)
· road surfaces and any bridges capable of supporting a 23‑tonne firefighting vehicle, with signage indicating load capacity
· suitable access for a Category 1 fire appliance to within 4 metres of the static water supply where no reticulated supply is available
Condition reason:
To comply with the requirements of Planning for Bushfire Protection 2019 and the Bushfire Management & Emergency Response Plan.

33. Hours of Construction
Construction work may only be undertaken during the following hours:
	DAY
	HOURS

	Monday to Friday
	7:00am to 8:00pm

	Saturday
	8:00am to 1:00pm

	Sunday & Public Holidays
	Nil



NOTE: Outside these hours, delivery of plant, equipment and materials may occur to fit with delivery schedules and as requested by police or other authorities for safety reasons. 
Condition reason:
To ensure the development does not unduly impact surrounding neighbours.

34. Dust Management
A water cart is required to be readily available to suppress dust during construction. During dry periods or high wind, construction works are to be delayed or postponed.
Condition reason:
To comply with the recommendations of the CEMP and reduce dust impacts.

35. Flood Protection
Any above-ground electrical infrastructure including the solar panels shall be set above 1:100 ARI (average recurrent interval) flood level.
Condition reason:
To ensure the infrastructure on site is flood-protected in the adopted design flood.

36. Waste Management
All building rubbish and debris, including that which can be windblown, shall be contained on site in a suitable container for disposal at an authorised Waste Landfill/Recycling Depot at regular periods. The container shall be erected on the site and shall be maintained for the term of the construction to the completion of the project. The waste container shall be regularly cleaned to ensure proper containment of the building wastes generated on the construction site.
Condition reason:
To ensure rubbish is contained and disposed of.

37. Demolition works
Demolition undertaken in the decommissioning of the site must be carried out in accordance with the provisions of AS2601-2001: The Demolition of Structures.

38. Hazardous Materials and Spill Containment
a) All hazardous materials associated with the development, including but not limited to transformer insulating oils, battery electrolyte by‑products, fire suppression agents, fuels and lubricants, must be stored, handled and managed to prevent soil or water contamination.
b) Any transformer forming part of the Medium Voltage Power Station must be installed within a fully bunded and impervious containment system with a capacity not less than 110% of the total oil volume of the largest vessel within the bund. The bund must be designed to prevent infiltration to soil and must be fitted with controlled drainage or a pump‑out point to allow removal of stormwater following inspection.
c) A Safety Data Sheet (SDS) for all insulating oils, fire suppression agents and other hazardous substances must be included in the Construction Environmental Management Plan (CEMP) and kept on site at all times.
d) Spill response equipment suitable for transformer oil, fuels and other hazardous liquids must be maintained at all work areas and at the MV Power Station. All personnel must be trained in spill response procedures.
Condition reason:
To ensure the MVPS is adequately bunded if containing transformer oil.
39. Discovery of Aboriginal Objects
While excavation or building work is being carried out, all such works must cease immediately if a relic or Aboriginal object is unexpectedly discovered. The applicant must notify the Heritage Council of NSW in respect of a relic and notify the Secretary of the Department of Planning and Environment and the Heritage Council of NSW in respect of an Aboriginal object. Building work may recommence at a time confirmed by either the Heritage Council of NSW or the Secretary of the Department of Planning and Environment. 
In this condition:
· “relic” means any deposit, artefact, object or material evidence that: 
1. relates to the settlement of the area that comprises New South Wales, not being Aboriginal settlement, and 
1. is of State or local heritage significance; and 
· “Aboriginal object” means any deposit, object or material evidence (not being a handicraft made for sale) relating to the Aboriginal habitation of the area that comprises New South Wales, being habitation before or concurrent with (or both) the occupation of that area by persons of non-Aboriginal extraction and includes Aboriginal remains.
Condition reason:
To ensure the protection of objects of potential significance during works.

40. Critical Stage Inspections 
Building work must be inspected on the occasions set out for critical stage inspections for building work under the Environmental Planning and Assessment Regulation 2021.
Condition reason:
To require approval to proceed with building work following each critical stage inspection and comply with the Regulation.

41. Native Vegetation 
There must be no removal or disturbance of native vegetation except as authorised by this consent, including canopy trees, understorey and ground cover vegetation without the prior written consent of Council. 
Condition reason: 
To ensure vegetation is maintained on the site.

42. Clearing for Asset Protection Zones (APZ)  

The applicant must ensure the clearing of vegetation to establish the APZ is confined to within the marked APZ boundary and is consistent with the Landscape Plan and bushfire Report, to the satisfaction of the principal certifier.
Condition reason:
To ensure vegetation clearance during construction is confined within the APZ.

43. Access width
The width of the internal access roads is to be a minimum of 6m for the length of the access to the development site in accordance with the recommendations of the approved Traffic Impact Assessment (TIA). Where upgrades to the internal access roads are required over lots owned by the Crown and other entities, written consent of the Crown and/or these entities is to be obtained prior to works taking place. 
Condition reason:
To ensure adequate road widths are provided in accordance with the approved TIA.
Prior to Occupation/Use
44. Occupation Certificate
The applicant is to obtain an Occupation Certificate pursuant to Section 6.3 of the Environmental Planning and Assessment Act 1979, from the Principal Certifier.
Condition reason:
To ensure compliance with the Act.
45. Site Environmental Management Plan
A Site Environmental Management Plan (SEMP) shall be submitted to Council for endorsement prior to the issue of any Occupation Certificate. The SEMP shall address, at minimum, the following issues:
a. Operation
b. Bushfire management
c. Noise management;
d. Dust management;
e. Weed and vermin management;
f. Land management including vegetation management;
g. Traffic Management;
h. Flooding and debris issues; and
i. Written notification to Council when decommissioning is to take place.
46. Completion of all Works
All works must be completed in accordance with the conditions of this consent prior to the issue of an Occupation Certificate including, but not limited to, the following
1. Car parking areas and vehicle access points;
1. Fencing;
1. Bushfire Protection Measures and standards as outlined in this consent shall be installed and completed;
1. All drainage works required to be undertaken in accordance with this consent shall be completed prior to the issue of an Occupation Certificate for the development. 
Following any construction or upgrading on site, the applicant must restore the ground cover of the site as soon as practicable, using suitable species and maintain ground cover. 
Condition reason: 
To ensure adequate arrangements have been made for the development.

Ongoing occupation and post-occupation
47. Vehicle Management
The premises shall be operated in accordance with the following vehicle management requirements:
1. All loading and unloading of vehicles must be undertaken wholly within the site and all vehicles must enter and leave the site in a forward direction. 
1. Sufficient car parking is to be provided on the site, with no car parking to occur on the public road network in the vicinity of the site. 
1. The vehicle entry and exit points are to be clearly signposted and visible from both the street and the site at all times and must be maintained in good condition for the life of the development. 
Condition reason:
To ensure the operation of the solar farm does not adversely affect the surrounding road network and has adequate car parking provided on the site. 

48. Groundcover Vegetation and Topsoil Protection
Groundcover vegetation must be established and maintained across all disturbed areas of the site (with the exception of areas identified in the Bushfire Management and Emergency Response Plan to be vegetation-free) to prevent erosion and protect topsoil. Species used for groundcover must be drought‑hardy, capable of providing persistent soil cover, and suitable for the local soil and climatic conditions identified in the Biodiversity Assessment Report.
Condition reason:
To ensure groundcover is maintained on site to minimise dust nuisance and retain topsoil.

49. Decommissioning
Within 18 months of the site being decommissioned, the site shall be returned, as far as practicable, to its condition prior to the commencement of construction in consultation with relevant landowners, unless the site is being retained for future development purposes. 
All solar panels and associated above ground structures including but not necessarily limited to, the substation, the control and facilities building and electrical infrastructure, including underground infrastructure to a depth of 300 millimetres, shall be removed from the site unless otherwise agreed by the Council, except where the substation, control room or overhead electricity lines are transferred to or in the control of the local electricity network operator. 
All other elements associated with the project, including site roads, shall be removed unless otherwise agreed to by the Council.
Condition reason:
To ensure the site is appropriately rehabilitated post-occupation to enable reuse as primary production land.

Advisory Notes
Other Approvals and Permits
A. The Applicant is solely responsible for obtaining any necessary permits including crane permits, road opening permits, hoarding or scaffolding permits, footpath occupation permits and/or any other approvals under Section 68 (Approvals) of the Local Government Act, 1993 or Section 138 of the Roads Act, 1993.

Responsibility for other Consents / Agreements
B. The Applicant is solely responsible for ensuring that all additional consents and agreements are obtained from other authorities, as relevant.

Disability Discrimination Act
C. This application has been assessed in accordance with the Environmental Planning and Assessment Act 1979. No guarantee is given that the proposal complies with the Disability Discrimination Act 1992. The Applicant/owner is responsible to ensure compliance with this and other anti-discrimination legislation. The Disability Discrimination Act 1992 covers disabilities not catered for in the minimum standards called up in the National Construction Code which references AS 1428.1 - Design for Access and Mobility. AS1428 Parts 2, 3 & 4 provides the most comprehensive technical guidance under the Disability Discrimination Act 1992 currently available in Australia.

Commonwealth Environment Protection and Biodiversity Conservation Act 1999
D. The Commonwealth Environment Protection and Biodiversity Conservation Act 1999 provides that a person must not take an action which has, will have, or is likely to have a significant impact on a matter of national environmental significance (NES) matter; or Commonwealth land, without an approval from the Commonwealth Environment Minister. This application has been assessed in accordance with the New South Wales Environmental Planning & Assessment Act, 1979. The determination of this assessment has not involved any assessment of the application of the Commonwealth legislation. It is the Applicant's responsibility to consult the Department of Sustainability, Environment, Water, Population and Communities to determine the need or otherwise for Commonwealth approval and you should not construe this grant of approval as notification to you that the Commonwealth Act does not have application. The Commonwealth Act may have application and you should obtain advice about this matter. There are severe penalties for non-compliance with the Commonwealth legislation.

Site Contamination issues During Construction
E. Should any new information come to light during demolition or construction works which has the potential to alter previous conclusions about site contamination then the Applicant must be immediately notified and works must cease. Works must not recommence on site until the consultation is made with the Department.

Covenants
F. It is possible that a covenant may affect the land which is the subject of this consent. The grant of this consent does not necessarily override that covenant. You should seek legal advice regarding the effect of any covenants which affect the land.

Dial Before You Dig
G. Underground assets may exist in the area that is subject to your application. In the interests of health and safety and in order to protect damage to third party assets please contact Dial before you dig at www.1100.com.au or telephone on 1100 before excavating or erecting structures (This is the law in NSW). If alterations are required to the configuration, size, form or design of the development upon contacting the Dial before You Dig service, an amendment to the development consent (or a new development application) may be necessary. Individuals owe asset owners a duty of care that must be observed when working in the vicinity of plant or assets. It is the individual’s responsibility to anticipate and request the nominal location of plant or assets on the relevant property via contacting the Dial before you dig service in advance of any construction or planning activities.

Telecommunications Act 1997 (Commonwealth)
H. Telstra (and its authorised contractors) are the only companies that are permitted to conduct works on Telstra’s network and assets. Any person interfering with a facility or installation owned by Telstra is committing an offence under the Criminal Code Act 1995 (Cth) and is liable for prosecution. Furthermore, damage to Telstra’s infrastructure may result in interruption to the provision of essential services and significant costs. If you are aware of any works or proposed works which may affect or impact on Telstra’s assets in any way, you are required to contact: Telstra’s Network Integrity Team on Phone Number 1800810443.

General
I. Development Consent does not lapse if the approved use has actually commenced or the proposed work is physically commenced before the lapse date except where a condition specifies a limit to the duration of the consent.





